How to upload (burn) BIOS on the 886LCD/ATX family.

Ref.: Kontron Technology/MLA/09092003.


From DOS you can upload a BIOS into a 886LCD/ATX motherboard.

Copy the directory "BIOS 886LCD\Tool" to a directory on your target 886LCD/ATX.
A bootable DOS Floppy Disk is also a possibility.


In the document D00440 "List of supported displays for 886LCD-ATX" you can 
find references (BIOS name) to all the 886LCD BIOS's available.


The same BIOS name can be found in the directory "BIOS 886LCD" depending on the 
type of 886LCD/ATX you are using. 


Copy the requested BIOS (BIN-file) to the above mentioned directory on your target 
886LCD/ATX. Make sure that only one (1) BIN-file is located in this directory.


Now, execute the Burn886.bat (only from DOS).

