Note:
The tools on this disk are delivered by ASILIANT technologies
which is the manufacturer of the VGA controller 69030
and are only passed through by PEP Modular Computers.

For further informations see www.asiliant.com

Contents of this disk:


Files delivered by Asiliant technologies
----------------------------------------

LICENSE.TXT      Software End User License Agreement

RELNOTE.DOC      Video source code release notes

UG180.PDF        VGABIOS OEM reference guide
                 read this file for informations on
                 BMP030.EXE, BMS-Files, SYS-Files

FPT55X.EXE       Flat panel timing program
FPTPROG.ICO      Icon for this program
55X-051.REL      Release notes for this program
FPT55X.HLP       Online Help for this program
ugfpt54x.doc     User guide for this program
fptapp07.doc     Flat panel timing application note

Bmp030.exe       Video BIOS Editor
VGA030.DAT       Sample VGABIOS binary
VGA030.BMS       BMS-File for the above binary
DRV030.SYS       VGABIOS loadable as a device driver

Files delivered by PEP modular computers
----------------------------------------
readme_pep.txt   This file !

CP331CRT.BIN     Binary file of the CP331 BIOS for CRT-only
CP331CRT.BMS     BMS-file of the above BIOS
CP331DU.BIN      Binary file of the CP331 BIOS usable for 
                 LVDS, Panel-Link, and CRT
CP331DU.BMS      BMS-file of the above BIOS


How to use these applications to create a new BIOS that 
supports a particular flatpanel

1) Read the doc-files and the ug180.pdf file. 
--------------------------------------------

These documents explain the functionality of the tools.

2) Calculate the parameters for your flatpanel
----------------------------------------------

tool: fpt55x.exe
required: flat-panel timing parameters

3) Add the values to your BIOS
------------------------------

tool: bmp030.exe
required: parameters from step 2

As a base for your adaptions use the VGABIOS-File CP331DU.BIN
in this directory. Replace on of the 16 Flatpanel table entries
by your parameters.

4) create the BIOS
------------------

Done from bmp030.exe
Save the VGABIOS binary file with Key [F10].
Optionally save the .BMS - File with [F6].


**************** IMPORTANT ********************
A bad timing setup may destroy the flatpanel.
The use is at your own risk!
***********************************************

PEP Modular Computers offers the adaption of a new panel
as a paid service.


