Set Key (Vender codes) can be changed by use of bf epoke command like: bf epoke 8 01

where 8 is the offset byte and 01 is the byte value.



The following offsets and values are possible.

786LCD-mITX options:
8	01	ESC-key 	to load Default CMOS settings. Press key after power up until kbd led flash.
8	0F	TAB			-"-
8	1D	left Ctrl		-"-
8	21	F-key			-"-
8	29	§/½			-"-
8	3A	Capslock		-"-
8	3B-44	F1-F10			-"-
8	45	NumLock			-"-
8	ff	no key	(default)


886LCD-M options:
8	01	ESC-key 	to load Default CMOS settings. Press key after power up until kbd led flash.
8	0F	TAB			-"-
8	1D	left Ctrl		-"-
8	21	F-key			-"-
8	29	§/½			-"-
8	3A	Capslock		-"-
8	3B-44	F1-F10			-"-
8	45	NumLock			-"-
8	ff	no key	(default)

9	/BIT0	KT Hardisk Lock (typical value fe)
9	ff	remove Harddisk Lock	(default)


886LCD-ATX-GV options:
(none available)


986LCD-M options:
8	01	ESC-key 	to load Default CMOS settings. Press key after power up until kbd led flash.
8	0F	TAB			-"-
8	1D	left Ctrl		-"-
8	21	F-key			-"-
8	29	§/½			-"-
8	3A	Capslock		-"-
8	3B-44	F1-F10			-"-
8	45	NumLock			-"-
8	ff	no key	(default)

9	01	ESC-key		to enter BIOS setup ("Press DEL to run Setup" will not be displayed)
9	0F	TAB			-"-
9	1D	left Ctrl		-"-
9	21	F-key			-"-
9	29	§/½			-"-
9	3A	Capslock		-"-
9	3B-44	F1-F10			-"-
9	45	NumLock			-"-
9	ff	Del	(default)
9	BIT7	disable the BBS popup(F11) and the Del key ability to exit quiet mode.
9	A1	(example:) F-key to enter BIOS setup + disable BBS popup and Del key to exit quiet mode.

a	fe	ESC-key		to eject the tray on all detected CD/DVD drives at reboot.
a	ff	no key	(default)


KT690:
8	01	ESC-key 	to load Default CMOS settings. Press key after power up until kbd led flash.
8	0F	TAB			-"-
8	1D	left Ctrl		-"-
8	21	F-key			-"-
8	29	§/½			-"-
8	3A	Capslock		-"-
8	3B-44	F1-F10			-"-
8	45	NumLock			-"-
8	ff	no key	(default)

9	01	ESC-key		to enter BIOS setup ("Press DEL to run Setup" will not be displayed)
9	0F	TAB			-"-
9	1D	left Ctrl		-"-
9	21	F-key			-"-
9	29	§/½			-"-
9	3A	Capslock		-"-
9	3B-44	F1-F10			-"-
9	45	NumLock			-"-
9	ff	Del	(default)


KT965 options:
(none available)



