=============================================================================
    Intel(R) Server Platform S2600CW FRU/SDR Update Release Notes
=============================================================================

INTEL(R) Server Boards and Systems
Intel Corporation
2111 N.E. 25th Avenue, Hillsboro, OR 97124 USA

=============================================================================

DATE:   April 17th, 2020

TO:     Intel(R) Server Platform S2600CW customers

SUBJECT:    IBMC(R) FRU/SDR update package S2600CW_FRUSDR_115 release notes

=============================================================================
                               LEGAL INFORMATION
=============================================================================
Information in this document is provided in connection with Intel products.
No license, express or implied, by estoppel or otherwise, to any intellectual
property rights is granted by this document. Except as provided in Intel's
Terms and Conditions of Sale for such products, Intel assumes no liability
whatsoever, and Intel disclaims any express or implied warranty, relating to
sale and/or use of Intel products including liability or warranties relating
to fitness for a particular purpose, merchantability, or infringement of any
patent, copyright or other intellectual property right. Intel Corporation may
have patents or pending patent applications, trademarks, copyrights, or other
intellectual property rights that relate to the presented subject matter.
The furnishing of documents and other materials and information does not
provide any license, express or implied, by estoppel or otherwise, to any
such patents, trademarks, copyrights, or other intellectual property rights.
Intel products are not intended for use in medical, life saving, or life
sustaining applications. Intel may make changes to specifications and product
descriptions at any time, without notice.

Intel is a registered trademark of Intel Corporation.

*Other names and brands are the property of their respective owners.

Copyright (c) 2020 Intel Corporation.

=============================================================================
                              ABOUT THIS RELEASE
=============================================================================

SDR file version:                   1.15
Baseboard FRU file version:         1.15
Master configuration file version:  1.15
FRUSDR utility version:             Version 14.1 Build 18

=============================================================================
        SYSTEM HARDWARE & SOFTWARE REQUIREMENTS/REVISIONS
=============================================================================

- This FRU/SDR package has only been tested on S2600CW FAB3 baseboards.

- BMC firmware rev 1.33(or later) MUST be preinstalled prior to installing
  this FRU/SDR package.

- BIOS R11.01.0036 or later

- MB Ver 03.01.02.002

=============================================================================
                      IMPORTANT INSTALLATION NOTES
=============================================================================

- None

=============================================================================
            INSTALLATION PROCEDURE
=============================================================================

1. Ensure BMC release 1.33 or later is pre-installed before attempting this
   FRU/SDR update.

2. Copy the entire contents of the Package file to the HDD or USB flash drive
      All of the files in this zip archive must reside in the same directory.

3. Boot to EFI and then run the following command to display the
   contents of the baseboard FRU device:

    FRUSDR /d FRU

   If device is empty(which is the case for all new FAB3 baseboards) or corrupted, then
   execute the following command to program the empty FRU device:

   For S2600CW:
        FRUSDR /fru S2600CW.fru

4. Now execute the following command to bring up the main FRU/SDR load menu:

    FRUSDR /cfg master.cfg


5. Select the option which is applicable to what you want to do. On a brand
   new baseboard I would highly recommend to run option 3 to program both
   the FRU and SDR. By reprogramming the FRU you will be given the option
   to input data from the keyboard into various chassis, board and product
   areas. Ensure that you select the correct chassis from the chassis
   selection menu otherwise your fan sensors will not be configured
   properly.

6. Once the package has finished its installation, I would highly recommend
   to DC power off the system and cycle AC power.

=============================================================================
                           KNOWN ISSUES/WORKAROUNDS
=============================================================================

- None

=============================================================================
                           FEATURES ADDED
=============================================================================
FCW_115
- Add KCS Ctrl Mode sensor.
- Upgrade FRUSDR.efi/IPMI.efi utility to Version 14.1 Build 18.

FCW_114
- Add MIC1_PRESCENT (PHI in Riser 1) ~ MIC4_PRESCENT (PHI in Riser 4).

FCW_113
- None.

FCW_112:
- Add one FRU file for BDW CPU.
- Change master.cfg to dynamitic probe FRU on the board.
- Cut in FRUSDR.efi/IPMI.efi utility Version 13.1 Build 8.
- Remove SDR "Bad User PWD" per Intel's request to fix a Hang issue.

FCW_111:
- Follow CWP_FSC Auto-SDR Config Sheet Rev2.1.xlsm.

FCW_110:
- Cut in FRUSDR.efi/IPMI.efi utility 13.1 build6 to support secure boot. 

FCW_109: 
- Add SDR "Bad User PWD" per Intel's request.

FCW_108: 
- Update error message in master.cfg.
- Follow CWP_FSC Auto-SDR Config Sheet Rev1.9.xlsm.

FCW_107:
- Update Shipping SDR(Test Plate FSC) and OTHER SDR: 
  Stepwise sub-record (lower & upper clipping curve).
  Remove Clamp sub-record 5, 11, 14.
- Update PWM of Stepwise Curve ID #1B (Global Stepwise Curve Records).
- Follow CWP_FSC Auto-SDR Config Sheet Rev1.8.xlsm.

FCW_104:
- Implement CCB273 and CCB278 per Intel reques SDR change.
  Change "Front Panel Temp", "IERR" SDR record and add "IERR Rec Info" SDR record.
- Follow CWP_FSC Auto-SDR Config Sheet Rev1.7.xlsm.
- Modify OTHER Chassis SDR per Intel request.

FCW_103:
- Add combo backplane oem sdr.

FCW_102:
- Modify the MIC tag in .sdr & .cfg file.
  RISER_X_FRU  -->  MIC_X_FRU
  RISER_X_MIC  -->  MICX_PRESCENT

FCW_101:
- Follow CWP_FSC Auto-SDR Config Sheet Rev1.5.xlsm.
- Follow CWP_FSC Auto-SDR Config Sheet Rev1.4.xlsm.

FCW_100:
- Follow CWP_FSC Auto-SDR Config Sheet Rev1.3.xlsm.

FCW_11:
- Follow CWP_FSC Auto-SDR Config Sheet Rev1.1.xlsm.

FCW_10:
- None.

FCW_09:
- Follow CWP_FSC Auto-SDR Config Sheet Rev1.0.xlsm.

FCW_08:
- None.

FCW_07:
- Follow CWP_FSC Auto-SDR Config Sheet Rev0.95.xlsm.
- Follow CWP_FSC Auto-SDR Config Sheet Rev0.9.xlsm.
- Add the MIC power sensor.

FCW_06:
- Follow CWP_FSC Auto-SDR Config Sheet Rev0.8.xlsm.
- Add MIC4 Sensors.

FCW_05:
- Follow CWP_FSC Auto-SDR Config Sheet Rev0.6.xlsm.
- Follow CWP_FSC Auto-SDR Config Sheet Rev0.7.xlsm.

FCW_04:
- Update MIC card detect function

FCW_03:
- Follow CWP_FSC Auto-SDR Config Sheet Rev0.5.xlsm.

FCW_02:
- Follow Cottonwood Pass FSC Config Sheet Rev0.4_140219.xlsm.

FCW_01:
- This package is only for PO builds.
- Update SDR as per Cottonwood Pass FSC Config Sheet Rev0.3_140108.xlsm

=============================================================================
                           ISSUES FIXED
=============================================================================
FCW_114:
- EPSD1504424500: [S2600CW]The PHI card's FRU info cannot be detected in EWS.
  Add MIC1_PRESCENT (PHI in Riser 1) ~ MIC4_PRESCENT (PHI in Riser 4).  
  
FCW_113:
- Fix the 2HSBP issue and the 1U combo HSBP HW problem.
  Add a "SET DISABLE_NVME_FUNCTIONS" entry into S2600CW/S2600KP/S2600TP CFG files.
  Add the 1D SUBTYPE records in the S2600CW SDR file.
- Fix the HDD presence error issue.

FCW_112:
- None.

FCW_111:
- EPSD100248748: FRU is not updating correctly

FCW_110:
- None.

FCW_109:
- None

FCW_108:
- EPSD100246883: SDR file contains miss formated records


FCW_107:
- None


FCW_104:
- EPSD100245463: S2600CW SDR Clamp sensors do not agree with chlamp sensor notes


FCW_103:
- None


FCW_102:
- EPSD100244415: A curve ID 0x05 data issue in S2600CW FRUSDR 1.01
- EPSD100026936: SDR auto-update failed on 550W SKU


FCW_101:
- None


FCW_100:
- None


FCW_11:
- None


FCW_10:
- EPSD100243004: Some sensors¡¦ comments and threshold setting are incorrect in SDR file


FCW_09:
- None


FCW_08:
EPSD100242185: Sensors in EWS will show 2 psu1 related sensors after inserting a different type PSU
EPSD100242147: Clone of: There are some unexpected PSU SELs after pull out the PSU


FCW_07:
EPSD100241767: There is no MIC power sensor for installed MIC card


FCW_06:
EPSD100241375: Insert SATA HDD in slot 4~7 but the HDD 4~7 sensor state are all deasserted
EPSD100241568: MIC3 status sensor numer is not correct
EPSD100241219: PI/P2 MTT sensor reading show incorrectly in EWS when memory throttling


FCW_05:
EPSD100240965: Some of system FAN failed to be read on UPM redundancy chassis
EPSD100240718: There are unnecessary events logged for fan redundancy and fan tach sensors during ac cycle stress test
EPSD100241356: ERR2 sensor name is inaccurate in SDR file
EPSD100026166: Sensor reading of MIC Margin is Not Available


FCW_04:
EPSD100240799: set SM signal command fail with BMC20 combo file
EPSD100241000: No SEL record for SDR auto configuration faults


FCW_03:
EPSD100239662: No sensor record define in SDR for BB +3.3V Vbat
EPSD100239697: Agg Thrm Mgn 1/2/3/4/5 sensors¡¯ reading/state are unavailable
EPSD100239929: Sensor reading of CPU1 VRD Temp didn¡¯t change when heating it
EPSD100239989: Clone of: BMC should not restart after FRUSDR Update is done with legacy method (BMC should just run init agent)
EPSD100239995: Clone of: EWS "FRU Information" Help section "FRU Product Information" has extra line item
EPSD100240231: sensor reading of BB +3.3V Vbat is abnormal
EPSD100240386: Processor VRD hot log can't indicate the real hot processor VRD
EPSD100240654: HDD status sensor name is not sequence when two 4x3.5 HSBP inserted
EPSD100240659: HSBP Status sensor removed from  EPS 1.1 (Sensor 69 - 6B)  but defined in SDR


FCW_02:
EPSD100239599: there are OEM Reserved,  (#0xB2)  loges via selview under EFI
EPSD100239620: [system] can not manually change fan speed in FRUSDR001
EPSD100239622: Fan present sensors are not loaded in redundancy chassis
EPSD100239643: Sensor "BMC FW Health" shows warning in EWS on chassis P4308V3XXMFENAPP
EPSD100239654: Sensor reading value is zero for System Airflow
EPSD100239659: SAS IOC Down Temp sensor¡¯s reading/state are unavailable on no sas board
EPSD100239661: There is no MTM Lvl Change sensor record defined in SDR
EPSD100239662: No sensor record define in SDR for BB +3.3V Vbat
EPSD100239663: Status Led still solid green when fan Tach sensor crossed lower non-critical and lower critical threshold
EPSD100239696: P1/P2 MEM VRD Hot sensors¡¯ reading/state are unavailable
EPSD100239697: Agg Thrm Mgn 1/2/3/4/5 sensors¡¯ reading/state are unavailable
EPSD100239887: there is extra one processor VRD  sensor record defined in SDR file
EPSD100239695: Some processor related  sensors' reading/state are unavailable
EPSD100240031: There is no event logged for sensor BMC Watchdog when BMC reset as WDT triggered


FCW_01:
- None.

=============================================================================
                             REFERENCE MATERIAL
=============================================================================
None
[END OF RELEASE NOTES]