How to (update/upload/burn/upgrade/flash) BIOS on the KT MB's.

Ref.: Kontron Technology/MLA/22-11-2009.



From MS-DOS, Windows you can upload a BIOS into the Motherboard like this:

Copy the files xxxxxxxx.rom, BF.EXE and Upd.bat to a directory on your target system.

Execute the Upd.bat

When the writing process is finished reset the board.

Enter BIOS if CMOS setup shall be modified.

Please notice the BF.EXE version must be version 7.21 or higher. By executing BF.EXE from 
DOS you will find the version 7.38 (dated 02/12/2009) displayed as "BFLASH V7.38".


