--------------------------------------------------------------------------------

VENDOR:             Kontron Modular Computers GmbH
SUPPORTED TARGETS:  Kontron KT690/mITX board

This file contains board-specific information for supported target boards.
Specifically, this file contains information on any BSP interface changes
from previous software or hardware versions, and contains caveats that the
user must be aware of before using this BSP. Additionally, the target board's
reference entry (online HTML documentation) provides board-specific information
necessary to run VxWorks, and should be read before this BSP is used.

--------------------------------------------------------------------------------
RELEASE R01.00

	Release for VxWorks 6.8 / Workbench 3.2

	CHIPSET / PROCESSOR:
	- Processor / CPU       : AMD(tm) Athlon Neo X2 Dual Core Processor L325
	- Chipset		: AMD SB600 Embedded
	- Graphics		: ATI Radeon X1250
	- Front Side Bus	: HyperTransport link, 800 MHz
	- MultiProcessing       : UniProcessor (HyperThreading not supported)
	- Main Memory           : 2xSODIMM up to 2GB DDR2
	- Bootdevice(s)         : Gigabit Ethernet Interfaces, CompactFlash,
	                          SATA, PATA HDDs
	- BIOS / BootLoader     : AMI BIOS
	- Power Management	: ACPI 3.0, ACPI 2.0 and APM 1.2

	ON-BOARD PERIPHERALS:
	- PCI                   : 1 x 33/66 MHz
	- PCI-Express           : 2 x (1x) slots
	- Ethernet              : 2 x Intel Gigabit Ethernet (I82567L)
	- USB                   : 10 x USB Host 2.0 (4 x Internal and 6 x external)
	- Serial                : 2 x RS232C
	- Timer                 : System, Auxiliary, Timestamp, Watchdog on WB83627
	- HDD         		: up to 4 SATA150/SATA300 w RAID 0/1 support  2x ATA100	
	- CompactFlash		: CF Type I + II
        - GPIO Port             : 8 lines (routed to FEATURE connector)
	- PS/2 Keyboard
	
	ON-BOARD LOGIC:
	- RealTimeClock (RTC)   : MC146818 compatible
	- Status Indication     : FAN and Temperature sensors on 
				  WB83627 SuperIO controller
	- Watchdog timer	: on WB83627 SuperIO controller

	ADDITIONAL / MIDDLEWARE:
	- Hardware Abstraction Layer
	- Booting via PXE protocol
	- VxWorks ED&R
	- WindRiver System Viewer


--------------------------------------------------------------------------------

