VxWorks 6.8/Workbench 3.2 BSP for Kontron KT690/mITX board

INSTALLATION:	
	NOTE: If you have any of previous versions of the BSP installed 
	DELETE OLD CONTENT before (both 'docs' and 'vxworks-6.8' parts).

	Copy content under VXW68-BSP-KT690 folder to Windriver
	installation folder.

	Restart the Workbench.

QUICKSTART BINARIES:
	bootrom.bin bootrom.pxe: bootloaders to boot from disk or PXE, 
		by default boots VxWorks image via Ethernet slot 0 
		from TFTP host: 10.0.0.99 (file: 'vxWorks')

	vxWorks: VIP project

	both bootloader and vxWorks use Serial Console (COM1, 115200 baud).

