--------------------------------------------------------------------------------

VENDOR:             Kontron Modular Computers GmbH
SUPPORTED TARGETS:  Kontron KTGM45 platform

This file contains board-specific information for supported target boards.
Specifically, this file contains information on any BSP interface changes
from previous software or hardware versions, and contains caveats that the
user must be aware of before using this BSP. Additionally, the target board's
reference entry (online HTML documentation) provides board-specific information
necessary to run VxWorks, and should be read before this BSP is used.

--------------------------------------------------------------------------------
RELEASE R01.04

	Release for VxWorks 6.8 / Workbench 3.2

	Supported Board Features:

	CHIPSET / PROCESSOR:
	- Processor / CPU       : Intel(R) Core(TM)2Duo Mobile
	                          Intel(R) Core(TM)2Quad Mobile incl. T9400
	- Chipset		: Intel GM45 + ICH9M-E Embedded Chipset
	- Graphics		: Intel GMA 4500 MHD graphics
	- Front Side Bus	: 667/800/1067 MHz
	- MultiProcessing       : Symmetric (SMP)
	- Main Memory           : 2xDIMM-240 up to 8GB DDR3
	- Bootdevice(s)         : Gigabit Ethernet Interfaces, CompactFlash,
	                          SATA (AHCI BIOS mode only), ATA HDDs
	- BIOS / BootLoader     : AMI BIOS in 8MB Flash
	- Power Management	: ACPI 3.0, ACPI 2.0 and APM 1.2

	ON-BOARD PERIPHERALS:
	- PCI                   : 1 x 33/66 MHz,
	- PCI-Express           : 1 x 16x 2.0/ SDVO for external graphics card 
				  or ADD2 cards
	                        : 1 x 4x in 16x slot
	- Ethernet              : 3 x Intel Gigabit Ethernet (1õ I82567LM
				  with Intel AMT 4.0 support, and 2x I82574L) 
	- USB                   : 12 x USB 2.0 (8 x Internal and 4 x external)
	- Serial                : 4 x RS232C with FIFO
	- Timer                 : System, Auxiliary, Timestamp, Watchdog
	- HDD         		: up to 4 SATA150/SATA300 w RAID 0/1 support (AHCI BIOS mode only)
				  1x ATA100	(JMicron controller should be enabled in BIOS)
	- CompactFlash		: CF Type I + II (JMicron controller should be enabled in BIOS)
	- PS/2 Keyboard
	- VGA compatible adapter
	
	ON-BOARD LOGIC:
	- RealTimeClock (RTC)   : MC146818 compatible
	- Status Indication     : FAN and Temperature sensors on 
				  WB83627 SuperIO controller

	ADDITIONAL / MIDDLEWARE:
	- Hardware Abstraction Layer
	- Booting via PXE protocol
	- VxWorks ED&R
	- WindRiver System Viewer

--------------------------------------------------------------------------------
