VxWorks 6.8/Workbench 3.2 BSP for Kontron KTGm45 board

INSTALLATION:	
	NOTE: If you have any of previous versions of the BSP installed 
	DELETE OLD CONTENT before (both 'docs' and 'vxworks-6.8' parts).

	Copy content under VXW68-BSP-KTGM45 folder to Windriver
	installation folder.

	Restart the Workbench.

QUICKSTART BINARIES:
	bootrom.bin bootrom.pxe: bootloaders to boot from disk or PXE, 
		by default boots VxWorks image via Ethernet slot 0 
		from FTP host: 192.168.100.1
		(user: 'target' password: 'qq' file: 'vxWorks')

	vxWorks: VIP project with INTEL_AHCI_STORAGE driver and HAL included

	both bootloader and vxWorks use Serial Console (COM1, 115200 baud).

