VxWorks 6.8/Workbench 3.2 BSP for Kontron KTQ45 board

INSTALLATION:	
	NOTE: If you have any of previous versions of the BSP installed 
	delete old content before (both 'docs' and 'vxworks-6.8' parts).

	Copy content under VXW68-BSP-KTQ45 folder to Windriver
	installation folder.

	Restart the Workbench.

QUICKSTART BINARIES:
	bootrom.bin bootrom.pxe: bootloaders to boot from disk or PXE, 
		by default boots VxWorks image from FTP host: 192.168.100.1
		(user: 'target' password: 'qq' file: 'vxWorks' + 'vxWorks.sym')

	vxWorks: VIP project with all 3 NIC ethernet configurred,
		gei0 is configured with IP 192.168.100.10
		gei1 and gei2 are set up to retrieve configuration by DHCP

	both bootloader and vxWorks use Serial Console (COM1) at 115200baud speed.

