VxWorks 6.9/Workbench 3.3 BSP

SYSTEM REQUIREMENTS:
	VxWorks 6.9 updated to 6.9.3
BIOS setup: (tested with ID KTQ45013)
	Exit -> Load Optimal Defaults
	Advanced -> IDE Configuration -> Configure SATA#1 as: [AHCI]
  for PXE boot:
	Advanced -> LAN Configuration -> ETH1 Configuration (Right): [With RPL/PXE boot]
			

INSTALLATION:	
	NOTE: If you have any of previous versions of the BSP installed 
	DELETE OLD CONTENT before (at least target/config/kontron_ktq45).

	Copy all content under VXW-BSP folder to Windriver
	installation folder.

	Restart the Workbench.

QUICKSTART BINARIES:
	bootrom.bin bootrom.pxe: bootloaders to boot from disk or PXE, 
				 use Serial Console (COM1, 115200 8N1).
	vxWorks - development profile image (uses the same console)
	the image runs in SMP mode

