--------------------------------------------------------------------------------

VENDOR:             Kontron AG
SUPPORTED TARGETS:  Kontron KTQ45/Flex platform

This file contains board-specific information for supported target boards.
Specifically, this file contains information on any BSP interface changes
from previous software or hardware versions, and contains caveats that the
user must be aware of before using this BSP. Additionally, the target board's
reference entry (online HTML documentation) provides board-specific information
necessary to run VxWorks, and should be read before this BSP is used.

--------------------------------------------------------------------------------
RELEASE R03.00

	Release for VxWorks 6.9.3.3 / Workbench 3.3.3

	Supported Board Features:

	CHIPSET / PROCESSOR:
	- Processor / CPU       : Intel Core2 Duo & Intel Core2 Quad incl. 
	                          E8400 & Q9650 desktop CPU
	- Chipset               : Intel Q45 + ICH10DO Embedded Chipset
	- Graphics              : Intel GMA 4500 graphics CRT output
	- Front Side Bus        : 800/1066/1333 MHz
	- MultiProcessing       : Symmetric (SMP)
	- Main Memory           : 4x DIMM-240 for up to 8 GB DDR3
	- Bootdevice(s)         : Gigabit Ethernet Interfaces, USB drive,
	                          SATA HDD
	- BIOS / BootLoader     : AMI BIOS in 8MB Flash
	- Power Management      : ACPI 3.0, ACPI 2.0 and APM 1.2

	ON-BOARD PERIPHERALS:
	- PCI                   : 2 x 33/66 MHz,
	- PCI-Express           : 1 x 16x 2.0/ SDVO for external graphics card 
	                          1x PCI-Express 4x in 16x slot
	- Ethernet              : 2x Intel Gigabit Ethernet, one with Intel AMT 5.0 support 
	- USB                   : 12 x USB 2.0 (4 x Internal and 8 x external)
	- Serial                : 2 x RS232C with FIFO
	- Timer                 : System, Auxiliary, Timestamp, Watchdog
	- HDD                   : up to 5 SATA150/SATA300
	- PS/2 Keyboard
	- VGA compatible adapter
	- Parallel port         : Parallel Port with SPP, ECP or EPP mode, via internal connector
	- GPIO                  : W83627 8 pins on the FEATURE connector
	- Hardware monitor      : W83627 temperature/voltage sensors 
	
	ON-BOARD LOGIC:
	- RealTimeClock (RTC)   : MC146818 compatible
	- Status Indication     : Temperature, fan and voltages

	ADDITIONAL / MIDDLEWARE:
	- KEAPI v2 
	- Booting via PXE protocol
	- VxWorks ED&R
	- WindRiver System Viewer

--------------------------------------------------------------------------------

SYSTEM REQUIREMENTS:
	VxWorks 6.9.3.3
	Exit -> Load Optimal Defaults
	Advanced -> IDE Configuration -> Configure SATA#1 as: [AHCI]
  for PXE boot:
	Advanced -> LAN Configuration -> ETH1 Configuration (Right): [With RPL/PXE boot]

KNOWN PROBLEMS and LIMITATIONS

 - Multistage boot pxe is not supported;
