VxWorks 6.8/Workbench 3.2 BSP

INSTALLATION:	
	NOTE: If you have any of previous versions of the BSP installed 
	DELETE OLD CONTENT before (target/config/kontron_ktq45).

	Copy underlying content from the VXW68-BSP folder to the Windriver installation folder.

	Restart the Workbench.

QUICKSTART BINARIES:
	bootrom.bin bootrom.pxe: bootloaders to boot from disk or PXE, 
				 use Serial Console (COM1, 115200 8N1).
	vxWorks - development profile image (uses the same console)

SYSTEM REQUIREMENTS:
	see release_notes.txt