--------------------------------------------------------------------------------

VENDOR:             Kontron Modular Computers GmbH
SUPPORTED TARGETS:  Kontron KTUS15/mITX board

This file contains board-specific information for supported target boards.
Specifically, this file contains information on any BSP interface changes
from previous software or hardware versions, and contains caveats that the
user must be aware of before using this BSP. Additionally, the target board's
reference entry (online HTML documentation) provides board-specific information
necessary to run VxWorks, and should be read before this BSP is used.

--------------------------------------------------------------------------------
RELEASE R01.00

	Release for VxWorks 6.8 / Workbench 3.2

	CHIPSET / PROCESSOR:
	- Processor / CPU       : Intel(R) Atom(TM) Z510/Z530
	- Chipset		: Intel SCH US15W
	- Graphics		: Intel GMA 500
	- Front Side Bus	: 400/533 MHz
	- MultiProcessing       : UniProcessor (HyperThreading not supported)
	- Main Memory           : 1xSODIMM up to 2GB DDR2
	- Bootdevice(s)         : Gigabit Ethernet Interfaces, CompactFlash,
	                          SATA, PATA HDDs
	- BIOS / BootLoader     : AMI BIOS
	- Power Management	: ACPI 3.0, ACPI 2.0 and APM 1.2

	ON-BOARD PERIPHERALS:
	- PCI                   : 1 x 33/66 MHz
	- PCI-Express           : 2 x (1x) slots
        - SD card interface     : 2 slots (Not supported)
	- Ethernet              : 1 x Intel Gigabit Ethernet (I82574L) 
	- USB                   : 8 x USB Host 2.0 (4 x Internal and 4 x external)
                                  1 x USB Device (shared with USB2 connector, not supported)
	- Serial                : 2/4 x RS232C
	- Timer                 : System, Auxiliary, Timestamp
	- HDD         		: up to 2 SATA150/SATA300 w RAID 0/1 support
				  2x ATA100	
	- CompactFlash		: CF Type I + II
        - GPIO Port             : 8 lines (routed to FEATURE connector)
	- PS/2 Keyboard
	
	ON-BOARD LOGIC:
	- RealTimeClock (RTC)   : MC146818 compatible
	- Status Indication     : FAN and Temperature sensors on 
				  WB83627 SuperIO controller



--------------------------------------------------------------------------------

BSP R01.00 limitations:

- Supports JMicron SATA controller AHCI/RAID mode only;
- For project "System Image" with PROFILE_BOOTAPP the component WDB_FOLDER 
should be excluded manually;
     