VxWorks 6.8/Workbench 3.2 BSP for Kontron KTUS15/mITX board

INSTALLATION:	
	NOTE: If you have any of previous versions of the BSP installed 
	delete old content before (both 'docs' and 'vxworks-6.8' parts).

	Copy content under VXW68-BSP-KTUS15 folder to Windriver
	installation folder.

	Restart the Workbench.

