--------------------------------------------------------------------------------

VENDOR:             Kontron Modular Computers GmbH
SUPPORTED TARGETS:  Kontron MOPSlcdLX

This file contains board-specific information for supported target boards.
Specifically, this file contains information on any BSP interface changes
from previous software or hardware versions, and contains caveats that the
user must be aware of before using this BSP. Additionally, the target board's
reference entry (online HTML documentation) provides board-specific information
necessary to run VxWorks, and should be read before this BSP is used.
--------------------------------------------------------------------------------
RELEASE R01.02

	Release for VxWorks 6.3 / Workbench 2.5 based on pcPentium BSP

	Supported Board Features:

	KEY:
	- Processor / CPU       : AMD Geode LX800 500 MHz
	- Main Memory           : up to 1GB DDR200/DDR266
	- Bootdevice(s)         : Fast Ethernet Interface, Floppy, ATA HDD
	- BIOS / BootLoader     : AWARD BIOS

	CHIPSET / PROCESSOR:
	- PCI                   : 33 Mhz, 32bit, 3.3V
        - ISA                   : AT/XT 
	- Timer                 : System, Auxiliary, Timestamp

	ON-BOARD PERIPHERALS:
	- Mass Storage          : Single channel ATA-controller: up to 2 ATA HDDs
	- Ethernet              : 1 x 10/100 Base-T Fast Ethernet (I82551ER)
	- USB                   : 2 x USB 2.0 ports
	- Serial                : 2 x RS232
        - Parallel              : 1 x LPT
        - Watchdog              
        - RTC


	ADDITIONAL / MIDDLEWARE:

	FIXED PDR (Product Discrepancy Reports):

        KNOWN ISSUES:
        - VxBus is supported by GNU compiler only
        - including OHCI/EHCI controller driver causes the system crash 
          during startup;
        - enabling FD driver while it's disabled at the BIOS causes 
          the bootloader/OS hang;
--------------------------------------------------------------------------------

