Digital-Logic AG XP Embedded BSP
================================

Version History
---------------

28.12.2009 DIP Version 1.5
- Added "Selector Prototype Component" as prototype for SMA200 Hardware selector

07.09.2009 DIP Version 1.4
- Added Intel Embedded Video driver for SMX945 based boards

23.01.2009 DIP Version 1.3
- Updated Int15 driver with support for A200 boards
- Updated Int15 tools with support for A200 boards
- Added SiI3132 SATA driver
- Added Intel 82574L Gigabit Ethernet driver
- Added Chipset driver for A200 based bords
- Added Sound driver for A200 based boards
- Added Graphic driver for A200 based boards
- Updated boot logo component (copy bootlogo into C:\boot.bmp)

10.12.2008 DIP Version 1.2.1
- Corrected Repository path in LX800\Chipset\DLAG LX800 Crypto AES.sld

02.06.2008 DIP Version 1.2
- Removed dependency "USB Boot V2.0" from SMX945 Usb drivers.
  Now the behavoir should be as in XP Pro.
  To restore the prevoius behaviour add "USB Boot V2.0" manually.

- Updated SMX945 integrated video controller driver to Version 6.14.10.4926

25.02.2008 DIP Version 1.1
- Added dependency for LX800 Video input driver

