VxWorks 6.8/Workbench 3.2 BSP



SYSTEM REQUIREMENTS:

	VxWorks 6.8 updated to 6.8.2
	BIOS setup: (make sure you have BIOS version KCC.21.02 or higher
	* Save & Exit -> Restore Defaults
	* Save & Exit -> Save Changes
	* Advanced -> Launch PXE OpROM [Enabled]
	* Save & Exit -> Save Changes and Reset
	The network will be used by default in this case.

INSTALLATION:	

	NOTE: If you have any of previous versions of the BSP installed 
	DELETE OLD CONTENT before (at least target/config/kontron_msmst).

	Copy all content under VXW68-BSP folder to Windriver
	installation folder.

	Restart the Workbench.

QUICKSTART BINARIES:

	bootrom.bin bootrom.pxe: bootloaders to boot from disk or PXE, 
				 use Serial Console (COM1, 115200 8N1).
	vxWorks - development profile image (uses the same console)
	the SMP mode is unsupported
