--------------------------------------------------------------------------------

VENDOR:             Kontron (KGSC)
SUPPORTED TARGETS:  Kontron MSMST board

This file contains board-specific information for supported target boards.
Specifically, this file contains information on any BSP interface changes
from previous software or hardware versions, and contains caveats that the
user must be aware of before using this BSP. Additionally, the target board's
reference entry (online HTML documentation) provides board-specific information
necessary to run VxWorks, and should be read before this BSP is used.

--------------------------------------------------------------------------------
RELEASE R01.00

	Release for VxWorks 6.8.2 / Workbench 3.2 	

	CHIPSET / PROCESSOR:
	- Processor / CPU       : Intel(R) Atom(TM) E6X5CT series
	- Chipset		: Intel(R) Tunnel Greek
	- Graphics		: Intel(R) Tunnel Greek
	- Front Side Bus	: 0.6/1.0/1.3 GHz
	- MultiProcessing       : UniProcessor (HyperThreading not supported)
	- Main Memory           : 1 or 2 GB DDR2
	- Bootdevice(s)         : Gigabit Ethernet Interface, SATA HDDs
	- BIOS / BootLoader     : AMI BIOS
	- Power Management	: ACPI 3.0, ACPI 2.0 and APM 1.2

	ON-BOARD PERIPHERALS:
	- PCI-Express           : 3 x PCIe x1, 4 x PCIe x1 
	- Ethernet              : 1 x Intel Gigabit Ethernet MAC
	- USB                   : 2 x USB 1.1/2.0/3,0
	- Serial                : 2 x RS232C
	- Timer                 : System, Auxiliary, Timestamp
	- HDD         		: up to 2 SATA300, RAID mode is not supported 
	
	ON-BOARD LOGIC:
	- RealTimeClock (RTC)   : MC146818 compatible

	ADDITIONAL / MIDDLEWARE:
	- Booting via PXE protocol
	- VxWorks ED&R
	- WindRiver System Viewer


--------------------------------------------------------------------------------

KNOWN PROBLEMS and LIMITATIONS

 - PROFILE_BOOTAPP doesn't work for a GNU toolchain
   It is recommended to build bootloader as "VxWorks bootloader project" 
   or use the diab toolchain.
 - the VxWorks.sym can't be loaded from a SATA disk 
   (use INCLUDE_STANDALONE_SYM_TBL)
 - KEAPI is implemented at prototype level only
 - USB is not supported
