Silicon Image SiI 3132 SATALink Controller and NEC uPD720200 USB3 Controller

Driver Installation Instructions

# Windows XP SP3 Fresh Installation

Follow the instructions in this section if you are performing a new installation of Windows XP SP3.

Copy all Files in the TXT_DRIVER_USB_SATA folder to a diskette and connect a USB Floppy drive to the MSMST.

1. Put your Windows XP SP3 CD into the CD/DVD-ROM drive.

2. Press F6 for third party SCSI or driver installation at the beginning of text mode installation. Insert the SATA and USB TXT driver diskette and press 's' (‘z’ on German version) when setup asks if you want to specify an additional device.

3. From the menu presented next, select ‘Renesas Electronics USB 3.0 Host Controller’ and press 'Enter'.

4. Press 's' when setup asks if you want to specify an additional device.

5. From the menu presented next, select ‘Renesas Electronics USB 3.0 Hub’ and press 'Enter'.

6. Press 's' when setup asks if you want to specify an additional device.

7. From the menu presented next, select ‘Silicon Image SiI 3132 SATALink Controller for Windows XP’ and press 'Enter'.

8. Press 'Enter' again when prompted to continue on with text mode setup.

9. Follow the setup instructions to select your choice for partition and file system.

10. After setup examines your disks, it will copy files from the CD to the hard drive selected above and restart the system. After restart the setup process will resume to finish the installation.