DAVICOM DM9PCI NDIS 2 Driver Installation Guide for PC-NFS

* Installing PC-NFS Software
1. Insert PC-NFS diskette 1 into drive A.
2. Change to driver A and enter INSTALL at command prompt
3. Specify "C:\NFS" as installation directory
4. Select "Ethernet" network connect
5. Use a manufacturer's NDIS driver
6. Specify "C:\NFS" as the target NDIS driver installation directory
7. Follow the instructions in the installation program

* Install NDIS driver for PC-NFS
1. Insert PC-NFS QUIKNDIS diskette into drive A.
2. Change to driver A and enter QUIKNDIS at command prompt
3. Select "Custom" type NDIS driver
4. Specify the full path of the directory containing the NDIS driver
5. Specify "DM9PCI" as .NIF file
6. use the current DRIVERNAME "DM9PCI$"
7. Select "Go ahead and modify"

* Configuring PC-NFS Software
1. Edit a file in C:\NFS named HOSTS containing the following items
	<local host IP address> 	<local host name>
	<server IP addres>		<server 1 name>
	<PCNFSD server IP address>	<PCNFSD name>
	<gateway IP address>		<gateway name>
2. Start NFSCONF program
3. From the Network menu, select "Direct Connect" to configure
   network connection

* Accessing network file with DOS
1. At the DOS prompt, enter NFSCONF
2. From the Resource menu, choose "Define Drive"
3. Enter the information requested.
4. After you return to DOS, you can access the file system by entering
   the driver letter you assigned to it followed by a colon.

For more detail information, refer to the manuals of PC-NFS published
by Sun Microsystem, Inc.
