
[+******************************************************************+]
[                     DAVICOM Semiconductor Inc.                     ]
[                  PCI Fast Ethernet Adapter (DM9102)                ]
[                 32-Bit ODI Driver Installation Guide               ]
[                                                                    ]
[          (C) Copyright 1997-2000 DAVICOM Semiconductor Inc.        ]
[                         All Rights Reserved.                       ]
[-******************************************************************-]


DM9102 supports the 32-Bit ODI Driver (SPEC. v3.31) (DM9PCI.LAN)
for all version Netware Server and Client 32 for DOS/Windows 95/
Windows 3.1.


Topics :
========

     I. Netware 4.11 Server 32-Bit ODI Driver Installation


Files Description :
===================

  \NW411\NW411.TXT      This file.


I. Netware 4.11 Server 32-Bit ODI Driver Installation
=====================================================

      1. Turn OFF your PC machine.
      2. Plug the DM9102 PCI Fast Ethernet Adapter into the PCI slot
         of PC machine.
      3. Reboot your PC machine to DOS prompt.
      4. Copy the NBI.NLM, MSM.NLM, ETHERTSM.NLM files from the Driver
         diskette to Netware directory.

           C:\NWSERVER> COPY A:\NW50\NW4X\*.NLM .

      5. Startup your Netware 4.11 Server.
      6. Load updated NBI, MSM, ETHERTSM modules on Netware console.

           NW411: LOAD C:NBI.NLM
           NW411: LOAD C:MSM.NLM
           NW411: LOAD C:ETHERTSM.NLM

      7. Run "LOAD INSTALL" on Netware console.

           NW411: LOAD INSTALL

      7. Select "Driver options" in the Installation Options.
      8. Select "Configure network drivers" in the Driver Options.
      9. Select "Select a driver" in the Additional Driver Actions.
     10. Press <Insert> key to install an unlisted driver.
     11. Press <F3> key to specify a different path.
     12. Insert the Driver diskette to the floppy (Drive A) and
         enter "A:\NW50" to specify a directory path.
     13. Select "DAVICOM PCI Fast Ethernet Adapter (DM9102) 32-Bit ODI
         (SPEC v3.31) MLID" to install.
     14. Enter the HIN Slot Number to the Slot field of the driver parameters.
     15. Choose the driver optional parameters (Media Mode, Line Speed),
         if NO value, it will be the default value.

           Media Mode : the default is AUTODETECT. (AUTODETECT, AUTOFULL,
                        AUTOHALF, 100FULL, 100HALF, 10FULL, 10HALF, 1M,
                        1MHSLP, 1MHSHP, 1MLSLP, 1MLSHP)
    Rx Remote Command : the default is Disable Rx Remote Command.
                        (Set RXCMD to Enable Rx Remote Command)
  Send Remote Command : the default is Disable Send Remote Command.
                        (Set SENDCMD to Enable Send Remote Command)
      Rx Flow Control : the default is Disable Rx Flow Control.
                        (Set RXFLW to Enable Rx Flow Control)
      Tx Flow Control : the default is Disable Tx Flow Control.
                        (Set TXFLW to Enable Tx Flow Control)
          Virtual LAN : the default is Disable VLAN function.
                        (Set VLAN to Enable VLAN function)
           Line Speed : NO default value. (SPEED=10, SPEED=100)

     16. Select "Save parameters and load driver" to load DM9PCI driver.
     17. Following the screen prompt to complete the driver installation.
     18. Login one workstation to the Netware server, and copy the
         NBI.NLM, MSM.NLM, ETHERTSM.NLM files from the Driver diskette
         to SYSTEM directory.

           F:\SYSTEM> COPY A:\NW50\NW4X\*.NLM .


<<< End of file >>>

