The follow paramenters are used in AUTOEXEC.NCF file of Novell Server to 
setup the DM9102AF/DM9102F/DM9009/DM9102AF+DM9801/DM9102AF+DM9802 adapter
(10/100 Fast Ethernet,10 Ethernet,1/10/100 Fast Ethernet LongRun/HomeRun)
                       
           Media Mode : the default is AUTODETECT. (AUTODETECT, AUTOFULL,
                        AUTOHALF, 100FULL, 100HALF, 10FULL, 10HALF, 1M,
                        1MHSLP, 1MHSHP, 1MLSLP, 1MLSHP)
    Rx Remote Command : the default is Disable Rx Remote Command.
                        (Set RXCMD to Enable Rx Remote Command)
  Send Remote Command : the default is Disable Send Remote Command.
                        (Set SENDCMD to Enable Send Remote Command)
      Rx Flow Control : the default is Disable Rx Flow Control.
                        (Set RXFLW to Enable Rx Flow Control)
      Tx Flow Control : the default is Disable Tx Flow Control.
                        (Set TXFLW to Enable Tx Flow Control)
          Virtual LAN : the default is Disable VLAN function.
                        (Set VLAN to Enable VLAN function)
           Line Speed : the default is Autodetect Ethernet Line Speed. 
                        (SPEED=10,100,500,1400,1600)
           ps:SPEED=500,1400,1600 for LongRun/HomeRun to setup speed.
     
<<< End of file >>>

