The fllow parameters are used in NET.CFG file of DOS/ODI client for user 
to setup the DM9102AF/DM9102F/DM9009/DM9102AF+DM9801/DM9102AF+DM9802 adapter
(10/100 Fast Ethernet,10 Ethernet,1/10/100 Fast Ethernet LongRun/HomeRun)

        SLOT 1          ;;Select Slot Number (FIRST Board)
        AUTO            ;;Autodetect 1M Home PNA and 10M/100M Ethernet Mode (Default)
        AUTOFULL        ;;Forced to Ethernet Full_Duplex (Auto-Speed) Mode
        AUTOHALF        ;;Forced to Ethernet Half_Duplex (Auto-Speed) Mode
        100FULL         ;;Forced to Ethernet 100M Full_Duplex Mode
        100HALF         ;;Forced to Ethernet 100M Half_Duplex Mode
        10FULL          ;;Forced to Ethernet 10M Full_Duplex Mode
        10HALF          ;;Forced to Ethernet 10M Half_Duplex Mode
        SPEED 100       ;;Forced to Ethernet 100M Mode
        SPEED 10        ;;Forced to Ethernet 10M Mode
        1M              ;;Forced to 1M Home PNA Mode (the same as 1MHSLP)
        NODE ADDRESS 0223456789AB    ;;Set Override Node Address

;***************************************************************************
; THE FOLLOWING PARAMETERS ARE USED ONLY FOR 1M HOME PNA SPECIFIC PURPOSE. *
; THE GENERAL USER DON'T NEED TO CARE ABOUT THE FOLLOWING PARAMETERS.      *
;***************************************************************************
        1MHSLP          ;;Forced to 1M Home PNA High Speed/Low Power Mode
        1MHSHP          ;;Forced to 1M Home PNA High Speed/Low Power Mode
        1MLSHP          ;;Forced to 1M Home PNA High Speed/Low Power Mode
        1MLSLP          ;;Forced to 1M Home PNA High Speed/Low Power Mode
        RXCMD           ;;Enable to accept 1M Remote Command
        SENDCMD         ;;Enable to send 1M Remote Command
        RXFLW           ;;Enable Rx Flow Control
        TXFLW           ;;Enable Tx Flow Control
        VLAN            ;;Enable VLAN Function
        SPEED1600       ;;For TUT LongRun Switch and HomeRun adapter support Speed 1600Kbps
        SPEED1400       ;;For TUT LongRun Switch and HomeRun adapter support Speed 1400Kbps
        SPEED500        ;;For TUT LongRun Switch and HomeRun adapter support Speed 500Kbps


