
[+******************************************************************+]
[                     DAVICOM Semiconductor Inc.                     ]
[                  PCI Fast Ethernet Adapter (DM9102)                ]
[                 32-Bit ODI Driver Installation Guide               ]
[                                                                    ]
[          (C) Copyright 1997-2000 DAVICOM Semiconductor Inc.        ]
[                         All Rights Reserved.                       ]
[-******************************************************************-]


DM9102 supports the 32-Bit ODI Driver (SPEC. v3.31) (DM9PCI.LAN)
for all version Netware Server and Client 32 for DOS/Windows 95/
Windows 3.1.


Topics :
========

     I. Netware 3.12 Server 32-Bit ODI Driver Installation


Files Description :
===================

  \NW312\NW312.TXT      This file.


I. Netware 3.12 Server 32-Bit ODI Driver Installation
=====================================================

      1. Turn OFF your PC machine.
      2. Plug the DM9102 PCI Fast Ethernet Adapter into the PCI slot
         of PC machine.
      3. Reboot your PC machine to DOS prompt.
      4. Copy DM9PCI.LAN, NBI31x.NLM, MSM31x.NLM, ETHERTSM.NLM files
         from the Driver diskette to Netware directory.

           C:\SERVER.312> COPY A:\NW50\DM9PCI.LAN .
           C:\SERVER.312> COPY A:\NW50\NW312\*.NLM .

      5. Startup your Netware 3.12 Server.

           C:\SERVER.312> SERVER

      6. Load NBI31x, MSM31x, ETHERTSM, DM9PCI modules on Netware console.

           : LOAD C:NBI31x
           : LOAD C:MSM31x
           : LOAD C:ETHERTSM
           : LOAD C:DM9PCI


<<< End of file >>>

