
[+******************************************************************+]
[                     DAVICOM Semiconductor Inc.                     ]
[                  PCI Fast Ethernet Adapter (DM9102)                ]
[                    ODI Driver Installation Guide                   ]
[                                                                    ]
[          (C) Copyright 1997-2000 DAVICOM Semiconductor Inc.        ]
[                         All Rights Reserved.                       ]
[-******************************************************************-]

        A) Install DOS ODI Driver on Netware Server

Files Description :
===================

  \DOSODI\DM9PCI.COM    DM9102 DOS ODI Driver
  \DOSODI\DM9PCI.INS    DM9102 DOS ODI Driver Installation File

A) Install DOS ODI Driver on Netware Server
===========================================

   1. Turn OFF your PC machine.
   2. Plug the DM9102 PCI Fast Ethernet Adapter into the PCI slot
      of PC machine.
   3. Reboot your PC machine to DOS prompt.
   4. Insert the Driver diskette to the floppy (Drive A) and
      run the following command to log into the Netware server.

        C:\> A:
        A:\> CD \DOSODI
        A:\DOSODI> STARTNET.BAT

   5. Change directory to Netware Client installation directory.

        F:\> CD \PUBLIC\CLIENT\VLM\IBM_6    (for Netware 4.11)
        (or F:\> CD \PUBLIC\CLIENT\DOSWIN for Netware 4.10)

   6. Run "INSTALL" to install the Netware Client files.

        F:\PUBLIC\CLIENT\VLM\IBM_6> INSTALL.EXE

   7. Select "Select the driver for your network board."
      to install driver.
   8. Insert the Driver diskette to the floppy (Drive A) and
      enter "A:\DOSODI" to specify a directory path.
   9. Select "DAVICOM PCI Fast Ethernet Adapter (DM9102)" to configure
      driver parameters.
  10. Select "DAVICOM PCI Fast Ethernet Adapter (DM9102)" in Network Board
      to configure driver parameters.
  11. Choose the driver parameter (Line Speed, Media Type),
      if NO value, it will be the default value.

           Media Type : the default is AUTO. (AUTO, AUTOFULL, AUTOHALF,
                        100FULL, 100HALF, 10FULL, 10HALF, 1M, 1MHSLP,
                        1MHSLP, 1MHSHP, 1MLSLP, 1MLSHP)
    Rx Remote Command : the default is Disable Rx Remote Command.
                        (Set RXCMD to Enable Rx Remote Command)
  Send Remote Command : the default is Disable Send Remote Command.
                        (Set SENDCMD to Enable Send Remote Command)
      Rx Flow Control : the default is Disable Rx Flow Control.
                        (Set RXFLW to Enable Rx Flow Control)
      Tx Flow Control : the default is Disable Tx Flow Control.
                        (Set TXFLW to Enable Tx Flow Control)
          Virtual LAN : the default is Disable VLAN function.
                        (Set VLAN to Enable VLAN function)
           Line Speed : NO default value. (10, 100)

  12. Press <F10> key to save the driver parameters into NET.CFG file.
  13. Select "Highlight here and press <Enter> to Install."
      to complete the driver installation.


<<< End of file >>>

