TSC-10/DD Revised version history

Ver 3.08.72P -> 3.08.74P (March 30, 2007)
Revision: We released a driver for 5 wire touch screen controller.
Revision: Changed not to accept double click on calibration screen.
Revision: Changed default setting of Timeout to 15.
Corrected: When you added a device, the problem which the same name was displayed was corrected.
Corrected: The problem which a device cannot choose on a property screen was corrected.
Corrected: The problem which program (tbsystry.exe) works without intending in the vicinity of 0:00 a.m. was corrected.
Corrected: When you used the system which a component about beep was not included in, the problem which it did not work normally was corrected.

Ver 3.08.70P -> 3.08.72P (August 11, 2006)
Corrected: Sound duration was corrected.

Ver 3.08.68P -> 3.08.70P (May 26, 2006)
Revision: Supports graphics cards that use stretched desktop modes.
Corrected: The problem which data were stored in spite of Timeout after having first EEPROM calibration was corrected.

ver 3.08.66P -> ver 3.08.68P (March 31, 2006)
Corrected: When not displaying an icon on the system tray and enable/disable of an EEPROM calibration were repeated, the problem which the order of the display of calibration point replaces was corrected.
Corrected: When the EEPROM calibration was performed and repeated, the problem in which the computer works abnormally was corrected.

ver 3.08.52P -> ver 3.08.66P (December 1, 2005)
Revision: The function in which the operation area of a touch screen can be specified arbitrarily is added.
Revision: The indicator is added after EEPROM calibration.
Corrected: The hot plug function was improved.
Corrected: In some hardware, the problem the beep when carrying out a calibration does not sound was corrected.
Corrected: When the operation area of a touch screen was made into a right half, and the EEPROM calibration was performed, the problem which cannot carry out position compensation normally was corrected.

ver 3.08.50P -> ver 3.08.52P (January 27, 2005)
Revision: Applicable OS is changed into Windows 2000/XP.
Revision: The function of redetecting a PnP device was deleted.

ver 3.08.46P -> ver 3.08.50P (December 24, 2004)
Revision: The function of redetecting a PnP device was added.
Corrected: In multi-monitor environment, when only a monitor 2 performs a calibration, the issue which the dialog box for checking was displayed on a monitor 1 was corrected.
Corrected: In multi-monitor environment, after finishing a calibration on a monitor 1, a calibration is continuously performed on a monitor 2. At calibration screen on monitor 2, the issue which calibration data is saved even if it presses the ESC key or it becomes time out was corrected.

ver 3.08.44P -> ver 3.08.46P (September 17, 2004)
Corrected: The backlight is woken up when cursor is in a right edge of a screen. After that, the backlight is turns off once again, without doing anything. Then, in some hardware, the problem that a touch loses its effect was corrected.

ver 3.08.42P -> ver 3.08.44P (September 14, 2004)
Revision: The touch in the outside of calibration area becomes effective.
Corrected: In WindowsNT4Workstation, the problem as which an error log is displayed was corrected.

ver 3.08.40P -> ver 3.08.42P (July 23, 2004)
Corrected: In some hardware, the problem which cannot return in one touch input from standby mode was corrected.
Corrected: In Windows 2000, when doing nothing without starting a screen saver, the problem which does not carry out click operation of the first touch was corrected.

ver 3.08.38P -> ver 3.08.40P (May 21, 2004)
Corrected: When the prompt which enters a password is displayed after making computer resume with a keyboard or a mouse from standby mode, the problem that a touch loses its effect was corrected.
Corrected: A back light is restored when a host receives independent 10h.

ver 3.08.32P -> ver 3.08.38P (February 20, 2004)
Revision: The addition of the function which fixes the problem generated by the non-compatibility of the COM port in some hardwares.

ver 3.08.16P -> ver 3.08.32P (Nobember 7, 2003)
Revision: When using a USB controller. "Unknown" which is in "Init state" item of the Status tab was changed into the blank.
Revision: It copes with Windows95, Windows98(SE), WindowsME, WindowsNT4Workstation and Windows2000Professional in addition to WindowsXP, too.

ver 3.08.06P -> ver 3.08.16P (January 30, 2003)
Revision: Only for WindowsXP.
Corrected: At calibration screen, the problem which calibration data is saved even if it presses the ESC key or it becomes time out was corrected.
Corrected: When the dialog of a "Check Calibration" is displayed, inputting other place is continued without pushing the "OK" button. The problem which calibration data is saved even if it becomes time out was corrected.

ver 3.05.22P -> ver 3.08.06P (November 25, 2002)
Revision: Id and Port item were added in the devices tab of property window. Similarly in a device tab, the function which the item of the controller is displayed in a red character when a cantroller cannot be used was added.
Revision: Deglitch function was added in the Advanced tab of property window.
Corrected: In Windows98(SE), when touching the inside of the MS-DOS prompt window on Windows, the problem that coordinates shift was corrected.
Corrected: In Windows95, when an IPX/SPX-compatible protocol and Microsoft network share service are installed as a network component, the problem that a touch loses its effect was corrected.

ver 3.05.16P -> ver 3.05.22P (September 30, 2002)
Revision: When cursor is in the right end of a screen and the back light of LCD is OFF. A back light is restored when a host receives independent 10h.

ver 3.05.06P -> ver 3.05.16P (July 12, 2002)
Corrected: OS is installed to PC when a USB function is OFF on BIOS. The fault that a serial controller does not operate is corrected.

ver 3.05.00P -> ver 3.05.06P (May 1, 2002)
Revision: It copes with Windows95, Windows98(SE), WindowsME, WindowsNT4Workstation and Windows2000Professional in addition to WindowsXP, too.
Revision: A clone function was added.

ver 3.04.00P -> ver 3.05.00P (March 7, 2002)
Revision:  It copes with a multi-touch screen.
Corrected: When this software is installed, "stop of the installation" is chosen, and a driver is loaded. After that, the problem that a PC restarts when it is inputted to the touch screen is corrected.
Corrected: When installation is done with a USB controller connected to the PC before installing this software, the problem that the number of USB controllers increases and it is indicated is corrected.

ver 3.04.00P (February 19, 2002)
    An upgrade along with the complete code renewal.
    ver3.x first release.