<Linux device driver for Realtek Ethernet controllers>

	This is the Linux device driver released for RealTek RTL8168B/8111B 
	and RTL8168C/8111C, Gigabit Ethernet controllers with PCI-Express 
	interface.

<Requirements>

	- Kernel source tree (supported Linux kernel 2.6.x and 2.4.x)
	- For linux kernel 2.4.x, this driver supports 2.4.20 and latter.
	- Compiler/binutils for kernel compilation

<Quick install with proper kernel settings>

	Unpack the tarball :
		# tar vjxf r8168-8.aaa.bb.tar.bz2

	Change to the directory:
		# cd r8168-8.aaa.bb

	If you are running the target kernel, then you should be able to do :

		# make clean modules	(as root or with sudo)
		# make install
		# depmod -a
		# insmod ./src/r8168.ko (or r8168.o in linux kernel 2.4.x)

	You can check whether the driver is loaded by using following commands.

		# lsmod | grep r8168
		# ifconfig -a

	If there is a device name, ethX, shown on the monitor, the linux 
	driver is loaded. Then, you can use the following command to activate 
	the ethX.

		# ifconfig ethX up

		,where X=0,1,2,...

<Set the network related information>
	1. Set manually
		a. Set the IP address of your machine.

			# ifconfig ethX "the IP address of your machine" 

		b. Set the IP address of DNS.

		   Insert the following configuration in /etc/resolv.conf.
		
			nameserver "the IP address of DNS"

		c. Set the IP address of gateway.

			# route add default gw "the IP address of gateway"

	2. Set by doing configurations in /etc/sysconfig/network-scripts
	   /ifcfg-ethX for Redhat and Fedora, or /etc/sysconfig/network
	   /ifcfg-ethX for SuSE. There are two examples to set network 
	   configurations.

		a. Fix IP address:
			DEVICE=eth0
			BOOTPROTO=static
			ONBOOT=yes
			TYPE=ethernet
			NETMASK=255.255.255.0
			IPADDR=192.168.1.1
			GATEWAY=192.168.1.254
			BROADCAST=192.168.1.255

		b. DHCP:
			DEVICE=eth0
			BOOTPROTO=dhcp
			ONBOOT=yes	

<Modify the MAC address>
	There are two ways to modify the MAC address of the NIC.
	1. Use ifconfig:

		# ifconfig ethX hw ether YY:YY:YY:YY:YY:YY

	   ,where X is the device number assigned by Linux kernel, and
		  YY:YY:YY:YY:YY:YY is the MAC address assigned by the user.

	2. Use ip:

		# ip link set ethX address YY:YY:YY:YY:YY:YY

	   ,where X is the device number assigned by Linux kernel, and
		  YY:YY:YY:YY:YY:YY is the MAC address assigned by the user.

<Force Link Status>

	1. Force the link status when insert the driver.

	   If the user is in the path ~/r8168, the link status can be forced 
	   to one of the 5 modes as following command.

		# insmod ./src/r8168.ko speed=SPEED_MODE duplex=DUPLEX_MODE autoneg=NWAY_OPTION

		,where
			SPEED_MODE	= 1000	for 1000Mbps
					= 100	for 100Mbps
					= 10	for 10Mbps
			DUPLEX_MODE	= 0	for half-duplex
					= 1	for full-duplex
			NWAY_OPTION	= 0	for auto-negotiation off (true force)
					= 1	for auto-negotiation on (nway force)
		For example:

			# insmod ./src/r8168.ko speed=100 duplex=0 autoneg=1

		will force PHY to operate in 100Mpbs Half-duplex(nway force).

	2. Force the link status by using ethtool.
		a. Insert the driver first.
		b. Make sure that ethtool exists in /sbin.
		c. Force the link status as the following command.

			# ethtool -s ethX speed SPEED_MODE duplex DUPLEX_MODE autoneg NWAY_OPTION

			,where
				SPEED_MODE	= 1000	for 1000Mbps
						= 100	for 100Mbps
						= 10	for 10Mbps
				DUPLEX_MODE	= half	for half-duplex
						= full	for full-duplex
				NWAY_OPTION	= off	for auto-negotiation off (true force)
						= on	for auto-negotiation on (nway force)

		For example:
		
			# ethtool -s eth0 speed 100 duplex full autoneg on

		will force PHY to operate in 100Mpbs Full-duplex(nway force).

