-- /*****************************************************************************
-- **                                                                          **
-- **  Copyright 2007 2012 Intel Corporation All Rights Reserved.              **
-- **                                                                          **
-- **  The material contained or described herein and all documents related    **
-- **  to such material ("Material") is owned by Intel Corporation or its      **
-- **  suppliers or licensors, and title to such Material remains with Intel   **
-- **  Corporation or its suppliers or licensors. The Material contains        **
-- **  proprietary information of Intel or its suppliers and licensors. The    **
-- **  Material is protected by worldwide copyright laws and treaty            **
-- **  provisions. No part of the Material may be used, copied, reproduced,    **
-- **  modified, published, uploaded, posted, transmitted, distributed or      **
-- **  disclosed in any way without Intel's prior express written permission.  **
-- **  No license under any patent, copyright or other intellectual property   **
-- **  rights in the Material is granted to or conferred upon you, either      **
-- **  expressly, by implication, inducement, estoppel or otherwise. Any       **
-- **  license under such intellectual property rights must be express and     **
-- **  approved by Intel in writing.                                           **
-- **                                                                          **
-- **  Unless otherwise agreed by Intel in writing, you may not remove or      **
-- **  alter this notice or any other notice embedded in Materials by Intel    **
-- **  or Intel’s suppliers or licensors in any way.                           **
-- *****************************************************************************/

-- FILE: INTELDCB.MIB
-- MIB Version = 1.9.1.0
--
-- For general information and support, go to the Intel support website at:
-- <http://support.intel.com>
--

INTEL-DCB-MIB DEFINITIONS ::= BEGIN

IMPORTS

    enterprises
        FROM RFC1155-SMI
    MODULE-IDENTITY,
    OBJECT-TYPE,
    NOTIFICATION-TYPE,
    Counter64,
    Integer32
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION,
    DisplayString
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP,
    NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    physicalAdapterIndex
        FROM INTEL-LAN-ADAPTERS-MIB
        ;


inteldcblan   MODULE-IDENTITY
  LAST-UPDATED "201110140000Z"   -- Oct 14, 2011
  ORGANIZATION "Intel Corp"
  CONTACT-INFO
         "Intel Corp
          http://www.intel.com/"
  DESCRIPTION
          "The MIB module for Intel DCB SNMP agent."

  REVISION    "201110140000Z"   -- Oct 14, 2011
  DESCRIPTION
          "Version 1.9.0
           Added dcbOsControlledEnable to dcbConfigTable"

  REVISION    "201107280000Z"   -- Jul 28, 2011
  DESCRIPTION
          "Version 1.7.0
           Corrected DISPLAY-HINTS for OCTET STRINGS"

  REVISION    "201105050000Z"   -- May 05, 2011
  DESCRIPTION
          "Version 1.6.2
           Added IEEE fields for DCBX support"

  REVISION    "201010110000Z"   -- Oct 11, 2010
  DESCRIPTION
          "Version 1.3.1
           Added Compliance section for SMI v2 errors from previous version"

  ::= { enterprises 4300 1 }


-- Categories

intel               OBJECT IDENTIFIER ::= { enterprises 343 }
products            OBJECT IDENTIFIER ::= { intel 2 }
nic-products        OBJECT IDENTIFIER ::= { products 7 }
intel-lan-adapters  OBJECT IDENTIFIER ::= { nic-products 2 }
intel-dcb           OBJECT IDENTIFIER ::= { nic-products 3 }


InterfaceIndex ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS       current
    DESCRIPTION
            "A unique value, greater than zero, for each interface or
            interface sub-layer in the managed system.  It is
            recommended that values are assigned contiguously starting
            from 1.  The value for each interface sub-layer must remain
            constant at least from one re-initialization of the entity's
            network management system to the next re-initialization."
    SYNTAX       Integer32 (1..2147483647)

Ables ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
            "A value defining disable or enable"
    SYNTAX       INTEGER {disable(0), enable(1)}

DcbPgFormat	::= TEXTUAL-CONVENTION
    DISPLAY-HINT "x"
    STATUS       current
    DESCRIPTION
         "A structure of 40 octets representing the Priority Group (PG) settings.
          - The first 8 octets represent the % (0..100) of link bandwidth assigned
            to the 8 Bandwidth Groups (BWG) (0..7).  The index into the 8 octets is the
            BWG ID.
          - The other 32 octets represent an array of eight 4-octet elements.  The
            index into the array is the User Priority (UP) (0..7).
            The four octets in each array element represent the following:
            Octet 1 is the Traffic Class (0..7) mapping of the UP.
            Octet 2 is the BWG ID (0..7) of the UP.
            Octet 3 is the % (0..100) of the BWG bandwidth assigned to the UP.
            Octet 4 is the strict priority setting of the UP. Which can be:
              0 - normal
              1 - group strict (SubType 1 only)
              2 - link strict
          - NOTE: Octet 3 is only supported by DCBX protocol SubType 1. In SubType
             2 all UPs assigned to a given BWG ID will be assigned an equal %."
    SYNTAX       OCTET STRING ( SIZE (40) )

DcbPfcFormat	::= TEXTUAL-CONVENTION
    DISPLAY-HINT "x"
    STATUS       current
    DESCRIPTION
        "An array of 8 octets representing the Priority Flow
         Control (PFC) settings for the 8 User Priorities.
         Each octet can take on the values:
                    disabled (0x0),
                    enabled (0x1)
         The index into the 8 octets is User Priority."
    SYNTAX       OCTET STRING ( SIZE (8) )
    
DcbMapFormat	::= TEXTUAL-CONVENTION
    DISPLAY-HINT "x"
    STATUS       current
    DESCRIPTION
        "An array of 8 octets representing the Traffic Class 
         mapping for the 8 User Priorities.
         Each octet can take on the values:
                    (0x00) through enabled (0x08)
         The index into the 8 octets is User Priority."
    SYNTAX       OCTET STRING ( SIZE (8) )

DcbUpAbleFormat	::= TEXTUAL-CONVENTION
    DISPLAY-HINT "x"
    STATUS       current
    DESCRIPTION
        "An array of 8 octets representing feature enablement
         for the 8 User Priorities.
         Each octet can take on the values:
                    disabled (0x0),
                    enabled  (0x1)
         The index into the 8 octets is User Priority."
    SYNTAX       OCTET STRING ( SIZE (8) )

-- ****************************************
-- Data Center Bridging Attr Tables
-- ****************************************
dcbTables OBJECT IDENTIFIER ::= { intel-dcb 1 }

dcbConfigTables OBJECT IDENTIFIER ::= { dcbTables 1 }

-- *********************************************************************
-- Data Center Bridging Attr Tables - DcbConfig
-- DCB Configuration
-- *********************************************************************
dcbConfigTable OBJECT-TYPE
    SYNTAX		SEQUENCE OF DcbConfigEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "General configuration parameters for DCB for all ports."
    ::= { dcbConfigTables 1 }

dcbConfigEntry OBJECT-TYPE
    SYNTAX		DcbConfigEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "DCB attributes common to all physical adapters.
        There is one 'entry' for each adapter."
    INDEX		{ physicalAdapterIndex }
    ::= { dcbConfigTable 1 }

DcbConfigEntry ::= SEQUENCE {
    dcbConfigEnable                   Ables,
    dcbVersion                        Integer32,
    dcbOsControlledEnable             Ables
}

dcbConfigEnable OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Enables or Disables the DCB on the associated physical adapter."
    ::= { dcbConfigEntry 1 }

dcbVersion  OBJECT-TYPE
    SYNTAX		Integer32 (1 .. 3)
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "Specifies the DCBX TLV version to be transmitted and processed by DCBX
         0 - Enables version detection and support for CEE and IEEE DCBX
         1 - Enables Pre-CEE DCBX TLVs
		 2 - Enables CEE DCBX TLVs
		 3 - Enables IEEE DCBX TLVs
		"
    ::= { dcbConfigEntry 2 }

dcbOsControlledEnable OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "Enables or Disables the ability for the OS to Control DCB configuration."
    ::= { dcbConfigEntry 3 }

-- *********************************************************************
-- Data Center Bridging Attr Tables - PgConfig
-- Priority Groups Configuration
-- *********************************************************************
dcbPgConfigTable OBJECT-TYPE
    SYNTAX		SEQUENCE OF DcbPgConfigEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "Configuration parameters for the Priority Groups DCB feature
         for all ports."
    ::= { dcbConfigTables 2 }

dcbPgConfigEntry OBJECT-TYPE
    SYNTAX		DcbPgConfigEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "Priority Groups attributes common to all physical adapters.
        There is one 'entry' for each adapter."
    INDEX		{physicalAdapterIndex}
    ::= { dcbPgConfigTable 1 }

DcbPgConfigEntry ::= SEQUENCE {
    dcbPgConfigEnable                   Ables,
    dcbPgConfigWilling                  Ables,
    dcbPgConfigAdvertise                Ables,
    dcbPgConfigBandwidths               DcbPgFormat,
    dcbPgConfigNumTCs                   Integer32,
    dcbPgConfigRecBandwidths            DcbPgFormat,
    dcbPgConfigRecEnable                Ables
}

dcbPgConfigEnable OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "Enables or Disables the Priority Group feature."
    ::= { dcbPgConfigEntry 1 }

dcbPgConfigWilling OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "Enables or Disables the Willing parameter for the Priority
         Group feature.  Enabled indicates that the local port will
         accept Priority Group parameters from a not Willing (disabled)
         peer port."
    ::= { dcbPgConfigEntry 2 }

dcbPgConfigAdvertise OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "Enables or Disables Priority Group parameter exchange via DCB
         Capabilities Exchange protocol."
    ::= { dcbPgConfigEntry 3 }

dcbPgConfigBandwidths OBJECT-TYPE
    SYNTAX		DcbPgFormat
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
         "A structure of 40 octets representing the Priority Group (PG) settings.
          - The first 8 octets represent the % (0..100) of link bandwidth assigned
            to the 8 Bandwidth Groups (BWG) (0..7).  The index into the 8 octets is the
            BWG ID.
          - The other 32 octets represent an array of eight 4-octet elements.  The
            index into the array is the User Priority (UP) (0..7).
            The four octets in each array element represent the following:
            Octet 1 is the Traffic Class (0..7) mapping of the UP.
            Octet 2 is the BWG ID (0..7) of the UP. Use BWG ID 15 to assign UP to link strict group.
            Octet 3 is the % (0..100) of the BWG bandwidth assigned to the UP.
            Octet 4 is the strict priority setting of the UP. Which can be:
              0 - normal
              1 - group strict (SubType 1 only)
              2 - link strict
          - NOTE: Octet 3 is only supported by DCBX protocol SubType 1. In SubType
             2 all UPs assigned to a given BWG ID will be assigned an equal %."
    ::= { dcbPgConfigEntry 4 }

dcbPgConfigNumTCs  OBJECT-TYPE
    SYNTAX		Integer32 (0 .. 32)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Number of TCs capable of supporting PG."
    ::= { dcbPgConfigEntry 5 }
    
dcbPgConfigRecBandwidths OBJECT-TYPE
    SYNTAX		DcbPgFormat
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "A structure of 40 octets representing the remote Recommended Priority Group (PG) settings.
         (Supported only in IEEE operation)
          - The first 8 octets represent the % (0..100) of link bandwidth assigned
            to the 8 Bandwidth Groups (BWG) (0..7).  The index into the 8 octets is the
            BWG ID.
          - The other 32 octets represent an array of eight 4-octet elements.  The
            index into the array is the User Priority (UP) (0..7).
            The four octets in each array element represent the following:
            Octet 1 is the Traffic Class (0..7) mapping of the UP.
            Octet 2 is the BWG ID (0..7) of the UP. Use BWG ID 15 to assign UP to link strict group.
            Octet 3 is unused.
            Octet 4 is the strict priority setting of the UP. Which can be:
              0 - normal
              2 - link strict
		"
    ::= { dcbPgConfigEntry 6 }

dcbPgConfigRecEnable OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "Enables or Disables the remote Priority Group Recommended TLV.
         (Supported only in IEEE operation)
		"
    ::= { dcbPgConfigEntry 7 }

-- *********************************************************************
-- Data Center Bridging Attr Tables - PgBwgConfig
-- Priority Groups Bandwidth Group Configuration
-- *********************************************************************
dcbPgBwgNameTable OBJECT-TYPE
    SYNTAX		SEQUENCE OF DcbPgBwgNameEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "The user supplied name associated with each bandwidth group."
    ::= { dcbConfigTables 3 }

dcbPgBwgNameEntry OBJECT-TYPE
    SYNTAX		DcbPgBwgNameEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "Bandwidth group names per port.
        There is one 'entry' for each interface."
    INDEX		{physicalAdapterIndex, dcbPgBwgId}
    ::= { dcbPgBwgNameTable 1 }

DcbPgBwgNameEntry ::= SEQUENCE {
    dcbPgBwgId                          Integer32,
    dcbPgBwgName                        DisplayString
}

dcbPgBwgId  OBJECT-TYPE
    SYNTAX		Integer32 (0 .. 7)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The Bandwidth Group ID number."
    ::= { dcbPgBwgNameEntry 1 }

dcbPgBwgName	 OBJECT-TYPE
    SYNTAX		DisplayString
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "The user supplied name for the Bandwidth Group."
    ::= { dcbPgBwgNameEntry 2 }

-- ************************************************************************
-- Data Center Bridging Attr Tables - PfcConfig
-- Priority Flow Control Configuration
-- ************************************************************************
dcbPfcConfigTable OBJECT-TYPE
    SYNTAX		SEQUENCE OF DcbPfcConfigEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "Priority Flow Control (PFC) attributes of DCB capable physical
         adapters."
    ::= { dcbConfigTables 4 }

dcbPfcConfigEntry OBJECT-TYPE
    SYNTAX		DcbPfcConfigEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "Priority Flow Control (PFC) settings for all User Priorities per
         port.  There is one 'entry' for each adapter."
    INDEX		{physicalAdapterIndex}
    ::= { dcbPfcConfigTable 1 }

DcbPfcConfigEntry ::= SEQUENCE {
    dcbPfcConfigEnable             Ables,
    dcbPfcConfigWilling            Ables,
    dcbPfcConfigAdvertise          Ables,
    dcbPfcConfigSettings           DcbPfcFormat,
    dcbPfcConfigNumTCs             Integer32
}

dcbPfcConfigEnable OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "Enables or Disables the Priority Flow Control feature."
    ::= { dcbPfcConfigEntry 1 }

dcbPfcConfigWilling OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "Enables or Disables the Willing parameter for the Priority
         Flow Control feature.  Enabled indicates that the local port will
         accept Priority Flow Control parameters from a not Willing (disabled)
         peer port."
    ::= { dcbPfcConfigEntry 2 }

dcbPfcConfigAdvertise OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "Enables or Disables the advertising Priority Flow Control
         parameters for this port to the peer via the protocol."
    ::= { dcbPfcConfigEntry 3 }

dcbPfcConfigSettings OBJECT-TYPE
    SYNTAX		DcbPfcFormat
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "The administrative Priority Flow Control (PFC) settings.
         An array of 8 octets representing the PFC settings for the 8
         User Priorities.  Each octet can take on the values:
                    disabled (0x0),
                    enabled (0x1)
         The index into the 8 octets is User Priority.
         "
    ::= { dcbPfcConfigEntry 4 }

dcbPfcConfigNumTCs  OBJECT-TYPE
    SYNTAX		Integer32 (0 .. 32)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Number of TCs capable of supporting PFC."
    ::= { dcbPfcConfigEntry 5 }

-- ************************************************************************
-- Data Center Bridging Attr Tables - FcoeConfig
-- FCoE Application Configuration
-- ************************************************************************
dcbFcoeConfigTable OBJECT-TYPE
    SYNTAX		SEQUENCE OF DcbFcoeConfigEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "FCoE Application attributes of DCB capable physical adapters."
    ::= { dcbConfigTables 5 }

dcbFcoeConfigEntry OBJECT-TYPE
    SYNTAX		DcbFcoeConfigEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "There is one 'entry' for each adapter."
    INDEX		{physicalAdapterIndex, dcbFcoeSubType}
    ::= { dcbFcoeConfigTable 1 }

DcbFcoeConfigEntry ::= SEQUENCE {
    dcbFcoeConfigEnable             Ables,
    dcbFcoeConfigWilling            Ables,
    dcbFcoeConfigAdvertise          Ables,
    dcbFcoeConfigData               OCTET STRING,
    dcbFcoeConfigSelector           Integer32,
    dcbFcoeConfigIdentifier         OCTET STRING
}

dcbFcoeConfigEnable OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "Enables or Disables the FCoE Application feature."
    ::= { dcbFcoeConfigEntry 1 }

dcbFcoeConfigWilling OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "Enables or Disables the Willing parameter for the FCoE
         Application feature.  Enabled indicates that the local
         port will accept FCoE Application parameters from a not
         Willing (disabled) peer port."
    ::= { dcbFcoeConfigEntry 2 }

dcbFcoeConfigAdvertise OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "Enables or Disables the advertising FCoE Application
         parameters for this port to the peer via the protocol."
    ::= { dcbFcoeConfigEntry 3 }

dcbFcoeConfigData OBJECT-TYPE
    SYNTAX		OCTET STRING ( SIZE (1) )
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "FCoE Application specific configuration."
    ::= { dcbFcoeConfigEntry 4 }

dcbFcoeConfigSelector OBJECT-TYPE
    SYNTAX		Integer32 (0 .. 4)
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "The local selector to specify the method of identifying  FCoE traffic.
         (Supported only in IEEE operation)
             0x01 - Ethertype
             0x02 - Well Known Port number over TCP, SCTP
             0x03 - Well Known Port number over UDP, DCCP
             0x04 - Well Known Port number over TCP, SCTP, UDP, DCCP
         "
    ::= { dcbFcoeConfigEntry 5 }
    
dcbFcoeConfigIdentifier OBJECT-TYPE
    SYNTAX		OCTET STRING ( SIZE (2) )
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "The local traffic identifier for the FCoE Application feature.
         (Supported only in IEEE operation)
         "
    ::= { dcbFcoeConfigEntry 6 }

-- ************************************************************************
-- Data Center Bridging Attr Tables - iScsiFcoeConfig
-- iSCSI Application Configuration
-- ************************************************************************

dcbiScsiConfigTable OBJECT-TYPE
    SYNTAX		SEQUENCE OF DcbiScsiConfigEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "iSCSI Application attributes of DCB capable physical adapters."
    ::= { dcbConfigTables 7 }

dcbiScsiConfigEntry OBJECT-TYPE
    SYNTAX		DcbiScsiConfigEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "There is one 'entry' for each adapter."
    INDEX		{physicalAdapterIndex, dcbiScsiSubType}
    ::= { dcbiScsiConfigTable 1 }

DcbiScsiConfigEntry ::= SEQUENCE {
    dcbiScsiConfigEnable             Ables,
    dcbiScsiConfigWilling            Ables,
    dcbiScsiConfigAdvertise          Ables,
    dcbiScsiConfigData               OCTET STRING,
    dcbiScsiConfigSelector           Integer32,
    dcbiScsiConfigIdentifier         OCTET STRING
}

dcbiScsiConfigEnable OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "Enables or Disables the iSCSI Application feature."
    ::= { dcbiScsiConfigEntry 1 }

dcbiScsiConfigWilling OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "Enables or Disables the Willing parameter for the iSCSI
         Application feature.  Enabled indicates that the local
         port will accept iSCSI Application parameters from a not
         Willing (disabled) peer port."
    ::= { dcbiScsiConfigEntry 2 }

dcbiScsiConfigAdvertise OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "Enables or Disables the advertising iSCSI Application
         parameters for this port to the peer via the protocol."
    ::= { dcbiScsiConfigEntry 3 }

dcbiScsiConfigData OBJECT-TYPE
    SYNTAX		OCTET STRING  ( SIZE (1) )
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "iSCSI Application specific configuration.
         "
    ::= { dcbiScsiConfigEntry 4 }

dcbiScsiConfigSelector OBJECT-TYPE
    SYNTAX		Integer32 (0 .. 4)
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "The local selector to specify the method of identifying  iSCSI traffic.
         (Supported only in IEEE operation)
             0x01 - Ethertype
             0x02 - Well Known Port number over TCP, SCTP
             0x03 - Well Known Port number over UDP, DCCP
             0x04 - Well Known Port number over TCP, SCTP, UDP, DCCP
         "
    ::= { dcbiScsiConfigEntry 5 }
    
dcbiScsiConfigIdentifier OBJECT-TYPE
    SYNTAX		OCTET STRING ( SIZE (2) )
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "The local traffic identifier for the iSCSI Application feature.
         (Supported only in IEEE operation)
         "
    ::= { dcbiScsiConfigEntry 6 }

-- *********************************************************************
-- Data Center Bridging Attr Tables - Operational Status
-- *********************************************************************
dcbOperTables OBJECT IDENTIFIER ::= { dcbTables 2 }

-- ************************************************************************
-- Data Center Bridging Operational Attr Tables - PgOper
-- Priority Groups Operational Status
-- ************************************************************************
dcbPgOperTable OBJECT-TYPE
    SYNTAX		SEQUENCE OF DcbPgOperEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "Configuration parameters for the Priority Groups DCB feature
         for all ports."
    ::= { dcbOperTables 1 }

dcbPgOperEntry OBJECT-TYPE
    SYNTAX		DcbPgOperEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "Priority Groups attributes common to all physical adapters.
        There is one 'entry' for each adapter."
    INDEX		{physicalAdapterIndex}
    ::= { dcbPgOperTable 1 }

DcbPgOperEntry ::= SEQUENCE {
    dcbPgOperVersion                Integer32,
    dcbPgOperMaxVersion             Integer32,
    dcbPgOperError                  Integer32,
    dcbPgOperMode                   Ables,
    dcbPgOperSyncd                  Integer32,
    dcbPgOperBandwidths             DcbPgFormat,
    dcbPgOperMappingUPtoTC          DcbMapFormat
}

dcbPgOperVersion OBJECT-TYPE
    SYNTAX		Integer32 (0..255)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The operational protocol version of the Priority Groups feature."
    ::= { dcbPgOperEntry 1 }

dcbPgOperMaxVersion OBJECT-TYPE
    SYNTAX		Integer32 (0..255)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The highest protocol version supported by the
         implementation of the Priority Groups feature."
    ::= { dcbPgOperEntry 2 }

dcbPgOperError OBJECT-TYPE
    SYNTAX		Integer32
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Current error status of the Priority Groups feature.  Bits in the
         Error value are defined as:
             0x00 - no error
             0x01 - feature mismatch with peer
             0x02 - error setting feature configuration
             0x04 - multiple feature TLVs received from peer
             0x08 - peer error
             0x10 - multiple LLDP neighbors present
             0x20 - feature not present in peer tlv
         "
    ::= { dcbPgOperEntry 3 }

dcbPgOperMode OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Operational status of the Priority Group feature.
         "
    ::= { dcbPgOperEntry 4 }

dcbPgOperSyncd OBJECT-TYPE
    SYNTAX		Integer32 (0..1)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Indicates the current synced state of the feature relative to
         the peer device.
         "
    ::= { dcbPgOperEntry 5 }

dcbPgOperBandwidths OBJECT-TYPE
    SYNTAX		DcbPgFormat
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
         "A structure of 40 octets representing the Priority Group (PG) settings.
          - The first 8 octets represent the % (0..100) of link bandwidth assigned
            to the 8 Bandwidth Groups (BWG) (0..7).  The index into the 8 octets is the
            BWG ID.
          - The other 32 octets represent an array of eight 4-octet elements.  The
            index into the array is the User Priority (UP) (0..7).
            The four octets in each array element represent the following:
            Octet 1 is the Traffic Class (0..7) mapping of the UP.
            Octet 2 is the BWG ID (0..7) of the UP.
            Octet 3 is the % (0..100) of the BWG bandwidth assigned to the UP.
            Octet 4 is the strict priority setting of the UP. Which can be:
              0 - normal
              1 - group strict (SubType 1 only)
              2 - link strict
          - NOTE: Octet 3 is only supported by DCBX protocol SubType 1. In SubType
             2 all UPs assigned to a given BWG ID will be assigned an equal %."
    ::= { dcbPgOperEntry 6 }
    
dcbPgOperMappingUPtoTC OBJECT-TYPE
    SYNTAX		DcbMapFormat
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
         "This field contains the operational mapping of UP to TC."
    ::= { dcbPgOperEntry 7 }

-- ************************************************************************
-- Data Center Bridging Attr Tables - PfcOper
-- Priority Flow Control Operational Status
-- ************************************************************************
dcbPfcOperTable OBJECT-TYPE
    SYNTAX		SEQUENCE OF DcbPfcOperEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "Priority Flow Control (PFC) attributes of DCB capable physical
         adapters."
    ::= { dcbOperTables 2 }

dcbPfcOperEntry OBJECT-TYPE
    SYNTAX		DcbPfcOperEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "Priority Flow Control (PFC) settings for all User Priorities per
         port.  There is one 'entry' for each adapter."
    INDEX		{physicalAdapterIndex}
    ::= { dcbPfcOperTable 1 }

DcbPfcOperEntry ::= SEQUENCE {
    dcbPfcOperVersion            Integer32,
    dcbPfcOperMaxVersion         Integer32,
    dcbPfcOperError              Integer32,
    dcbPfcOperMode               Ables,
    dcbPfcOperSyncd              Integer32,
    dcbPfcOperSettings           DcbPfcFormat
}

dcbPfcOperVersion OBJECT-TYPE
    SYNTAX		Integer32 (0..255)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The operational protocol version of the Priority Flow Control
         feature."
    ::= { dcbPfcOperEntry 1 }

dcbPfcOperMaxVersion OBJECT-TYPE
    SYNTAX		Integer32 (0..255)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The highest protocol version supported by the
         implementation of the Priority Flow Control feature."
    ::= { dcbPfcOperEntry 2 }

dcbPfcOperError OBJECT-TYPE
    SYNTAX		Integer32
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Current error status of the Priority Flow Control feature.  Bits in the
         Error value are defined as:
             0x00 - no error
             0x01 - feature mismatch with peer
             0x02 - error setting feature configuration
             0x04 - multiple feature TLVs received from peer
             0x08 - peer error
             0x10 - multiple LLDP neighbors present
             0x20 - feature not present in peer tlv"
    ::= { dcbPfcOperEntry 3 }

dcbPfcOperMode OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Operational status of the Priority Flow Control feature."
    ::= { dcbPfcOperEntry 4 }

dcbPfcOperSyncd OBJECT-TYPE
    SYNTAX		Integer32 (0..1)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Indicates the current synced state of the feature relative to
         the peer device."
    ::= { dcbPfcOperEntry 5 }

dcbPfcOperSettings OBJECT-TYPE
    SYNTAX		DcbPfcFormat
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The administrative Priority Flow Control (PFC) settings.
         An array of 8 octets representing the PFC settings for the 8
         User Priorities.  Each octet can take on the values:
                    disabled (0x0),
                    enabled (0x1)
         The index into the 8 octets is User Priority.
         "
    ::= { dcbPfcOperEntry 6 }

-- ************************************************************************
-- Data Center Bridging Attr Tables - FcoeOper
-- Application Operational Status
-- ************************************************************************
dcbFcoeOperTable OBJECT-TYPE
    SYNTAX		SEQUENCE OF DcbFcoeOperEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "FCoE Application attributes of DCB capable physical
         adapters."
    ::= { dcbOperTables 3 }

dcbFcoeOperEntry OBJECT-TYPE
    SYNTAX		DcbFcoeOperEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "FCoE Application settings for all User Priorities per
         port.  There is one 'entry' for each adapter."
    INDEX		{physicalAdapterIndex, dcbFcoeSubType}
    ::= { dcbFcoeOperTable 1 }

DcbFcoeOperEntry ::= SEQUENCE {
    dcbFcoeOperVersion            Integer32,
    dcbFcoeOperMaxVersion         Integer32,
    dcbFcoeOperError              Integer32,
    dcbFcoeOperMode               Ables,
    dcbFcoeOperSyncd              Integer32,
    dcbFcoeOperData               OCTET STRING,
    dcbFcoeSubType                Integer32,
    dcbFcoeOperSelector           Integer32,
    dcbFcoeOperIdentifier         OCTET STRING
}

dcbFcoeOperVersion OBJECT-TYPE
    SYNTAX		Integer32 (0..255)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The operational protocol version of the FCoE
         Application:subtype feature."
    ::= { dcbFcoeOperEntry 1 }

dcbFcoeOperMaxVersion OBJECT-TYPE
    SYNTAX		Integer32 (0..255)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The highest protocol version supported by the
         implementation of the FCoE Application:subtype
         feature."
    ::= { dcbFcoeOperEntry 2 }

dcbFcoeOperError OBJECT-TYPE
    SYNTAX		Integer32
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Current error status of the FCoE Application:subtype
         feature.  Bits in the Error value are defined as:
             0x00 - no error
             0x01 - feature mismatch with peer
             0x02 - error setting feature configuration
             0x04 - multiple feature TLVs received from peer
             0x08 - peer error
             0x10 - multiple LLDP neighbors present
             0x20 - feature not present in peer tlv"
    ::= { dcbFcoeOperEntry 3 }

dcbFcoeOperMode OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Operational status of the FCoE Application:subtype
         feature."
    ::= { dcbFcoeOperEntry 4 }

dcbFcoeOperSyncd OBJECT-TYPE
    SYNTAX		Integer32 (0..1)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Indicates the current synced state of the FCoE
         Application feature relative to the peer device."
    ::= { dcbFcoeOperEntry 5 }

dcbFcoeOperData OBJECT-TYPE
    SYNTAX		OCTET STRING ( SIZE (1) )
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The operational FCoE Application specific configuration."
    ::= { dcbFcoeOperEntry 6 }

dcbFcoeSubType OBJECT-TYPE
    SYNTAX		Integer32 (0..1)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Indicates the SubType of the FCoE Application feature."
    ::= { dcbFcoeOperEntry 7 }

dcbFcoeOperSelector OBJECT-TYPE
    SYNTAX		Integer32 (0 .. 4)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The operational selector to specify the method of identifying  FCoE traffic.
         (Supported only in IEEE operation)
             0x01 - Ethertype
             0x02 - Well Known Port number over TCP, SCTP
             0x03 - Well Known Port number over UDP, DCCP
             0x04 - Well Known Port number over TCP, SCTP, UDP, DCCP
         "
    ::= { dcbFcoeOperEntry 8 }
    
dcbFcoeOperIdentifier OBJECT-TYPE
    SYNTAX		OCTET STRING ( SIZE (2) )
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The operational traffic identifier for the FCoE Application feature.
         (Supported only in IEEE operation)
         "
    ::= { dcbFcoeOperEntry 9 }

-- ************************************************************************
-- Data Center Bridging Attr Tables - iScsiFcoeOper
-- iSCSI Application Operational Status
-- ************************************************************************
dcbiScsiOperTable OBJECT-TYPE
    SYNTAX		SEQUENCE OF DcbiScsiOperEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "iSCSI Application attributes of DCB capable physical
         adapters."
    ::= { dcbOperTables 5 }

dcbiScsiOperEntry OBJECT-TYPE
    SYNTAX		DcbiScsiOperEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "iSCSI Application settings for all User Priorities per
         port.  There is one 'entry' for each adapter."
    INDEX		{physicalAdapterIndex, dcbiScsiSubType}
    ::= { dcbiScsiOperTable 1 }

DcbiScsiOperEntry ::= SEQUENCE {
    dcbiScsiOperVersion            Integer32,
    dcbiScsiOperMaxVersion         Integer32,
    dcbiScsiOperError              Integer32,
    dcbiScsiOperMode               Ables,
    dcbiScsiOperSyncd              Integer32,
    dcbiScsiOperData               OCTET STRING,
    dcbiScsiSubType                Integer32,
    dcbiScsiOperSelector           Integer32,
    dcbiScsiOperIdentifier         OCTET STRING
}

dcbiScsiOperVersion OBJECT-TYPE
    SYNTAX		Integer32 (0..255)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The operational protocol version of the iSCSI
         Application:subtype feature."
    ::= { dcbiScsiOperEntry 1 }

dcbiScsiOperMaxVersion OBJECT-TYPE
    SYNTAX		Integer32 (0..255)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The highest protocol version supported by the
         implementation of the iSCSI Application:subtype
         feature."
    ::= { dcbiScsiOperEntry 2 }

dcbiScsiOperError OBJECT-TYPE
    SYNTAX		Integer32
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Current error status of the iSCSI Application:subtype
         feature.  Bits in the Error value are defined as:
             0x00 - no error
             0x01 - feature mismatch with peer
             0x02 - error setting feature configuration
             0x04 - multiple feature TLVs received from peer
             0x08 - peer error
             0x10 - multiple LLDP neighbors present
             0x20 - feature not present in peer tlv"
    ::= { dcbiScsiOperEntry 3 }

dcbiScsiOperMode OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Operational status of the iSCSI Application:subtype
         feature."
    ::= { dcbiScsiOperEntry 4 }

dcbiScsiOperSyncd OBJECT-TYPE
    SYNTAX		Integer32 (0..1)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Indicates the current synced state of the iSCSI
         Application feature relative to the peer device.
         "
    ::= { dcbiScsiOperEntry 5 }

dcbiScsiOperData OBJECT-TYPE
    SYNTAX		OCTET STRING ( SIZE (1) )
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The operational iSCSI Application specific configuration."
    ::= { dcbiScsiOperEntry 6 }

dcbiScsiSubType OBJECT-TYPE
    SYNTAX		Integer32 (0..1)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Indicates the SubType of the iSCSI Application feature."
    ::= { dcbiScsiOperEntry 7 }

dcbiScsiOperSelector OBJECT-TYPE
    SYNTAX		Integer32 (0 .. 4)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The operational selector to specify the method of identifying  iSCSI traffic.
         (Supported only in IEEE operation)
             0x01 - Ethertype
             0x02 - Well Known Port number over TCP, SCTP
             0x03 - Well Known Port number over UDP, DCCP
             0x04 - Well Known Port number over TCP, SCTP, UDP, DCCP
         "
    ::= { dcbiScsiOperEntry 8 }
    
dcbiScsiOperIdentifier OBJECT-TYPE
    SYNTAX		OCTET STRING ( SIZE (2) )
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The operational traffic identifier for the iSCSI Application feature.
         (Supported only in IEEE operation)
         "
    ::= { dcbiScsiOperEntry 9 }


-- ************************************************************************
-- Data Center Bridging Attr Tables - DcbOper
-- DCB Operational Status
-- ************************************************************************
dcbOperTable OBJECT-TYPE
    SYNTAX		SEQUENCE OF DcbOperEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "General configuration parameters for DCB for all physical adapters."
    ::= { dcbOperTables 6 }

dcbOperEntry OBJECT-TYPE
    SYNTAX		DcbOperEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "DCB attributes common to all physical adapters.
        There is one 'entry' for each adapter."
    INDEX		{physicalAdapterIndex}
    ::= { dcbOperTable 1 }

DcbOperEntry ::= SEQUENCE {
    dcbOperVersion           Integer32
}

dcbOperVersion OBJECT-TYPE
    SYNTAX		Integer32 (0..3)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The DCBX TLV version currently transmitted by DCBX
         1 - Pre-CEE DCBX TLVs
		 2 - CEE DCBX TLVs
		 3 - IEEE DCBX TLVs
		"
    ::= { dcbOperEntry 1 }


-- *********************************************************************
-- Data Center Bridging Attr Tables - Peer Status
-- *********************************************************************
dcbPeerTables OBJECT IDENTIFIER ::= { dcbTables 3 }

-- ************************************************************************
-- Data Center Bridging Peer Attr Tables - PgPeer
-- Priority Groups Peer Status
-- ************************************************************************

dcbPgPeerTable OBJECT-TYPE
    SYNTAX		SEQUENCE OF DcbPgPeerEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "Configuration parameters for the Priority Groups DCB feature
         for all ports."
    ::= { dcbPeerTables 1 }

dcbPgPeerEntry OBJECT-TYPE
    SYNTAX		DcbPgPeerEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "Priority Groups attributes common to all physical adapters.
        There is one entry for each adapter."
    INDEX		{physicalAdapterIndex}
    ::= { dcbPgPeerTable 1 }

DcbPgPeerEntry ::= SEQUENCE {
    dcbPgPeerEnable                 Ables,
    dcbPgPeerWilling                Ables,
    dcbPgPeerVersion                Integer32,
    dcbPgPeerMaxVersion             Integer32,
    dcbPgPeerError                  Integer32,
    dcbPgPeerBandwidths             DcbPgFormat,
    dcbPgPeerNumTCs                 Integer32
}

dcbPgPeerEnable OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Enable state of the peer's Priority Group feature."
    ::= { dcbPgPeerEntry 1 }

dcbPgPeerWilling OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Willing state of the peer's Priority Group feature."
    ::= { dcbPgPeerEntry 2 }

dcbPgPeerVersion OBJECT-TYPE
    SYNTAX		Integer32 (0..255)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The peer's operational protocol version of the Priority Groups feature."
    ::= { dcbPgPeerEntry 3 }

dcbPgPeerMaxVersion OBJECT-TYPE
    SYNTAX		Integer32 (0..255)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The peer's highest protocol version supported by the
         implementation of the Priority Groups feature."
    ::= { dcbPgPeerEntry 4 }

dcbPgPeerError OBJECT-TYPE
    SYNTAX		Integer32
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The peer's error flag for the Priority Groups feature.
         "
    ::= { dcbPgPeerEntry 5 }

dcbPgPeerBandwidths OBJECT-TYPE
    SYNTAX		DcbPgFormat
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
         "A structure of 40 octets representing the Priority Group (PG) settings.
          - The first 8 octets represent the % (0..100) of link bandwidth assigned
            to the 8 Bandwidth Groups (BWG) (0..7).  The index into the 8 octets is the
            BWG ID.
          - The other 32 octets represent an array of eight 4-octet elements.  The
            index into the array is the User Priority (UP) (0..7).
            The four octets in each array element represent the following:
            Octet 1 is undefined.
            Octet 2 is the BWG ID (0..7) of the UP.
            Octet 3 is the % (0..100) of the BWG bandwidth assigned to the UP.
            Octet 4 is the strict priority setting of the UP. Which can be:
              0 - normal
              1 - group strict (SubType 1 only)
              2 - link strict
          - NOTE: Octet 3 is only supported by DCBX protocol SubType 1. In SubType
             2 all UPs assigned to a given BWG ID will be assigned an equal %."
    ::= { dcbPgPeerEntry 6 }

dcbPgPeerNumTCs  OBJECT-TYPE
    SYNTAX		Integer32 (0 .. 32)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Number of TCs capable of supporting PG."
    ::= { dcbPgPeerEntry 7 }

-- ************************************************************************
-- Data Center Bridging Attr Tables - PfcPeer
-- Priority Flow Control Configuration
-- ************************************************************************
dcbPfcPeerTable OBJECT-TYPE
    SYNTAX		SEQUENCE OF DcbPfcPeerEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "Priority Flow Control (PFC) attributes of DCB capable physical
         adapters."
    ::= { dcbPeerTables 2 }

dcbPfcPeerEntry OBJECT-TYPE
    SYNTAX		DcbPfcPeerEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "Priority Flow Control (PFC) settings for all User Priorities per
         port.  There is one 'entry' for each adapter."
    INDEX		{physicalAdapterIndex}
    ::= { dcbPfcPeerTable 1 }

DcbPfcPeerEntry ::= SEQUENCE {
    dcbPfcPeerEnable                 Ables,
    dcbPfcPeerWilling                Ables,
    dcbPfcPeerVersion                Integer32,
    dcbPfcPeerMaxVersion             Integer32,
    dcbPfcPeerError                  Integer32,
    dcbPfcPeerSettings               DcbPfcFormat,
    dcbPfcPeerNumTCs                 Integer32
}

dcbPfcPeerEnable OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Enable state of the peer's Priority Flow Control feature."
    ::= { dcbPfcPeerEntry 1 }

dcbPfcPeerWilling OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Willing state of the peer's Priority Flow Control feature."
    ::= { dcbPfcPeerEntry 2 }

dcbPfcPeerVersion OBJECT-TYPE
    SYNTAX		Integer32 (0..255)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The peer's operational protocol version of the Priority Flow Control feature."
    ::= { dcbPfcPeerEntry 3 }

dcbPfcPeerMaxVersion OBJECT-TYPE
    SYNTAX		Integer32 (0..255)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The peer's highest protocol version supported by the
         implementation of the Priority Flow Control feature."
    ::= { dcbPfcPeerEntry 4 }

dcbPfcPeerError OBJECT-TYPE
    SYNTAX		Integer32
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The peer's error flag for the Priority Flow Control feature.
         "
    ::= { dcbPfcPeerEntry 5 }

dcbPfcPeerSettings OBJECT-TYPE
    SYNTAX		DcbPfcFormat
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The peer's Priority Flow Control (PFC) settings.
         An array of 8 octets representing the PFC settings for the 8
         User Priorities.  Each octet can take on the values:
                    disabled (0x0),
                    enabled (0x1)
         The index into the 8 octets is User Priority.
         "
    ::= { dcbPfcPeerEntry 6 }

dcbPfcPeerNumTCs  OBJECT-TYPE
    SYNTAX		Integer32 (0 .. 32)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Number of TCs capable of supporting PFC."
    ::= { dcbPfcPeerEntry 7 }

-- ************************************************************************
-- Data Center Bridging Attr Tables - FcoePeer
-- Application Configuration
-- ************************************************************************
dcbFcoePeerTable OBJECT-TYPE
    SYNTAX		SEQUENCE OF DcbFcoePeerEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "Application attributes of DCB capable physical
         adapters."
    ::= { dcbPeerTables 3 }

dcbFcoePeerEntry OBJECT-TYPE
    SYNTAX		DcbFcoePeerEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "FCoE Application settings for all User Priorities per
         port.  There is one 'entry' for each adapter."
    INDEX		{physicalAdapterIndex, dcbFcoeSubType}
    ::= { dcbFcoePeerTable 1 }

DcbFcoePeerEntry ::= SEQUENCE {
    dcbFcoePeerEnable                 Ables,
    dcbFcoePeerWilling                Ables,
    dcbFcoePeerVersion                Integer32,
    dcbFcoePeerMaxVersion             Integer32,
    dcbFcoePeerError                  Integer32,
    dcbFcoePeerData                   OCTET STRING,
    dcbFcoePeerSelector				  Integer32,
    dcbFcoePeerIdentifier			  OCTET STRING
}

dcbFcoePeerEnable OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Enable state of the peer's FCoE Application feature."
    ::= { dcbFcoePeerEntry 1 }

dcbFcoePeerWilling OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Willing state of the peer's FCoE Application feature.
		 (Not valid in IEEE operation)"
    ::= { dcbFcoePeerEntry 2 }

dcbFcoePeerVersion OBJECT-TYPE
    SYNTAX		Integer32 (0..255)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The peer's operational protocol version of the FCoE
         Application feature."
    ::= { dcbFcoePeerEntry 3 }

dcbFcoePeerMaxVersion OBJECT-TYPE
    SYNTAX		Integer32 (0..255)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The peer's highest protocol version supported by the
         implementation of the FCoE Application feature."
    ::= { dcbFcoePeerEntry 4 }

dcbFcoePeerError OBJECT-TYPE
    SYNTAX		Integer32
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The peer's error flag for the FCoE Application feature."
    ::= { dcbFcoePeerEntry 5 }

dcbFcoePeerData OBJECT-TYPE
    SYNTAX		OCTET STRING ( SIZE (1) )
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The peer's operational FCoE Application specific
         configuration."
    ::= { dcbFcoePeerEntry 6 }

dcbFcoePeerSelector OBJECT-TYPE
    SYNTAX		Integer32 (0 .. 4)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The peer's selector to specify the method of identifying  FCoE traffic.
         (Supported only in IEEE operation)
             0x01 - Ethertype
             0x02 - Well Known Port number over TCP, SCTP
             0x03 - Well Known Port number over UDP, DCCP
             0x04 - Well Known Port number over TCP, SCTP, UDP, DCCP
         "
    ::= { dcbFcoePeerEntry 7 }
    
dcbFcoePeerIdentifier OBJECT-TYPE
    SYNTAX		OCTET STRING ( SIZE (2) )
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The peer's traffic identifier for the FCoE Application feature.
         (Supported only in IEEE operation)
         "
    ::= { dcbFcoePeerEntry 8 }

-- ************************************************************************
-- Data Center Bridging Attr Tables - iScsiFcoePeer
-- iSCSI Application Configuration
-- ************************************************************************
dcbiScsiPeerTable OBJECT-TYPE
    SYNTAX		SEQUENCE OF DcbiScsiPeerEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "iSCSI Application attributes of DCB capable physical
         adapters."
    ::= { dcbPeerTables 5 }

dcbiScsiPeerEntry OBJECT-TYPE
    SYNTAX		DcbiScsiPeerEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "iSCSI Application settings for all User Priorities per
         port.  There is one 'entry' for each adapter."
    INDEX		{physicalAdapterIndex, dcbiScsiSubType}
    ::= { dcbiScsiPeerTable 1 }

DcbiScsiPeerEntry ::= SEQUENCE {
    dcbiScsiPeerEnable                 Ables,
    dcbiScsiPeerWilling                Ables,
    dcbiScsiPeerVersion                Integer32,
    dcbiScsiPeerMaxVersion             Integer32,
    dcbiScsiPeerError                  Integer32,
    dcbiScsiPeerData                   OCTET STRING,
    dcbiScsiPeerSelector               Integer32,
    dcbiScsiPeerIdentifier             OCTET STRING
}

dcbiScsiPeerEnable OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Enable state of the peer's iSCSI Application feature."
    ::= { dcbiScsiPeerEntry 1 }

dcbiScsiPeerWilling OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Willing state of the peer's iSCSI Application feature.
		 (Not valid in IEEE operation)"
    ::= { dcbiScsiPeerEntry 2 }

dcbiScsiPeerVersion OBJECT-TYPE
    SYNTAX		Integer32 (0..255)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The peer's operational protocol version of the iSCSI
         Application feature."
    ::= { dcbiScsiPeerEntry 3 }

dcbiScsiPeerMaxVersion OBJECT-TYPE
    SYNTAX		Integer32 (0..255)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The peer's highest protocol version supported by the
         implementation of the iSCSI Application feature."
    ::= { dcbiScsiPeerEntry 4 }

dcbiScsiPeerError OBJECT-TYPE
    SYNTAX		Integer32
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The peer's error flag for the iSCSI Application feature."
    ::= { dcbiScsiPeerEntry 5 }

dcbiScsiPeerData OBJECT-TYPE
    SYNTAX		OCTET STRING ( SIZE (1) )
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The peer's iSCSI Application specific configuration."
    ::= { dcbiScsiPeerEntry 6 }

dcbiScsiPeerSelector OBJECT-TYPE
    SYNTAX		Integer32 (0 .. 4)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The peer's selector to specify the method of identifying  iSCSI traffic.
         (Supported only in IEEE operation)
             0x01 - Ethertype
             0x02 - Well Known Port number over TCP, SCTP
             0x03 - Well Known Port number over UDP, DCCP
             0x04 - Well Known Port number over TCP, SCTP, UDP, DCCP
         "
    ::= { dcbiScsiPeerEntry 7 }
    
dcbiScsiPeerIdentifier OBJECT-TYPE
    SYNTAX		OCTET STRING ( SIZE (2) )
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "The peer's traffic identifier for the iSCSI Application feature.
         (Supported only in IEEE operation)
         "
    ::= { dcbiScsiPeerEntry 8 }

-- *********************************************************************
-- Data Center Bridging Attr Tables - StatisticsTables
-- *********************************************************************
dcbStatisticsTables OBJECT IDENTIFIER ::= { dcbTables 4 }

-- ************************************************************************
-- Data Center Bridging Attr Tables - PgStats
-- ************************************************************************
dcbPgStatsTable OBJECT-TYPE
    SYNTAX		SEQUENCE OF DcbPgStatsEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "Statistics entry for DCB Priority Grouping feature."
    ::= { dcbStatisticsTables 1 }

dcbPgStatsEntry OBJECT-TYPE
    SYNTAX		DcbPgStatsEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "Priority Group statistics common to all Physical Adapters.
        There is one 'entry' for each adapter."
    INDEX		{physicalAdapterIndex, pgTrafficClassIndex}
    ::= { dcbPgStatsTable 1 }

DcbPgStatsEntry ::= SEQUENCE {
    dcbPgStatsInFrames                          Counter64,
    dcbPgStatsOutFrames                         Counter64,
    dcbPgStatsOutFrmOverflowDiscards     Counter64,
    dcbPgStatsInFrmOverflowDiscards      Counter64,
    dcbPgStatsInOctets                          Counter64,
    dcbPgStatsOutOctets                         Counter64,
    pgTrafficClassIndex                         Integer32
}

dcbPgStatsInFrames OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Number of packets received for this class"
    ::= { dcbPgStatsEntry 1 }

dcbPgStatsOutFrames OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Number of packets transmitted for this class"
    ::= { dcbPgStatsEntry 2 }

dcbPgStatsOutFrmOverflowDiscards OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Number of transmitted frames discarded at this class due
         resource overflow (congestion - Q, buffer overflow)"
    ::= { dcbPgStatsEntry 3 }

dcbPgStatsInFrmOverflowDiscards OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Number of received frames discarded at this class due
         resource overflow (congestion - Q, buffer overflow)"
    ::= { dcbPgStatsEntry 4 }

dcbPgStatsInOctets OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Number of octets received for this class"
    ::= { dcbPgStatsEntry 5 }

dcbPgStatsOutOctets OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Number of octets transmitted for this class"
    ::= { dcbPgStatsEntry 6 }

pgTrafficClassIndex OBJECT-TYPE
    SYNTAX		Integer32 (0..255)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Traffic Class"
    ::= { dcbPgStatsEntry 7 }

-- ************************************************************************
-- Data Center Bridging Attr Tables - PfcStats
-- ************************************************************************
dcbPfcStatsTable OBJECT-TYPE
    SYNTAX		SEQUENCE OF DcbPfcStatsEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "Statistics table for DCB Priority Flow Control feature."
    ::= { dcbStatisticsTables 2 }

dcbPfcStatsEntry OBJECT-TYPE
    SYNTAX		DcbPfcStatsEntry
    MAX-ACCESS	not-accessible
    STATUS		current
    DESCRIPTION
        "Priority Flow Control statistics common to all Physical Adapters.
        There is one 'entry' for each adapter."
    INDEX		{physicalAdapterIndex, pfcUserPriorityIndex}
    ::= { dcbPfcStatsTable 1 }

DcbPfcStatsEntry ::= SEQUENCE {
    dcbPfcStatsInXoffFrames         Counter64,
    dcbPfcStatsInXonFrames          Counter64,
    dcbPfcStatsOutXoffFrames        Counter64,
    dcbPfcStatsOutXonFrames         Counter64,
    dcbPfcStatsXonToXoffs           Counter64,
    pfcUserPriorityIndex            Integer32
}

dcbPfcStatsInXoffFrames OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Number of Priority Flow Control Xoff frames received"
    ::= { dcbPfcStatsEntry 1 }

dcbPfcStatsInXonFrames OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Number of Priority Flow Control Xon frames received"
    ::= { dcbPfcStatsEntry 2 }

dcbPfcStatsOutXoffFrames OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Number of Priority Flow Control Xoff frames transmitted"
    ::= { dcbPfcStatsEntry 3 }

dcbPfcStatsOutXonFrames OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Number of Priority Flow Control Xon frames transmitted"
    ::= { dcbPfcStatsEntry 4 }

dcbPfcStatsXonToXoffs OBJECT-TYPE
    SYNTAX		Counter64
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "Number of times status has transitioned from 'not paused'
         to 'paused'."
    ::= { dcbPfcStatsEntry 5 }

pfcUserPriorityIndex OBJECT-TYPE
    SYNTAX		Integer32 (0..255)
    MAX-ACCESS	read-only
    STATUS		current
    DESCRIPTION
        "User Priority"
    ::= { dcbPfcStatsEntry 6 }

-- ******
-- events
-- ******

events OBJECT IDENTIFIER ::= { intel-dcb 2 }

-- **********************
-- DCB Events
-- **********************
dcbEvents OBJECT IDENTIFIER ::= { events 5 }

dcbTraps OBJECT IDENTIFIER ::= { dcbEvents 1 }

dcbPgOperStatusChangedTrap 	NOTIFICATION-TYPE
    OBJECTS		{ physicalAdapterIndex, dcbPgOperMode, dcbPgOperBandwidths, dcbPgOperMappingUPtoTC}
    STATUS		current
    DESCRIPTION
        "The Priority Groups operational mode
         or operational configuration for the adapter has changed."
    ::= { dcbTraps 1 }

dcbPfcOperStatusChangedTrap NOTIFICATION-TYPE
    OBJECTS	 	{ physicalAdapterIndex, dcbPfcOperMode, dcbPfcOperSettings }
    STATUS		current
    DESCRIPTION
        "The Priority Flow Control operational mode
         or operational configuration for the adapter has changed."
    ::= { dcbTraps 2 }

dcbFcoeOperStatusChangedTrap NOTIFICATION-TYPE
    OBJECTS	 	{ physicalAdapterIndex, dcbFcoeSubType, dcbFcoeOperMode, dcbFcoeOperData }
    STATUS		current
    DESCRIPTION
        "The FCoE Application:SubType operational mode
         or operational configuration for the adapter has changed."
    ::= { dcbTraps 3 }

dcbiScsiOperStatusChangedTrap NOTIFICATION-TYPE
    OBJECTS	 	{ physicalAdapterIndex, dcbiScsiSubType, dcbiScsiOperMode, dcbiScsiOperData }
    STATUS		current
    DESCRIPTION
        "The iSCSI Application:SubType operational mode or operational configuration for the adapter has changed."
    ::= { dcbTraps 5 }

dcbPgOperStatusChgTrapEnable OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "Enable or disable traps for the adapter's Priority
         Group Oper mode/configuration changed condition.
         The user can set this value."
    ::= { dcbEvents 2 }

dcbPfcOperStatusChgTrapEnable OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "Enable or disable traps for the adapter's Priority Flow
         Control Oper mode/configuration changed condition.
         The user can set this value."
    ::= { dcbEvents 3 }

dcbFcoeOperStatusChgTrapEnable OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "Enable or disable traps for the adapter's FCoE
         Application Oper mode/configuration changed condition.
         The user can set this value."
    ::= { dcbEvents 4 }

dcbiScsiOperStatusChgTrapEnable OBJECT-TYPE
    SYNTAX		Ables
    MAX-ACCESS	read-write
    STATUS		current
    DESCRIPTION
        "Enable or disable traps for the  adapter's iSCSI
         Application Oper mode/configuration changed condition.
         The user can set this value."
    ::= { dcbEvents 6 }


--
-- Compliance Statements
--

inteldcblanConformance  OBJECT IDENTIFIER ::= { inteldcblan 1 }

dcbiScsiGroups			OBJECT IDENTIFIER ::= { inteldcblanConformance 5 }
dcbPgGroups				OBJECT IDENTIFIER ::= { inteldcblanConformance 10 }
dcbPfcGroups			OBJECT IDENTIFIER ::= { inteldcblanConformance 15 }
dcbFcoeGroups			OBJECT IDENTIFIER ::= { inteldcblanConformance 20 }
dcbMiscGroups			OBJECT IDENTIFIER ::= { inteldcblanConformance 25 }
dcbNotificationGroups   OBJECT IDENTIFIER ::= { inteldcblanConformance 12 }
inteldcblanCompliances  OBJECT IDENTIFIER ::= { inteldcblanConformance 30 }

inteldcblanCompliance  MODULE-COMPLIANCE
     STATUS      current

     DESCRIPTION
       "Compliance statements for the Intel DCB Lan Agent."

     MODULE -- this module
     MANDATORY-GROUPS { dcbiScsiGroup, dcbPgGroup, dcbPfcGroup, dcbFcoeGroup, dcbMiscGroup, dcbNotificationGroup }

     ::= { inteldcblanCompliances 1 }

dcbiScsiGroup OBJECT-GROUP
     OBJECTS { dcbiScsiConfigEnable,dcbiScsiConfigWilling,dcbiScsiConfigAdvertise,dcbiScsiConfigData,
                dcbiScsiConfigSelector, dcbiScsiConfigIdentifier,
                dcbiScsiOperVersion,dcbiScsiOperMaxVersion,dcbiScsiOperError,
                dcbiScsiOperMode,dcbiScsiOperSyncd,dcbiScsiSubType,
                dcbiScsiOperSelector, dcbiScsiOperIdentifier,
                dcbiScsiPeerEnable,dcbiScsiPeerWilling,dcbiScsiPeerVersion,
                dcbiScsiPeerMaxVersion,dcbiScsiPeerError,dcbiScsiPeerData,
                dcbiScsiPeerSelector, dcbiScsiPeerIdentifier,
                dcbiScsiOperStatusChgTrapEnable
                }
      STATUS current
      DESCRIPTION
        "A collection for Dcb iSCSI Group"
       ::= { dcbiScsiGroups 1 }

dcbPgGroup OBJECT-GROUP
     OBJECTS { dcbPgConfigEnable, dcbPgConfigRecEnable,
                dcbPgConfigWilling, dcbPgConfigAdvertise, dcbPgConfigBandwidths,
                dcbPgConfigNumTCs, dcbPgBwgId,
                dcbPgBwgName, dcbPgConfigRecBandwidths,
                dcbPgPeerEnable, dcbPgPeerWilling,
                dcbPgPeerVersion, dcbPgPeerMaxVersion, dcbPgPeerError, dcbPgPeerBandwidths,
                dcbPgPeerNumTCs, dcbiScsiOperData,
                dcbPgStatsInFrames, pgTrafficClassIndex, pfcUserPriorityIndex,
                dcbPgStatsOutFrames, dcbPgStatsOutFrmOverflowDiscards,
                dcbPgStatsInFrmOverflowDiscards, dcbPgStatsInOctets,
                dcbPgStatsOutOctets,
                dcbPgOperStatusChgTrapEnable,
                dcbPgOperBandwidths, dcbPgOperMappingUPtoTC, dcbPgOperSyncd, dcbPgOperMode, dcbPgOperError,
                dcbPgOperMaxVersion, dcbPgOperVersion
                }
      STATUS current
      DESCRIPTION
        "A collection for Dcb Pg Group"
       ::= { dcbPgGroups 1 }

dcbPfcGroup OBJECT-GROUP
     OBJECTS { dcbPfcConfigEnable,
                dcbPfcConfigWilling, dcbPfcConfigAdvertise, dcbPfcConfigSettings, dcbPfcConfigNumTCs,
                dcbPfcPeerEnable, dcbPfcPeerWilling,
                dcbPfcPeerVersion, dcbPfcPeerMaxVersion, dcbPfcPeerError, dcbPfcPeerSettings,
                dcbPfcPeerNumTCs,
                dcbPfcStatsInXoffFrames, dcbPfcStatsInXonFrames, dcbPfcStatsOutXoffFrames,
                dcbPfcStatsOutXonFrames, dcbPfcStatsXonToXoffs,
                dcbPfcOperStatusChgTrapEnable,
                dcbPfcOperSettings, dcbPfcOperSyncd, dcbPfcOperMode, dcbPfcOperError,
                dcbPfcOperMaxVersion, dcbPfcOperVersion
                }
      STATUS current
      DESCRIPTION
        "A collection for Dcb Pfc Group"
       ::= { dcbPfcGroups 1 }

dcbFcoeGroup OBJECT-GROUP
     OBJECTS {  dcbFcoeConfigEnable, dcbFcoeConfigSelector, dcbFcoeConfigIdentifier,
                dcbFcoeConfigWilling, dcbFcoeConfigAdvertise, dcbFcoeConfigData,
                dcbFcoePeerEnable, dcbFcoePeerSelector, dcbFcoePeerIdentifier,
                dcbFcoePeerWilling, dcbFcoePeerVersion, dcbFcoePeerMaxVersion,
                dcbFcoePeerError, dcbFcoePeerData,
                dcbFcoeOperStatusChgTrapEnable,
                dcbFcoeSubType, dcbFcoeOperData, dcbFcoeOperSyncd,
                dcbFcoeOperMode, dcbFcoeOperError, dcbFcoeOperMaxVersion,
                dcbFcoeOperVersion, dcbFcoeOperSelector, dcbFcoeOperIdentifier
                }
      STATUS current
      DESCRIPTION
        "A collection for Dcb FCOE Group"
       ::= { dcbFcoeGroups 1 }

dcbMiscGroup OBJECT-GROUP
     OBJECTS { dcbConfigEnable, dcbVersion, dcbOperVersion, dcbOsControlledEnable
                }
      STATUS current
      DESCRIPTION
        "A collection for Dcb Misc Group"
       ::= { dcbMiscGroups 1 }

dcbNotificationGroup NOTIFICATION-GROUP
    NOTIFICATIONS  {
        dcbiScsiOperStatusChangedTrap,
        dcbPgOperStatusChangedTrap,
        dcbPfcOperStatusChangedTrap,
        dcbFcoeOperStatusChangedTrap
    }
    STATUS current
    DESCRIPTION
        "A collection of notification  for Dcb Group"
       ::= { dcbNotificationGroups 1 }

-- Compliance statement end

END
