
Intel 8255xER / 82562 Fast Ethernet Embedded XP driver Information

November 21
================================================================


This embedded XP driver supports Intel 8255xER and 82562 CICH Fast Ethernet controllers 



Driver installation procedure
================================================================

(1). Using the embedded XP component database manager, import the .sld file (e100.sld) into your database. 

(2). Set the file paths for e100e325.sys, e100exp.inf, and e100.sld
	
	Do either of the following:

	     - Copy e100ent.sys, e100b325.sys, e100.sld, e100exp.inf, and net559ER.inf to c:\e100exp

	or

	     - Copy e100ent.sys, e100b325.sys, e100.sld, e100exp.inf, and net559ER.inf to the directory of your choice
	     - Using the embedded XP component manager, open e100.sld and select the component you want to install
	     - Open the "files" section of the component
	     - In the right pane, for each file, right click and select "properties"
	     - Click the "advanced" button
	     - Highlight the "SrcPath" line and click the "edit" button
	     - Change the value to the directory where the respective file resides.  Be sure to include the drive
	       letter, but do not include a trailing backslash ( \ )
	     - Click "OK" to save these changes

(3). In the embedded XP target designer:

        Under hardware->devices->Network Adapters, add the network adapter you'd like to include in your image
	       Intel(R) Pro/100 VE Network Connection, 
	       Intel(R) Pro/100 VM Network Connection,
               Intel(R) 82562 based Fast Ethernet Connection*, or
	       Intel(R) 8255xER Fast Ethernet Controller

	*This component is for CICH devices (Device ID 2459 and 245D).
	 

(4). Build and Install your OS image according to the instructions provided with the Microsoft embedded XP Target Designer.



