************************************************************
** ENU *****************************************************
************************************************************
*                                                           
*  Intel(R) Chipset Software Installation Utility
*  Installation Readme
*                                                           
*  NOTE:  This document refers to systems containing the 
*         following Intel chipsets: 
*              Intel(R) 810  Chipset 
*              Intel(R) 810E Chipset
*              Intel(R) 815  Chipset
*              Intel(R) 815E Chipset
*              Intel(R) 820  Chipset
*              Intel(R) 820E Chipset
*              Intel(R) 840  Chipset
*              Intel(R) 430TX PCIset 
*              Intel(R) 440BX AGPset 
*              Intel(R) 440DX AGPset 
*              Intel(R) 440EX AGPset 
*              Intel(R) 440GX AGPset 
*              Intel(R) 440LX AGPset 
*              Intel(R) 440MX Chipset 
*              Intel(R) 440ZX AGPset
*              
*
************************************************************
************************************************************


************************************************************
*  CONTENTS OF THIS DOCUMENT
************************************************************
This document contains the following sections:

1.  Overview
2.  System Requirements
3.  Installing the Software
    3A. Installing the Software in Interactive Mode
    3B. Installing the Software in Silent Mode
    3C. List of Available Command Line Flag Options
4.  Verifying Installation of the Software
5.  Contents of the Distribution Package
6.  Identifying the Software Version Number
7.  Troubleshooting

************************************************************
* 1.  OVERVIEW
************************************************************
The Intel(R) Chipset Software Installation Utility installs
to the target system the Windows* INF files that outline to 
the operating system how the chipset components will be 
configured.  This is needed for the proper functioning of
the following features:

   - Core PCI and ISAPNP Services
   - AGP Support
   - IDE/ATA33/ATA66 Storage Support
   - USB Support
   - Identification of Intel Chipset Components in 
     Device Manager

************************************************************
* 2.  SYSTEM REQUIREMENTS 
************************************************************
1.  The software included with this distribution package is 
    designed to operate with the following chipset 
    configurations:

          Intel(R) 810  Chipset 
          Intel(R) 810E Chipset
          Intel(R) 815  Chipset
          Intel(R) 815E Chipset
          Intel(R) 820  Chipset
          Intel(R) 820E Chipset
          Intel(R) 840  Chipset
          Intel(R) 430TX PCIset 
          Intel(R) 440BX AGPset 
          Intel(R) 440DX AGPset 
          Intel(R) 440EX AGPset 
          Intel(R) 440GX AGPset 
          Intel(R) 440LX AGPset 
          Intel(R) 440MX Chipset 
          Intel(R) 440ZX AGPset
              
2.  One of the following operating systems must be 
    installed on the system:
    Windows 95      4.00.950   (Original release)
    Windows 95      4.00.950a  (OSR1)
    Windows 95      4.00.950b  (OSR2 without USB 
                                Supplement)
    Windows 95      4.00.950b  (OSR2.1 with USB 
                                Supplement)
    Windows 95      4.00.950c  (OSR2.5 with or 
                                without USB Supplement)
    Windows 98      4.10.1998  (Original release)
    Windows 98 Second Edition
                    4.10.2222  (Original release)         
    Windows 2000    5.00.2195  (Original release)

To verify which operating system has been installed onto 
the target system, follow the steps below:

    a.  Click on Start.
    b.  Select Settings.
    c.  Select Control Panel.
    d.  Double-click on the System icon.
    e.  Click on the General system properties tab.
    f.  Verify which OS has been installed by reading
        the System information.
                              
3.  The software should be installed on systems with at
    least 32 MB of system memory.

4.  There should be sufficient hard disk space in the <TEMP>
    directory (typically C:\WINDOWS\TEMP) of the system on
    which this software is installed.

Please check with your system provider to determine which 
operating system and Intel chipset are used in your system.  

************************************************************
* 3.  INSTALLING THE SOFTWARE 
************************************************************
This software can be installed in two modes: Interactive or 
Silent.  The Interactive Mode requires user input during
installation; the Silent Mode does not.

Additionally, this software offers a set of command line
flag options that enable extended installation functionality.
The command line flags are not case-sensitive.  See Section 
3C for detailed descriptions of these flags.

Important Note:
The Intel(R) Chipset Software Installation Utility is 
distributed in two formats -- self extracting .EXE files
(INFINST_xxx.EXE) or compressed .ZIP files (INFINST_xxx.ZIP).  
Depending on which distribution format is being executed, 
the command-line syntax may differ.  See Section 3C for more
details.


************************************************************
* 3A.  INSTALLING THE SOFTWARE IN INTERACTIVE MODE
************************************************************
1.  Check the System Requirements.  The operating system 
    must be fully installed and running on the system before
    running this software.

2.  Close any running applications.  Otherwise, you may
    experience difficulties.

3.  Run the InstallShield* installation program:
       Self-extracting .EXE distribution: INFINST_xxx.EXE
       Compressed .ZIP distribution     : SETUP.EXE

4.  You will be prompted to agree to the license agreement.  
    If you do not agree, the Installer will exit before 
    extracting any files.
    
5.  Follow the on-screen instructions and use the default
    settings to complete the setup, once the operating
    system has rebooted.

6.  This completes the installation of the Intel(R) Chipset 
    Software Installation Utility.  


************************************************************
* 3B.  INSTALLING THE SOFTWARE IN SILENT MODE
************************************************************
1.  Check the System Requirements.  The operating system 
    must be fully installed and running on the system before 
    running this software.

2.  Close any running applications.  Otherwise, you may 
    experience difficulties.

3.  Run the InstallShield installation program:
    For silent install with auto-reboot:
       Self-extracting .EXE distribution: INFINST_xxx.EXE -a -b -s
       Compressed .ZIP distribution     : SETUP.EXE -b -s
    - OR -
    For silent install without auto-reboot:
       Self-extracting .EXE distribution: INFINST_xxx.EXE -a -s
       Compressed .ZIP distribution     : SETUP.EXE -s

4.  The utility will perform the necessary updates and record
    the installation status in the following system registry 
    key:
        HKEY_LOCAL_MACHINE\Software\Intel\INFInst

5.  If the utility was invoked with the "-b" flag, the 
    system will automatically reboot if the update was
    successful.

    NOTE:  The system MUST be rebooted for all device updates
           to take effect.

6.  To determine whether the install was successful, verify 
    the 'install' value in the registry key specified in Step 5.

    The following table describes the various parameter values:

    Value      Type      Data            Description
    ------     ----      ----            -----------
    "install"  String    "success"       The installation was successful.
                         "fail"          The installation was not successful.
                                         No INF files were copied to the 
                                         system.                

    "reboot"   String    "Yes"           A reboot is required to complete 
                                         the installation.
                         "No"            No reboot is required to complete 
                                         the installation.
                                
    "version"  String    <varies>        Current version number of the 
                                         Intel(R) Chipset Software 
                                         Installation Utility
                                         

************************************************************
* 3C.  LIST OF AVAILABLE COMMAND LINE FLAG OPTIONS
************************************************************
The Intel(R) Chipset Software Installation Utility supports  
several command line flags for various installation options. 
All command line flags and parameters must be separated by a 
space, except for the language code after the '-L' flag.

Due to the different distribution formats available for the
Intel(R) Chipset Software Installation Utility, the command
line flag syntax may vary:

1. Self-Extracting .EXE Distribution:
      When installing this software using the .EXE distribution,
      an extra '-A' must be appended to the INFINST_xxx.EXE 
      program call (i.e. INFINST_ENU.EXE -A) in order to 
      successfully pass command line parameters.  The extra 
      '-A' flag for the self-extracting .EXE package
      is DIFFERENT from the '-A' command line flag option 
      described below.  

      Example: To extract INF files using the '-A' flag 
               described below, the installation program 
               should be invoked as follows:  
          
               INFINST_ENU.EXE -A -A (optional -P)

2. Compressed .ZIP Distribution:
      When installing this software using the .ZIP distribution,
      there is no need to append any extra flags to the SETUP.EXE 
      program call in order to pass command line flags.
      Example: To extract INF files using the '-A' flag 
               described below, the installation program 
               should be invoked as follows:  
                        
               SETUP.EXE -A (optional -P)

Below is a list of all the available command line flags that
may be used with the program call.  Note that the '-L' and 
the '-S' flags MUST be specified at the end of the command line 
flag list.

Flag            Description
----            -----------
-?              Help flag.  Displays the list of available command line
                flags.  This parameter works in the Interactive mode only.  
-A              Extracts INF files, README.TXT, RELNOTES.TXT, and 
                instructions for OEM preload (PRELOAD.TXT) to either 
                "C:\Program Files\Intel\InfInst" or the <Installation Path> directory 
                specified using the '-P' flag.  The software will NOT
                install these INF files to the system.  This flag can 
                be combined only with the '-P' flag option.  All other 
                options will be ignored if the '-A' flag is specified. 
                This parameter works in either Silent mode or Interactive 
                mode.

-B              Automatically reboots the system after installation.  
                This flag is ignored if '-A' flag is specified.  This 
                parameter works in either Silent mode or Interactive mode.

-L<LangCode>    Forces the InstallShield user interface to 
                display the specified language during setup.  
                Note that there should be NO spaces between '-L' 
                and the 4-digit language code (see below).  This 
                flag and the '-S' flag must be placed at the end 
                of the command line flag list.  This parameter works 
                in Interactive mode only.

-P <Installation Path>   
                Specifies the HDD location to which the INF program
                files are copied.  If this flag is not specified 
                at the command line, the <Installation Path> 
                directory is by default assumed to be:
                
                   C:\Program Files\Intel\INFInst
                
                If this flag is used without the
                '-A' option, only README.TXT and RELNOTES.TXT will
                be copied to <Installation Path>.  The directory name can 
                include spaces.  In this case, however, a pair of double
                quotes (") must enclose the directory name.  This parameter 
                works in either Silent mode or Interactive mode.

-S              Runs the Installer in silent mode.  No user interface
                is displayed.   This flag and the '-L' flag
                must be placed at the end of the command line
                flag list.

                
Below are the language codes used with the '-L' flag:

    Language                   <LangCode>
    --------                   ----------
    Chinese (PRC)                 0804
    Chinese (Taiwan)              0404
    Danish                        0006
    Dutch                         0013
    English (UK - International)  0809
    English (US)                  0409
    Finnish                       000B
    French (Canadian)             0C0C
    French (Standard)             040C
    German                        0007
    Italian                       0010
    Japanese                      0011
    Korean                        0012
    Norwegian                     0014
    Polish                        0015
    Portuguese (Brazilian)        0416
    Portuguese (Standard)         0816
    Russian                       0019
    Spanish                       000A
    Swedish                       001D
    Thai                          001E

************************************************************
* 4.  VERIFYING INSTALLATION OF THE SOFTWARE
************************************************************
Run Device Manager to verify the correct installation and
usage of the INF files.

For Windows 95, Windows 98 and Windows 98 Second Edition:

   1.  Click on Start.
   2.  Select Settings.
   3.  Select Control Panel.
   4.  Double-click on System icon.
   5.  Click on Device Manager tab.
   6.  Click on View Devices by Connection button.
   7.  Click on Plug and Play BIOS, or 
       Advanced Configuration and Power Interface (ACPI) BIOS.
   8.  Click on PCI bus.

For Windows 2000:

   1.  Click on Start.
   2.  Select Settings.
   3.  Select Control Panel.
   4.  Double-click on System icon.
   5.  Click on Hardware tab.
   6.  Click on Device Manager button.
   7.  From the View menu, select menu item Devices by connection.
   8.  Click on Standard PC, or
       Advanced Configuration and Power Interface (ACPI) PC.
   9.  Click on PCI bus.

After the Device Manager is launched as described above, check the 
descriptions for the following entries:

    *** NOTE:  Device Manager will display only the names of devices         
               currently detected in the system.

    Intel(R) 810 Chipset:
        Intel(R) 82810 System and Graphics Controller 
        -or-
        Intel(R) 82810 DC-100 System and Graphics Controller
  
    Intel(R) 810E Chipset:
        Intel(R) 82810E DC-133 System and Graphics Controller

    Intel(R) 820 Chipset:
        Intel(R) 82820 Processor to I/O Controller
        Intel(R) 82820 Processor to AGP Controller

    Intel(R) 840 Chipset:
        Intel(R) 82840 Processor to I/O Controller 
        Intel(R) 82840 Processor to AGP Controller 
        Intel(R) 82840 PCI Bridge 
              
     Intel(R) 82806AA PCI 64-bit Hub:
        Intel(R) 82806AA Advanced Programmable Interrupt Controller
        Intel(R) 82806AA PCI Bridge
        Intel(R) 82806AA Controller (reserved)

    Intel(R) 82801AA I/O Controller Hub (ICH):
        Intel(R) 82801AA LPC Interface Controller 
        Intel(R) 82801AA Ultra ATA Controller 
        Intel(R) 82801AA USB Universal Host Controller 
        Intel(R) 82801AA SMBus Controller 
        Intel(R) 82801AA PCI Bridge 
      
    Intel(R) 82801AB I/O Controller Hub (ICH0):
        Intel(R) 82801AB LPC Interface Controller 
        Intel(R) 82801AB Ultra ATA Controller 
        Intel(R) 82801AB USB Universal Host Controller 
        Intel(R) 82801AB SMBus Controller 
        Intel(R) 82801AB PCI Bridge 

    Intel(R) 82371AB PCI to ISA/IDE Xcelerator (PIIX4):
        Intel(R) 82371AB PCI to ISA bridge (EIO mode)
        Intel(R) 82371AB PCI to ISA bridge (ISA mode)
        Intel(R) 82371AB Power Management Controller
        Intel(R) 82371AB/EB/MB PCI Bus Master IDE Controller
        Intel(R) 82371AB/EB/MB PCI to USB Universal Host Controller
   
    Intel(R) 82371EB/MB PCI to ISA/IDE Xcelerator (PIIX4):
        Intel(R) 82371EB/MB PCI to ISA bridge (EIO mode)
        Intel(R) 82371EB/MB PCI to ISA bridge (ISA mode)
        Intel(R) 82371EB/MB Power Management Controller
        Intel(R) 82371AB/EB/MB PCI Bus Master IDE Controller
        Intel(R) 82371AB/EB/MB PCI to USB Universal Host Controller

    Intel(R) 82371SB PCI to ISA/IDE Xcelerator (PIIX3):
        Intel(R) 82371SB PCI to ISA bridge
        Intel(R) 82371SB PCI Bus Master IDE Controller
        Intel(R) 82371SB PCI to USB Universal Host Controller    

    Intel(R) 440MX Chipset:
        Intel(R) 82440MX Processor to I/O Controller
        Intel(R) 82440MX PCI to ISA Bridge
        Intel(R) 82440MX Power Management Controller
        Intel(R) 82440MX Bus Master IDE Controller
        Intel(R) 82440MX USB Universal Host Controller

    Intel(R) 430TX PCIset:
        Intel(R) 82443TX Processor to PCI bridge

    Intel(R) 440BX AGPset, Intel(R) 440DX AGPset, Intel(R) 440ZX AGPset:
        Intel(R) 82443BX/ZX/DX Processor to PCI bridge
        Intel(R) 82443BX/ZX/DX Processor to AGP controller

    Intel(R) 440GX AGPset:
        Intel(R) 82443GX Processor to PCI bridge
        Intel(R) 82443GX Processor to AGP controller

    Intel(R) 440LX AGPset:
        Intel(R) 82443LX Processor to PCI bridge
        Intel(R) 82443LX Processor to AGP controller

    Intel(R) 815 Chipset:
        Intel(R) 82815 Processor to I/O Controller - 1130 
        Intel(R) 82815 Processor to AGP Controller - 1131 

   Intel(R) 82801BA/BAM I/O Controller Hub:
        Intel(R) 82801BA LPC Interface Controller - 2440 
        Intel(R) 82801BA PCI Bridge - 244E 
        Intel(R) 82801BA Ultra ATA Storage Controller - 244B 
        Intel(R) 82801BA/BAM SMBus Controller - 2443 
        Intel(R) 82801BA/BAM USB Universal Host Controller - 2442 
        Intel(R) 82801BA/BAM USB Universal Host Controller - 2444 
        Intel(R) 82801BA/BAM AC '97 Audio Controller - 2445 

10. On certain systems, the following device may also be updated:

    Intel(R) 810, Intel(R) 810E, Intel(R) 815, Intel(R) 815E,
    Intel(R) 820, Intel(R) 820E or Intel(R) 840 Chipset:

     a. Click on View Devices by Connection button.
     b. Click on Plug & Play BIOS, or
        Advanced Configuration and Power Interface (ACPI) BIOS.     
     c. Verify that the following entry is present:
        Intel(R) 82802 Firmware Hub Device -OR-
        Intel(R) Security Driver


************************************************************
* 5.  CONTENTS OF THE DISTRIBUTION PACKAGE
************************************************************
The Intel(R) Chipset Software Installation Utility package 
contains the following items:

    File(s)       
    -------
    INFINST_xxx.EXE -or- INFINST_xxx.ZIP
    README.TXT
    RELNOTES.TXT

The version of the software included in the distribution
package is specified in the file RELNOTES.TXT.  

RELNOTES.TXT is available in English only.

After installation on a Windows 95 or Windows 98 system, 
one or more of the following INF files are copied 
to the <Windows>\INF directory:

    File(s)
    -------
    440MXCOR.INF
    440MXIDE.INF
    440MXUSB.INF
    810.INF
    810B.INF
    815.INF
    820.INF
    820B.INF
    840.INF
    ICHx.INF
    ICHxIDE.INF
    ICHxSMB.INF
    ICHxUSB.INF
    IFWH.INF
    IHOST.INF
    P64H.INF
    P64HRES.INF
    PIIXXIDE.INF
    PIIXXUSB.INF
    PIIX4.INF
    ICH2CORE.INF
    ICH2IDE.INF
    ICH2SMB.INF
    ICH2USB.INF
    ICH2AUD.INF
    
   *** NOTE:  Only the files that reference the currently 
              detected devices are copied to the system.
              If the -A option is exercised, the files are
              not copied to the <Windows>\INF directory.
              See Section 3C for more information.

One or more of the following digital signature files are 
installed to the <Windows>\CATROOT directory on a 
Windows 98 system ONLY:

    File(s)
    -------
    440MXCOR.CAT
    440MXIDE.CAT
    440MXUSB.CAT
    810.CAT
    820.CAT
    820B.CAT
    840.CAT
    ICHx.CAT
    ICHxIDE.CAT
    ICHxSMB.CAT
    ICHxUSB.CAT
    IFWH.CAT
    P64H.CAT
    P64HRES.CAT
    815.CAT
    ICH2CORE.CAT
    ICH2IDE.CAT
    ICH2SMB.CAT
    ICH2USB.CAT
    ICH2AUD.CAT

   *** NOTE:  Only the files that reference the currently 
              detected devices are copied to the system.
              If the -A option is exercised, the files are
              not copied to the <Windows>\CATROOT directory.
              See Section 3C for more information.              

************************************************************
* 6.  IDENTIFYING THE SOFTWARE VERSION NUMBER
************************************************************
The version of the software included in the distribution
package is specified in the file RELNOTES.TXT.  

RELNOTES.TXT is available in English only.

The version of the software included in the distribution 
package can also be identified by examining the following 
registry location:

    Key name:   \\HKEY_LOCAL_MACHINE\Software\Intel\InfInst
    Value name: version

************************************************************
* 7.  TROUBLESHOOTING
************************************************************
It is assumed that the system requirements in Section 2 
above have been satisfied.

Issue:      System locks up during Device Manager Remove or 
            during restart.

Solution:   System lockup can occur during Restart as a 
            result of several possible system issues.  In 
            the event of system lockup, restart the machine 
            and view Device Manager.  If devices are listed 
            properly and the system experiences no further 
            problems, then the .INF file restore process was 
            successful.  If devices are not configured 
            correctly, try re-running the procedures outlined 
            in Section 3.

            If this does not fix problems or further 
            problems are experienced, reinstall the 
            operating system.


Issue:      After running the setup program and rebooting the
            machine, Windows reports that it cannot find one 
            of the following files:
                  ESDI_506.pdr

Solution:   Click Browse in the dialog box where this problem
            occurs, locate the
                  <Windows>\System\IOSubsys

            directory and click OK.  The system should
            be able to locate this file in this directory 
            and continue re-enumerating for the new devices.

Issue:      After running the setup program and rebooting the
            machine, Windows reports that it cannot find one 
            of the following files:
 
                  UHCD.SYS
                  USBD.SYS
                  USBHUB.SYS

Solution:   Click Browse in the dialog box where this problem
            occurs, locate the

                  <Windows>\System32\drivers (for Windows 98)
                   -or-
                  <Windows>\System           (for Windows 95)

            directory, and click OK.  The system should
            be able to locate this file in this directory 
            and continue re-enumerating for the new devices.

Issue:      During setup, installation stops and prompts for one
            of the following files:
      
                  UHCD.SYS
                  USBD.SYS
                  USBHUB.SYS

Solution:   Ensure that the Windows 95 USB Supplement has been 
            installed prior to running the Intel(R) Chipset Software 
            Installation Utility setup program.

Issue:      After running the setup program and rebooting the
            machine, Windows reports that it cannot find the 
            following file:
                  isapnp.vxd

Solution:   Click Browse in the dialog box where this problem
            occurs, locate the

                  <Windows>\System

            directory, and click OK.  The system should
            be able to locate this file in this directory 
            and continue re-enumerating for the new devices.

Issue:      After performing the silent install, the 
            HKLM\Software\Intel\InfInst key was not created 
            or the data of the value "install" is not 
            "success".

Solution:   This is caused by one of the following scenarios:
               - The current system does not contain 
                 a supported operating system, or
               - The current system does not contain 
                 a supported chipset.

            Verify the System Requirements in Section 2.

************************************************************
************************************************************
* DISCLAIMER
************************************************************
Intel is making no claims of usability, efficacy or 
warranty.  
The INTEL SOFTWARE LICENSE AGREEMENT
(OEM / IHV / ISV Distribution & Single User) 
completely defines the licensed use of this software.
************************************************************
Information in this document is provided in connection with 
Intel products.  No license, express or implied, by estoppel 
or otherwise, to any intellectual property rights is granted 
by this document.  Intel assumes no liability whatsoever, 
and Intel disclaims any express or implied warranty 
relating to sale and/or use of Intel products, including 
liability or warranties relating to fitness for a particular 
purpose, merchantability or infringement of any patent, 
copyright or other intellectual property right.  Intel 
products are not intended for use in medical, life saving, 
or life-sustaining applications.

************************************************************
Intel Corporation disclaims all warranties and liabilities 
for the use of this document and the information contained 
herein, and assumes no responsibility for any errors which 
may appear in this document, nor does Intel make a 
commitment to update the information contained herein.  Intel 
reserves the right to make changes to this document at any 
time, without notice.
************************************************************
************************************************************

* Third-party brands and names are the property of their 
respective owners.

Copyright (c) Intel Corporation, 1997-2000


