 -- Copyright (C) 1991-2011 Altera Corporation
 -- Your use of Altera Corporation's design tools, logic functions 
 -- and other software and tools, and its AMPP partner logic 
 -- functions, and any output files from any of the foregoing 
 -- (including device programming or simulation files), and any 
 -- associated documentation or information are expressly subject 
 -- to the terms and conditions of the Altera Program License 
 -- Subscription Agreement, Altera MegaCore Function License 
 -- Agreement, or other applicable license agreement, including, 
 -- without limitation, that your use is for the sole purpose of 
 -- programming logic devices manufactured by Altera and sold by 
 -- Altera or its authorized distributors.  Please refer to the 
 -- applicable agreement for further details.
 -- 
 -- This is a Quartus II output file. It is for reporting purposes only, and is
 -- not intended for use as a Quartus II input file. This file cannot be used
 -- to make Quartus II pin assignments - for instructions on how to make pin
 -- assignments, please see Quartus II help.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- NC            : No Connect. This pin has no internal connection to the device.
 -- DNU           : Do Not Use. This pin MUST NOT be connected.
 -- VCCPGM        : Dedicated power pin for configuration, which MUST be connected to 1.8V, 2.5V or 3.0V depending on the requirements of the configuration device.
 -- VCCINT        : Dedicated power pin, which MUST be connected to VCC  (0.9V).
 -- VCCIO         : Dedicated power pin, which MUST be connected to VCC
 --                 of its bank.
 --					Bank 3C:		2.5V
 --					Bank 3A:		2.5V
 --					Bank 4A:		2.5V
 --					Bank 5A:		2.5V
 --					Bank 6A:		3.3V
 --					Bank 7A:		2.5V
 --					Bank 8A:		3.3V
 --					Bank 8C:	2.5V
 -- RREF          : External reference resistor for the quad, MUST be connected to
 --                 GND via a 2k Ohm resistor.
 -- GND           : Dedicated ground pin. Dedicated GND pins MUST be connected to GND.
 --					It can also be used to report unused dedicated pins. The connection
 --					on the board for unused dedicated pins depends on whether this will
 --					be used in a future design. One example is device migration. When
 --					using device migration, refer to the device pin-tables. If it is a
 --					GND pin in the pin table or if it will not be used in a future design
 --					for another purpose the it MUST be connected to GND. If it is an unused
 --					dedicated pin, then it can be connected to a valid signal on the board
 --					(low, high, or toggling) if that signal is required for a different
 --					revision of the design.
 -- GND+          : Unused input pin. It can also be used to report unused dual-purpose pins.
 --					This pin should be connected to GND. It may also be connected  to a
 --					valid signal  on the board  (low, high, or toggling)  if that signal
 --					is required for a different revision of the design.
 -- GND*          : Unused  I/O  pin.   For transceiver I/O banks, connect each pin marked GND*
 --           	    either individually through a 10k Ohm resistor to GND or tie all pins
 --           	    together and connect through a single 10k Ohm resistor to GND.
 -- RESERVED      : Unused I/O pin, which MUST be left unconnected.
 -- RESERVED_INPUT    : Pin is tri-stated and should be connected to the board.
 -- RESERVED_INPUT_WITH_WEAK_PULLUP    : Pin is tri-stated with internal weak pull-up resistor.
 -- RESERVED_INPUT_WITH_BUS_HOLD       : Pin is tri-stated with bus-hold circuitry.
 -- RESERVED_OUTPUT_DRIVEN_HIGH        : Pin is output driven high.
 -- GXB_GND*      : Unused GXB Receiver or dedicated reference clock pin. This pin
 --                 must be connected to GXB_GND through a 10k Ohm resistor.
 -- GXB_NC        : Unused GXB Transmitter or dedicated clock output pin. This pin
 --                 must not be connected.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- Pin directions (input, output or bidir) are based on device operating in user mode.
 ---------------------------------------------------------------------------------

Quartus II 64-Bit Version 10.1 Build 197 01/19/2011 Service Pack 1 SJ Full Version
CHIP  "msmst_test"  ASSIGNED TO AN: EP2AGXE6XXFPGA

Pin Name/Usage               : Location  : Dir.   : I/O Standard      : Voltage : I/O Bank  : User Assignment
-------------------------------------------------------------------------------------------------------------
GND                          : A3        : gnd    :                   :         :           :                
GND                          : A4        : gnd    :                   :         :           :                
hsmc_rxn[4]                  : A5        : bidir  : 2.5 V             :         : 7A        : Y              
hsmc_rxp[4]                  : A6        : bidir  : 2.5 V             :         : 7A        : Y              
hsmc_rxn[5]                  : A7        : bidir  : 2.5 V             :         : 7A        : Y              
hsmc_rxp[5]                  : A8        : bidir  : 2.5 V             :         : 7A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : A9        :        :                   :         : 7A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : A10       :        :                   :         : 7A        :                
hsmc_rxn[6]                  : A11       : bidir  : 2.5 V             :         : 7A        : Y              
hsmc_rxp[6]                  : A12       : bidir  : 2.5 V             :         : 7A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : A13       :        :                   :         : 7A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : A14       :        :                   :         : 7A        :                
hsmc_d0_2n                   : A15       : bidir  : 2.5 V             :         : 7A        : Y              
hsmc_d0_2p                   : A16       : bidir  : 2.5 V             :         : 7A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : A17       :        :                   :         : 7A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : A18       :        :                   :         : 7A        :                
hsmc_clkout1n                : A19       : output : 2.5 V             :         : 7A        : Y              
hsmc_clkout1p                : A20       : output : 2.5 V             :         : 7A        : Y              
lpc_ad[3]                    : A21       : input  : 3.3-V LVCMOS      :         : 8A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : A22       :        :                   :         : 8A        :                
gpio_rxn[8]                  : A23       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_rxp[8]                  : A24       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_rxn[3]                  : A25       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_rxp[3]                  : A26       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_rxn[4]                  : A27       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_rxp[4]                  : A28       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
GND                          : A29       : gnd    :                   :         :           :                
GND                          : A30       : gnd    :                   :         :           :                
GND                          : A31       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AA1       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AA2       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AA3       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AA4       :        :                   :         : 5A        :                
VCCIO5A                      : AA5       : power  :                   : 2.5V    : 5A        :                
GND                          : AA6       : gnd    :                   :         :           :                
GND                          : AA7       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AA8       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AA9       :        :                   :         : 5A        :                
VREFB5AN0                    : AA10      : power  :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AA11      :        :                   :         : 5A        :                
GND                          : AA12      : gnd    :                   :         :           :                
VCC                          : AA13      : power  :                   : 0.9V    :           :                
GND                          : AA14      : gnd    :                   :         :           :                
VCC                          : AA15      : power  :                   : 0.9V    :           :                
GND                          : AA16      : gnd    :                   :         :           :                
VCC                          : AA17      : power  :                   : 0.9V    :           :                
GND                          : AA18      : gnd    :                   :         :           :                
VCC                          : AA19      : power  :                   : 0.9V    :           :                
GND                          : AA20      : gnd    :                   :         :           :                
VCC                          : AA21      : power  :                   : 0.9V    :           :                
GND                          : AA22      : gnd    :                   :         :           :                
GND                          : AA23      : gnd    :                   :         :           :                
VCCA                         : AA24      : power  :                   : 2.5V    :           :                
GND                          : AA25      : gnd    :                   :         :           :                
VCCL_GXB                     : AA26      : power  :                   : 1.1V    :           :                
GND                          : AA27      : gnd    :                   :         :           :                
GND                          : AA28      : gnd    :                   :         :           :                
GND                          : AA29      : gnd    :                   :         :           :                
GND                          : AA30      : gnd    :                   :         :           :                
clk_100MHz_pcie5             : AA31      : input  : HCSL              :         : QL0       : Y              
clk_100MHz_pcie5(n)          : AA32      : input  : HCSL              :         : QL0       : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : AB1       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AB2       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AB3       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AB4       :        :                   :         : 5A        :                
GND                          : AB5       : gnd    :                   :         :           :                
GND                          : AB6       : gnd    :                   :         :           :                
VCCIO5A                      : AB7       : power  :                   : 2.5V    : 5A        :                
GND                          : AB8       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AB9       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AB10      :        :                   :         : 5A        :                
GND                          : AB11      : gnd    :                   :         :           :                
GND                          : AB12      : gnd    :                   :         :           :                
VCCPD4A                      : AB13      : power  :                   : 2.5V    : 4A        :                
VCCPD4A                      : AB14      : power  :                   : 2.5V    : 4A        :                
GND                          : AB15      : gnd    :                   :         :           :                
GND                          : AB16      : gnd    :                   :         :           :                
VCCPD3A                      : AB17      : power  :                   : 2.5V    : 3A        :                
VCCPD3A                      : AB18      : power  :                   : 2.5V    : 3A        :                
GND                          : AB19      : gnd    :                   :         :           :                
VCCPD3C                      : AB20      : power  :                   : 2.5V    : 3C        :                
GND                          : AB21      : gnd    :                   :         :           :                
VCC                          : AB22      : power  :                   : 0.9V    :           :                
GND                          : AB23      : gnd    :                   :         :           :                
GND                          : AB24      : gnd    :                   :         :           :                
VCCL_GXB                     : AB25      : power  :                   : 1.1V    :           :                
GND                          : AB26      : gnd    :                   :         :           :                
VCCL_GXB                     : AB27      : power  :                   : 1.1V    :           :                
GND                          : AB28      : gnd    :                   :         :           :                
GXB_NC                       : AB29      :        :                   :         : QL0       :                
GXB_NC                       : AB30      :        :                   :         : QL0       :                
GND                          : AB31      : gnd    :                   :         :           :                
GND                          : AB32      : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AC1       :        :                   :         : 5A        :                
GND                          : AC2       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AC3       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AC4       :        :                   :         : 5A        :                
GND                          : AC5       : gnd    :                   :         :           :                
GND                          : AC6       : gnd    :                   :         :           :                
GND                          : AC7       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AC8       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AC9       :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AC10      :        :                   :         : 5A        :                
hsmc_txp[13]                 : AC11      : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_txp[15]                 : AC12      : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_txp[9]                  : AC13      : bidir  : 2.5 V             :         : 4A        : Y              
VREFB4AN0                    : AC14      : power  :                   :         : 4A        :                
hsmc_clkout2p                : AC15      : output : 2.5 V             :         : 4A        : Y              
hsmc_clkout2n                : AC16      : output : 2.5 V             :         : 4A        : Y              
VCCCB                        : AC17      : power  :                   : 1.5V    :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AC18      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AC19      :        :                   :         : 3A        :                
VREFB3AN0                    : AC20      : power  :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AC21      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AC22      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AC23      :        :                   :         : 3A        :                
GND                          : AC24      : gnd    :                   :         :           :                
GND                          : AC25      : gnd    :                   :         :           :                
GND                          : AC26      : gnd    :                   :         :           :                
GND                          : AC27      : gnd    :                   :         :           :                
GND                          : AC28      : gnd    :                   :         :           :                
GND                          : AC29      : gnd    :                   :         :           :                
GND                          : AC30      : gnd    :                   :         :           :                
GXB_GND*                     : AC31      :        :                   :         : QL0       :                
GXB_GND*                     : AC32      :        :                   :         : QL0       :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AD1       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AD2       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AD3       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AD4       :        :                   :         : 5A        :                
VCCIO5A                      : AD5       : power  :                   : 2.5V    : 5A        :                
GND                          : AD6       : gnd    :                   :         :           :                
GND                          : AD7       : gnd    :                   :         :           :                
VCCD_PLL_3                   : AD8       : power  :                   : 0.9V    :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AD9       :        :                   :         : 4A        :                
VCCIO4A                      : AD10      : power  :                   : 2.5V    : 4A        :                
hsmc_txn[13]                 : AD11      : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_txn[15]                 : AD12      : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_txn[9]                  : AD13      : bidir  : 2.5 V             :         : 4A        : Y              
VCCIO4A                      : AD14      : power  :                   : 2.5V    : 4A        :                
VCCIO4A                      : AD15      : power  :                   : 2.5V    : 4A        :                
hsmc_clkin2p                 : AD16      : input  : 2.5 V             :         : 3A        : Y              
VCCIO3A                      : AD17      : power  :                   : 2.5V    : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AD18      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AD19      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AD20      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AD21      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AD22      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AD23      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AD24      :        :                   :         : 3A        :                
VCCA_PLL_4                   : AD25      : power  :                   : 2.5V    :           :                
GND                          : AD26      : gnd    :                   :         :           :                
GND                          : AD27      : gnd    :                   :         :           :                
GND                          : AD28      : gnd    :                   :         :           :                
tx_out                       : AD29      : output : 1.5-V PCML        :         : QL0       : Y              
tx_out(n)                    : AD30      : output : 1.5-V PCML        :         : QL0       : Y              
GND                          : AD31      : gnd    :                   :         :           :                
GND                          : AD32      : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AE1       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AE2       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AE3       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AE4       :        :                   :         : 5A        :                
GND                          : AE5       : gnd    :                   :         :           :                
GND                          : AE6       : gnd    :                   :         :           :                
VCCIO5A                      : AE7       : power  :                   : 2.5V    : 5A        :                
GND                          : AE8       : gnd    :                   :         :           :                
VCCA_PLL_3                   : AE9       : power  :                   : 2.5V    :           :                
VCCIO4A                      : AE10      : power  :                   : 2.5V    : 4A        :                
GND                          : AE11      : gnd    :                   :         :           :                
hsmc_txp[8]                  : AE12      : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_txn[8]                  : AE13      : bidir  : 2.5 V             :         : 4A        : Y              
GND                          : AE14      : gnd    :                   :         :           :                
VCCIO4A                      : AE15      : power  :                   : 2.5V    : 4A        :                
hsmc_clkin2n                 : AE16      : input  : 2.5 V             :         : 3A        : Y              
GND                          : AE17      : gnd    :                   :         :           :                
VCCIO3A                      : AE18      : power  :                   : 2.5V    : 3A        :                
VCCIO3A                      : AE19      : power  :                   : 2.5V    : 3A        :                
GND                          : AE20      : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AE21      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AE22      :        :                   :         : 3A        :                
VCCIO3C                      : AE23      : power  :                   : 2.5V    : 3C        :                
VCCD_PLL_4                   : AE24      : power  :                   : 0.9V    :           :                
MSEL3                        : AE25      :        :                   :         : 3C        :                
GND                          : AE26      : gnd    :                   :         :           :                
GND                          : AE27      : gnd    :                   :         :           :                
GND                          : AE28      : gnd    :                   :         :           :                
GND                          : AE29      : gnd    :                   :         :           :                
GND                          : AE30      : gnd    :                   :         :           :                
rx_in                        : AE31      : input  : 1.5-V PCML        :         : QL0       : Y              
rx_in(n)                     : AE32      : input  : 1.5-V PCML        :         : QL0       : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : AF1       :        :                   :         : 5A        :                
GND                          : AF2       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AF3       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AF4       :        :                   :         : 5A        :                
GND                          : AF5       : gnd    :                   :         :           :                
GND                          : AF6       : gnd    :                   :         :           :                
GND                          : AF7       : gnd    :                   :         :           :                
VCCIO4A                      : AF8       : power  :                   : 2.5V    : 4A        :                
GND                          : AF9       : gnd    :                   :         :           :                
GND                          : AF10      : gnd    :                   :         :           :                
VCCIO4A                      : AF11      : power  :                   : 2.5V    : 4A        :                
GND                          : AF12      : gnd    :                   :         :           :                
GND                          : AF13      : gnd    :                   :         :           :                
VCCIO4A                      : AF14      : power  :                   : 2.5V    : 4A        :                
GND                          : AF15      : gnd    :                   :         :           :                
GND                          : AF16      : gnd    :                   :         :           :                
VCCIO3A                      : AF17      : power  :                   : 2.5V    : 3A        :                
GND                          : AF18      : gnd    :                   :         :           :                
GND                          : AF19      : gnd    :                   :         :           :                
VCCIO3A                      : AF20      : power  :                   : 2.5V    : 3A        :                
GND                          : AF21      : gnd    :                   :         :           :                
GND                          : AF22      : gnd    :                   :         :           :                
GND                          : AF23      : gnd    :                   :         :           :                
VCCIO3C                      : AF24      : power  :                   : 2.5V    : 3C        :                
GND                          : AF25      : gnd    :                   :         :           :                
GND                          : AF26      : gnd    :                   :         :           :                
GND                          : AF27      : gnd    :                   :         :           :                
GND                          : AF28      : gnd    :                   :         :           :                
nCONFIG                      : AF29      :        :                   :         : 3C        :                
GND                          : AF30      : gnd    :                   :         :           :                
GND                          : AF31      : gnd    :                   :         :           :                
GND                          : AF32      : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AG1       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AG2       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AG3       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AG4       :        :                   :         : 5A        :                
VCCIO5A                      : AG5       : power  :                   : 2.5V    : 5A        :                
GND                          : AG6       : gnd    :                   :         :           :                
GND                          : AG7       : gnd    :                   :         :           :                
GND                          : AG8       : gnd    :                   :         :           :                
GND                          : AG9       : gnd    :                   :         :           :                
GND                          : AG10      : gnd    :                   :         :           :                
GND                          : AG11      : gnd    :                   :         :           :                
GND                          : AG12      : gnd    :                   :         :           :                
GND                          : AG13      : gnd    :                   :         :           :                
GND                          : AG14      : gnd    :                   :         :           :                
GND                          : AG15      : gnd    :                   :         :           :                
GND                          : AG16      : gnd    :                   :         :           :                
GND                          : AG17      : gnd    :                   :         :           :                
GND                          : AG18      : gnd    :                   :         :           :                
GND                          : AG19      : gnd    :                   :         :           :                
GND                          : AG20      : gnd    :                   :         :           :                
GND                          : AG21      : gnd    :                   :         :           :                
GND                          : AG22      : gnd    :                   :         :           :                
GND                          : AG23      : gnd    :                   :         :           :                
GND                          : AG24      : gnd    :                   :         :           :                
GND                          : AG25      : gnd    :                   :         :           :                
GND                          : AG26      : gnd    :                   :         :           :                
GND                          : AG27      : gnd    :                   :         :           :                
GND                          : AG28      : gnd    :                   :         :           :                
nSTATUS                      : AG29      :        :                   :         : 3C        :                
NC                           : AG30      :        :                   :         :           :                
GND                          : AG31      : gnd    :                   :         :           :                
RREF                         : AG32      :        :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AH1       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AH2       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AH3       :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AH4       :        :                   :         : 5A        :                
GND                          : AH5       : gnd    :                   :         :           :                
VCCIO4A                      : AH6       : power  :                   : 2.5V    : 4A        :                
GND                          : AH7       : gnd    :                   :         :           :                
GND                          : AH8       : gnd    :                   :         :           :                
VCCIO4A                      : AH9       : power  :                   : 2.5V    : 4A        :                
GND                          : AH10      : gnd    :                   :         :           :                
GND                          : AH11      : gnd    :                   :         :           :                
VCCIO4A                      : AH12      : power  :                   : 2.5V    : 4A        :                
GND                          : AH13      : gnd    :                   :         :           :                
GND                          : AH14      : gnd    :                   :         :           :                
GND                          : AH15      : gnd    :                   :         :           :                
GND                          : AH16      : gnd    :                   :         :           :                
GND                          : AH17      : gnd    :                   :         :           :                
VCCIO3A                      : AH18      : power  :                   : 2.5V    : 3A        :                
GND                          : AH19      : gnd    :                   :         :           :                
GND                          : AH20      : gnd    :                   :         :           :                
VCCIO3A                      : AH21      : power  :                   : 2.5V    : 3A        :                
GND                          : AH22      : gnd    :                   :         :           :                
GND                          : AH23      : gnd    :                   :         :           :                
VCCIO3A                      : AH24      : power  :                   : 2.5V    : 3A        :                
GND                          : AH25      : gnd    :                   :         :           :                
GND                          : AH26      : gnd    :                   :         :           :                
VCCIO3C                      : AH27      : power  :                   : 2.5V    : 3C        :                
GND                          : AH28      : gnd    :                   :         :           :                
nCE                          : AH29      :        :                   :         : 3C        :                
NC                           : AH30      :        :                   :         :           :                
GND                          : AH31      : gnd    :                   :         :           :                
GND                          : AH32      : gnd    :                   :         :           :                
GND                          : AJ1       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AJ2       :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AJ3       :        :                   :         : 4A        :                
GND                          : AJ4       : gnd    :                   :         :           :                
hsmc_rxp[11]                 : AJ5       : bidir  : 2.5 V             :         : 4A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : AJ6       :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AJ7       :        :                   :         : 4A        :                
hsmc_rxp[12]                 : AJ8       : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_rxp[10]                 : AJ9       : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_rxp[13]                 : AJ10      : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_rxp[15]                 : AJ11      : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_rxp[14]                 : AJ12      : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_rxp[16]                 : AJ13      : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_txp[16]                 : AJ14      : bidir  : 2.5 V             :         : 4A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : AJ15      :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AJ16      :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AJ17      :        :                   :         : 4A        :                
hsmc_clkin0                  : AJ18      : input  : 2.5 V             :         : 4A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : AJ19      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AJ20      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AJ21      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AJ22      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AJ23      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AJ24      :        :                   :         : 3A        :                
~ALTERA_nCEO~ / RESERVED_OUTPUT_OPEN_DRAIN : AJ25      : output : 2.5 V             :         : 3A        : N              
RESERVED_INPUT_WITH_WEAK_PULLUP : AJ26      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AJ27      :        :                   :         : 3A        :                
GND                          : AJ28      : gnd    :                   :         :           :                
MSEL2                        : AJ29      :        :                   :         : 3C        :                
CONF_DONE                    : AJ30      :        :                   :         : 3C        :                
GND                          : AJ31      : gnd    :                   :         :           :                
GND                          : AJ32      : gnd    :                   :         :           :                
GND                          : AK1       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AK2       :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AK3       :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AK4       :        :                   :         : 4A        :                
hsmc_rxn[11]                 : AK5       : bidir  : 2.5 V             :         : 4A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : AK6       :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AK7       :        :                   :         : 4A        :                
hsmc_rxn[12]                 : AK8       : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_rxn[10]                 : AK9       : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_rxn[13]                 : AK10      : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_rxn[15]                 : AK11      : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_rxn[14]                 : AK12      : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_rxn[16]                 : AK13      : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_txn[16]                 : AK14      : bidir  : 2.5 V             :         : 4A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : AK15      :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AK16      :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AK17      :        :                   :         : 4A        :                
GND+                         : AK18      :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AK19      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AK20      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AK21      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AK22      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AK23      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AK24      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AK25      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AK26      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AK27      :        :                   :         : 3A        :                
GND                          : AK28      : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AK29      :        :                   :         : 3A        :                
MSEL0                        : AK30      :        :                   :         : 3C        :                
MSEL1                        : AK31      :        :                   :         : 3C        :                
GND                          : AK32      : gnd    :                   :         :           :                
GND                          : AL1       : gnd    :                   :         :           :                
GND                          : AL2       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AL3       :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AL4       :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AL5       :        :                   :         : 4A        :                
GND                          : AL6       : gnd    :                   :         :           :                
hsmc_txp[11]                 : AL7       : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_txp[10]                 : AL8       : bidir  : 2.5 V             :         : 4A        : Y              
GND                          : AL9       : gnd    :                   :         :           :                
hsmc_txp[12]                 : AL10      : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_txn[12]                 : AL11      : bidir  : 2.5 V             :         : 4A        : Y              
GND                          : AL12      : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AL13      :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AL14      :        :                   :         : 4A        :                
GND                          : AL15      : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AL16      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AL17      :        :                   :         : 3A        :                
GND                          : AL18      : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AL19      :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AL20      :        :                   :         : 3A        :                
GND                          : AL21      : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AL22      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AL23      :        :                   :         : 3A        :                
GND                          : AL24      : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AL25      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AL26      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AL27      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AL28      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AL29      :        :                   :         : 3A        :                
nIO_PULLUP                   : AL30      :        :                   :         : 3C        :                
GND                          : AL31      : gnd    :                   :         :           :                
GND                          : AL32      : gnd    :                   :         :           :                
GND                          : AM2       : gnd    :                   :         :           :                
GND                          : AM3       : gnd    :                   :         :           :                
GND                          : AM4       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AM5       :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AM6       :        :                   :         : 4A        :                
hsmc_txn[11]                 : AM7       : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_txn[10]                 : AM8       : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_rxp[9]                  : AM9       : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_rxn[9]                  : AM10      : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_txp[14]                 : AM11      : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_txn[14]                 : AM12      : bidir  : 2.5 V             :         : 4A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : AM13      :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AM14      :        :                   :         : 4A        :                
hsmc_rxp[8]                  : AM15      : bidir  : 2.5 V             :         : 4A        : Y              
hsmc_rxn[8]                  : AM16      : bidir  : 2.5 V             :         : 4A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : AM17      :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AM18      :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AM19      :        :                   :         : 4A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AM20      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AM21      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AM22      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AM23      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AM24      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AM25      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AM26      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AM27      :        :                   :         : 3A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : AM28      :        :                   :         : 3A        :                
GND                          : AM29      : gnd    :                   :         :           :                
GND                          : AM30      : gnd    :                   :         :           :                
GND                          : AM31      : gnd    :                   :         :           :                
GND                          : B1        : gnd    :                   :         :           :                
GND                          : B2        : gnd    :                   :         :           :                
GND                          : B3        : gnd    :                   :         :           :                
hsmc_rxn[3]                  : B4        : bidir  : 2.5 V             :         : 7A        : Y              
hsmc_rxp[3]                  : B5        : bidir  : 2.5 V             :         : 7A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : B6        :        :                   :         : 7A        :                
GND                          : B7        : gnd    :                   :         :           :                
hsmc_txn[3]                  : B8        : bidir  : 2.5 V             :         : 7A        : Y              
hsmc_txn[1]                  : B9        : bidir  : 2.5 V             :         : 7A        : Y              
GND                          : B10       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : B11       :        :                   :         : 7A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : B12       :        :                   :         : 7A        :                
GND                          : B13       : gnd    :                   :         :           :                
hsmc_txn[7]                  : B14       : bidir  : 2.5 V             :         : 7A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : B15       :        :                   :         : 7A        :                
GND                          : B16       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : B17       :        :                   :         : 7A        :                
hsmc_d1_3n                   : B18       : bidir  : 2.5 V             :         : 7A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : B19       :        :                   :         : 7A        :                
GND                          : B20       : gnd    :                   :         :           :                
lpc_ad[2]                    : B21       : input  : 3.3-V LVCMOS      :         : 8A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : B22       :        :                   :         : 8A        :                
GND                          : B23       : gnd    :                   :         :           :                
gpio_rxn[7]                  : B24       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_rxn[5]                  : B25       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
GND                          : B26       : gnd    :                   :         :           :                
gpio_rxn[2]                  : B27       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
TDO                          : B28       : output :                   :         : 8C        :                
ASDO                         : B29       :        :                   :         : 8C        :                
TCK                          : B30       : input  :                   :         : 8C        :                
GND                          : B31       : gnd    :                   :         :           :                
GND                          : B32       : gnd    :                   :         :           :                
GND                          : C1        : gnd    :                   :         :           :                
GND                          : C2        : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : C3        :        :                   :         : 7A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : C4        :        :                   :         : 7A        :                
hsmc_rxn[2]                  : C5        : bidir  : 2.5 V             :         : 7A        : Y              
hsmc_txn[2]                  : C6        : bidir  : 2.5 V             :         : 7A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : C7        :        :                   :         : 7A        :                
hsmc_txp[3]                  : C8        : bidir  : 2.5 V             :         : 7A        : Y              
hsmc_txp[1]                  : C9        : bidir  : 2.5 V             :         : 7A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : C10       :        :                   :         : 7A        :                
hsmc_rxn[1]                  : C11       : bidir  : 2.5 V             :         : 7A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : C12       :        :                   :         : 7A        :                
hsmc_txp[7]                  : C13       : bidir  : 2.5 V             :         : 7A        : Y              
hsmc_rxp[7]                  : C14       : bidir  : 2.5 V             :         : 7A        : Y              
hsmc_rxp[0]                  : C15       : bidir  : 2.5 V             :         : 7A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : C16       :        :                   :         : 7A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : C17       :        :                   :         : 7A        :                
hsmc_d1_3p                   : C18       : bidir  : 2.5 V             :         : 7A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : C19       :        :                   :         : 7A        :                
lpc_ad[1]                    : C20       : input  : 3.3-V LVCMOS      :         : 8A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : C21       :        :                   :         : 8A        :                
gpio_txn[7]                  : C22       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_txn[6]                  : C23       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_rxp[7]                  : C24       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_rxp[5]                  : C25       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_txn[1]                  : C26       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_rxp[2]                  : C27       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
nCSO                         : C28       :        :                   :         : 8C        :                
DATA0                        : C29       : input  :                   :         : 8C        :                
DCLK                         : C30       : bidir  :                   :         : 8C        :                
GND                          : C31       : gnd    :                   :         :           :                
GND                          : C32       : gnd    :                   :         :           :                
GND                          : D1        : gnd    :                   :         :           :                
DNU                          : D2        :        :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : D3        :        :                   :         : 7A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : D4        :        :                   :         : 7A        :                
hsmc_rxp[2]                  : D5        : bidir  : 2.5 V             :         : 7A        : Y              
hsmc_txp[2]                  : D6        : bidir  : 2.5 V             :         : 7A        : Y              
hsmc_txn[4]                  : D7        : bidir  : 2.5 V             :         : 7A        : Y              
hsmc_txp[4]                  : D8        : bidir  : 2.5 V             :         : 7A        : Y              
hsmc_txn[6]                  : D9        : bidir  : 2.5 V             :         : 7A        : Y              
hsmc_txp[6]                  : D10       : bidir  : 2.5 V             :         : 7A        : Y              
hsmc_rxp[1]                  : D11       : bidir  : 2.5 V             :         : 7A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : D12       :        :                   :         : 7A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : D13       :        :                   :         : 7A        :                
hsmc_rxn[7]                  : D14       : bidir  : 2.5 V             :         : 7A        : Y              
hsmc_rxn[0]                  : D15       : bidir  : 2.5 V             :         : 7A        : Y              
GND+                         : D16       :        :                   :         : 8A        :                
lpc_clk                      : D17       : input  : 3.3-V LVCMOS      :         : 8A        : Y              
gpio_txn[8]                  : D18       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_txp[8]                  : D19       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
lpc_ad[0]                    : D20       : input  : 3.3-V LVCMOS      :         : 8A        : Y              
lpc_frame_n                  : D21       : input  : 3.3-V LVCMOS      :         : 8A        : Y              
gpio_txp[7]                  : D22       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_txp[6]                  : D23       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_rxn[6]                  : D24       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_rxp[6]                  : D25       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_txp[1]                  : D26       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : D27       :        :                   :         : 8A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : D28       :        :                   :         : 8A        :                
TMS                          : D29       : input  :                   :         : 8C        :                
TDI                          : D30       : input  :                   :         : 8C        :                
GND                          : D31       : gnd    :                   :         :           :                
GND                          : D32       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : E1        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : E2        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : E3        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : E4        :        :                   :         : 6A        :                
GND                          : E5        : gnd    :                   :         :           :                
VCCIO7A                      : E6        : power  :                   : 2.5V    : 7A        :                
GND                          : E7        : gnd    :                   :         :           :                
GND                          : E8        : gnd    :                   :         :           :                
VCCIO7A                      : E9        : power  :                   : 2.5V    : 7A        :                
GND                          : E10       : gnd    :                   :         :           :                
GND                          : E11       : gnd    :                   :         :           :                
VCCIO7A                      : E12       : power  :                   : 2.5V    : 7A        :                
GND                          : E13       : gnd    :                   :         :           :                
GND                          : E14       : gnd    :                   :         :           :                
GND                          : E15       : gnd    :                   :         :           :                
GND                          : E16       : gnd    :                   :         :           :                
GND                          : E17       : gnd    :                   :         :           :                
VCCIO8A                      : E18       : power  :                   : 3.3V    : 8A        :                
GND                          : E19       : gnd    :                   :         :           :                
GND                          : E20       : gnd    :                   :         :           :                
VCCIO8A                      : E21       : power  :                   : 3.3V    : 8A        :                
GND                          : E22       : gnd    :                   :         :           :                
GND                          : E23       : gnd    :                   :         :           :                
VCCIO8A                      : E24       : power  :                   : 3.3V    : 8A        :                
GND                          : E25       : gnd    :                   :         :           :                
GND                          : E26       : gnd    :                   :         :           :                
VCCIO8C                      : E27       : power  :                   : 2.5V    : 8C        :                
GND                          : E28       : gnd    :                   :         :           :                
GND                          : E29       : gnd    :                   :         :           :                
GND                          : E30       : gnd    :                   :         :           :                
GND                          : E31       : gnd    :                   :         :           :                
VCCBAT                       : E32       : power  :                   : 2.5V    :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : F1        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : F2        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : F3        :        :                   :         : 6A        :                
arria_rst_n                  : F4        : input  : 3.3-V LVCMOS      :         : 6A        : Y              
VCCIO6A                      : F5        : power  :                   : 3.3V    : 6A        :                
GND                          : F6        : gnd    :                   :         :           :                
GND                          : F7        : gnd    :                   :         :           :                
GND                          : F8        : gnd    :                   :         :           :                
GND                          : F9        : gnd    :                   :         :           :                
GND                          : F10       : gnd    :                   :         :           :                
GND                          : F11       : gnd    :                   :         :           :                
GND                          : F12       : gnd    :                   :         :           :                
GND                          : F13       : gnd    :                   :         :           :                
GND                          : F14       : gnd    :                   :         :           :                
GND                          : F15       : gnd    :                   :         :           :                
GND                          : F16       : gnd    :                   :         :           :                
GND                          : F17       : gnd    :                   :         :           :                
GND                          : F18       : gnd    :                   :         :           :                
GND                          : F19       : gnd    :                   :         :           :                
GND                          : F20       : gnd    :                   :         :           :                
GND                          : F21       : gnd    :                   :         :           :                
GND                          : F22       : gnd    :                   :         :           :                
GND                          : F23       : gnd    :                   :         :           :                
GND                          : F24       : gnd    :                   :         :           :                
GND                          : F25       : gnd    :                   :         :           :                
GND                          : F26       : gnd    :                   :         :           :                
GND                          : F27       : gnd    :                   :         :           :                
GND                          : F28       : gnd    :                   :         :           :                
GXB_NC                       : F29       :        :                   :         : QL1       :                
GXB_NC                       : F30       :        :                   :         : QL1       :                
GND                          : F31       : gnd    :                   :         :           :                
GND                          : F32       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : G1        :        :                   :         : 6A        :                
GND                          : G2        : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : G3        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : G4        :        :                   :         : 6A        :                
GND                          : G5        : gnd    :                   :         :           :                
GND                          : G6        : gnd    :                   :         :           :                
GND                          : G7        : gnd    :                   :         :           :                
VCCIO7A                      : G8        : power  :                   : 2.5V    : 7A        :                
GND                          : G9        : gnd    :                   :         :           :                
GND                          : G10       : gnd    :                   :         :           :                
VCCIO7A                      : G11       : power  :                   : 2.5V    : 7A        :                
GND                          : G12       : gnd    :                   :         :           :                
GND                          : G13       : gnd    :                   :         :           :                
VCCIO7A                      : G14       : power  :                   : 2.5V    : 7A        :                
GND                          : G15       : gnd    :                   :         :           :                
GND                          : G16       : gnd    :                   :         :           :                
VCCIO7A                      : G17       : power  :                   : 2.5V    : 7A        :                
GND                          : G18       : gnd    :                   :         :           :                
GND                          : G19       : gnd    :                   :         :           :                
VCCIO8A                      : G20       : power  :                   : 3.3V    : 8A        :                
GND                          : G21       : gnd    :                   :         :           :                
VCCIO8A                      : G22       : power  :                   : 3.3V    : 8A        :                
GND                          : G23       : gnd    :                   :         :           :                
VCCIO8C                      : G24       : power  :                   : 2.5V    : 8C        :                
GND                          : G25       : gnd    :                   :         :           :                
GND                          : G26       : gnd    :                   :         :           :                
GND                          : G27       : gnd    :                   :         :           :                
GND                          : G28       : gnd    :                   :         :           :                
GND                          : G29       : gnd    :                   :         :           :                
GND                          : G30       : gnd    :                   :         :           :                
GXB_GND*                     : G31       :        :                   :         : QL1       :                
GXB_GND*                     : G32       :        :                   :         : QL1       :                
RESERVED_INPUT_WITH_WEAK_PULLUP : H1        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : H2        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : H3        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : H4        :        :                   :         : 6A        :                
GND                          : H5        : gnd    :                   :         :           :                
GND                          : H6        : gnd    :                   :         :           :                
VCCIO6A                      : H7        : power  :                   : 3.3V    : 6A        :                
GND                          : H8        : gnd    :                   :         :           :                
VCCA_PLL_2                   : H9        : power  :                   : 2.5V    :           :                
VCCIO7A                      : H10       : power  :                   : 2.5V    : 7A        :                
GND                          : H11       : gnd    :                   :         :           :                
hsmc_txn[0]                  : H12       : bidir  : 2.5 V             :         : 7A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : H13       :        :                   :         : 7A        :                
GND                          : H14       : gnd    :                   :         :           :                
VCCIO7A                      : H15       : power  :                   : 2.5V    : 7A        :                
gpio_txn[4]                  : H16       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
GND                          : H17       : gnd    :                   :         :           :                
gpio_txn[2]                  : H18       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
VCCIO8A                      : H19       : power  :                   : 3.3V    : 8A        :                
GND                          : H20       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : H21       :        :                   :         : 8A        :                
VCCIO8A                      : H22       : power  :                   : 3.3V    : 8A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : H23       :        :                   :         : 8A        :                
VCCD_PLL_1                   : H24       : power  :                   : 0.9V    :           :                
VCCIO8C                      : H25       : power  :                   : 2.5V    : 8C        :                
GND                          : H26       : gnd    :                   :         :           :                
GND                          : H27       : gnd    :                   :         :           :                
GND                          : H28       : gnd    :                   :         :           :                
GXB_NC                       : H29       :        :                   :         : QL1       :                
GXB_NC                       : H30       :        :                   :         : QL1       :                
GND                          : H31       : gnd    :                   :         :           :                
GND                          : H32       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : J1        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : J2        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : J3        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : J4        :        :                   :         : 6A        :                
VCCIO6A                      : J5        : power  :                   : 3.3V    : 6A        :                
GND                          : J6        : gnd    :                   :         :           :                
GND                          : J7        : gnd    :                   :         :           :                
VCCD_PLL_2                   : J8        : power  :                   : 0.9V    :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : J9        :        :                   :         : 6A        :                
VCCIO7A                      : J10       : power  :                   : 2.5V    : 7A        :                
hsmc_txp[0]                  : J11       : bidir  : 2.5 V             :         : 7A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : J12       :        :                   :         : 7A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : J13       :        :                   :         : 7A        :                
GND+                         : J14       :        :                   :         : 7A        :                
VCCIO7A                      : J15       : power  :                   : 2.5V    : 7A        :                
gpio_txn[5]                  : J16       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_txp[4]                  : J17       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_txp[2]                  : J18       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
VCCIO8A                      : J19       : power  :                   : 3.3V    : 8A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : J20       :        :                   :         : 8A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : J21       :        :                   :         : 8A        :                
VCCIO8A                      : J22       : power  :                   : 3.3V    : 8A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : J23       :        :                   :         : 8A        :                
DNU                          : J24       :        :                   :         :           :                
VCCA_PLL_1                   : J25       : power  :                   : 2.5V    :           :                
GND                          : J26       : gnd    :                   :         :           :                
GND                          : J27       : gnd    :                   :         :           :                
GND                          : J28       : gnd    :                   :         :           :                
GND                          : J29       : gnd    :                   :         :           :                
GND                          : J30       : gnd    :                   :         :           :                
GXB_GND*                     : J31       :        :                   :         : QL1       :                
GXB_GND*                     : J32       :        :                   :         : QL1       :                
RESERVED_INPUT_WITH_WEAK_PULLUP : K1        :        :                   :         : 6A        :                
GND                          : K2        : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : K3        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : K4        :        :                   :         : 6A        :                
GND                          : K5        : gnd    :                   :         :           :                
GND                          : K6        : gnd    :                   :         :           :                
VCCIO6A                      : K7        : power  :                   : 3.3V    : 6A        :                
GND                          : K8        : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : K9        :        :                   :         : 6A        :                
hsmc_txn[5]                  : K10       : bidir  : 2.5 V             :         : 7A        : Y              
hsmc_txp[5]                  : K11       : bidir  : 2.5 V             :         : 7A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : K12       :        :                   :         : 7A        :                
GND+                         : K13       :        :                   :         : 7A        :                
VREFB7AN0                    : K14       : power  :                   :         : 7A        :                
VCCCB                        : K15       : power  :                   : 1.5V    :           :                
gpio_txp[5]                  : K16       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_txn[3]                  : K17       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_txp[3]                  : K18       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : K19       :        :                   :         : 8A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : K20       :        :                   :         : 8A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : K21       :        :                   :         : 8A        :                
gpio_clkoutn                 : K22       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_clkoutp                 : K23       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_rxp[1]                  : K24       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
gpio_rxn[1]                  : K25       : bidir  : 3.3-V LVTTL       :         : 8A        : Y              
GND                          : K26       : gnd    :                   :         :           :                
GND                          : K27       : gnd    :                   :         :           :                
GND                          : K28       : gnd    :                   :         :           :                
GXB_GND*                     : K29       :        :                   :         : QL1       :                
GXB_GND*                     : K30       :        :                   :         : QL1       :                
GND                          : K31       : gnd    :                   :         :           :                
GND                          : K32       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : L1        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : L2        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : L3        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : L4        :        :                   :         : 6A        :                
GND                          : L5        : gnd    :                   :         :           :                
GND                          : L6        : gnd    :                   :         :           :                
GND                          : L7        : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : L8        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : L9        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : L10       :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : L11       :        :                   :         : 7A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : L12       :        :                   :         : 7A        :                
GND                          : L13       : gnd    :                   :         :           :                
VCCPD7A                      : L14       : power  :                   : 2.5V    : 7A        :                
VCCPD7A                      : L15       : power  :                   : 2.5V    : 7A        :                
GND                          : L16       : gnd    :                   :         :           :                
GND                          : L17       : gnd    :                   :         :           :                
VCCPD8A                      : L18       : power  :                   : 3.3V    : 8A        :                
VCCPD8A                      : L19       : power  :                   : 3.3V    : 8A        :                
GND                          : L20       : gnd    :                   :         :           :                
VCCPD8C                      : L21       : power  :                   : 2.5V    : 8C        :                
GND                          : L22       : gnd    :                   :         :           :                
VREFB8AN0                    : L23       : power  :                   :         : 8A        :                
GND                          : L24       : gnd    :                   :         :           :                
GND                          : L25       : gnd    :                   :         :           :                
VCCL_GXB                     : L26       : power  :                   : 1.1V    :           :                
GND                          : L27       : gnd    :                   :         :           :                
GND                          : L28       : gnd    :                   :         :           :                
GND                          : L29       : gnd    :                   :         :           :                
GND                          : L30       : gnd    :                   :         :           :                
GXB_GND*                     : L31       :        :                   :         : QL1       :                
GXB_GND*                     : L32       :        :                   :         : QL1       :                
RESERVED_INPUT_WITH_WEAK_PULLUP : M1        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : M2        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : M3        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : M4        :        :                   :         : 6A        :                
VCCIO6A                      : M5        : power  :                   : 3.3V    : 6A        :                
GND                          : M6        : gnd    :                   :         :           :                
GND                          : M7        : gnd    :                   :         :           :                
VCCIO6A                      : M8        : power  :                   : 3.3V    : 6A        :                
VCCIO6A                      : M9        : power  :                   : 3.3V    : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : M10       :        :                   :         : 6A        :                
GND                          : M11       : gnd    :                   :         :           :                
GND                          : M12       : gnd    :                   :         :           :                
GND                          : M13       : gnd    :                   :         :           :                
VCC                          : M14       : power  :                   : 0.9V    :           :                
GND                          : M15       : gnd    :                   :         :           :                
VCC                          : M16       : power  :                   : 0.9V    :           :                
GND                          : M17       : gnd    :                   :         :           :                
VCC                          : M18       : power  :                   : 0.9V    :           :                
GND                          : M19       : gnd    :                   :         :           :                
VCC                          : M20       : power  :                   : 0.9V    :           :                
GND                          : M21       : gnd    :                   :         :           :                
VCC                          : M22       : power  :                   : 0.9V    :           :                
GND                          : M23       : gnd    :                   :         :           :                
GND                          : M24       : gnd    :                   :         :           :                
VCCL_GXB                     : M25       : power  :                   : 1.1V    :           :                
GND                          : M26       : gnd    :                   :         :           :                
VCCL_GXB                     : M27       : power  :                   : 1.1V    :           :                
GND                          : M28       : gnd    :                   :         :           :                
GXB_NC                       : M29       :        :                   :         : QL1       :                
GXB_NC                       : M30       :        :                   :         : QL1       :                
GND                          : M31       : gnd    :                   :         :           :                
GND                          : M32       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : N1        :        :                   :         : 6A        :                
GND                          : N2        : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : N3        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : N4        :        :                   :         : 6A        :                
GND                          : N5        : gnd    :                   :         :           :                
GND                          : N6        : gnd    :                   :         :           :                
VCCIO6A                      : N7        : power  :                   : 3.3V    : 6A        :                
GND                          : N8        : gnd    :                   :         :           :                
VCCIO6A                      : N9        : power  :                   : 3.3V    : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : N10       :        :                   :         : 6A        :                
VCCPD6A                      : N11       : power  :                   : 3.3V    : 6A        :                
GND                          : N12       : gnd    :                   :         :           :                
VCC                          : N13       : power  :                   : 0.9V    :           :                
GND                          : N14       : gnd    :                   :         :           :                
VCC                          : N15       : power  :                   : 0.9V    :           :                
GND                          : N16       : gnd    :                   :         :           :                
VCC                          : N17       : power  :                   : 0.9V    :           :                
GND                          : N18       : gnd    :                   :         :           :                
VCC                          : N19       : power  :                   : 0.9V    :           :                
GND                          : N20       : gnd    :                   :         :           :                
VCC                          : N21       : power  :                   : 0.9V    :           :                
GND                          : N22       : gnd    :                   :         :           :                
GND                          : N23       : gnd    :                   :         :           :                
VCCA                         : N24       : power  :                   : 2.5V    :           :                
GND                          : N25       : gnd    :                   :         :           :                
VCCL_GXB                     : N26       : power  :                   : 1.1V    :           :                
GND                          : N27       : gnd    :                   :         :           :                
GND                          : N28       : gnd    :                   :         :           :                
GND                          : N29       : gnd    :                   :         :           :                
GND                          : N30       : gnd    :                   :         :           :                
GXB_GND*                     : N31       :        :                   :         : QL1       :                
GXB_GND*                     : N32       :        :                   :         : QL1       :                
RESERVED_INPUT_WITH_WEAK_PULLUP : P1        :        :                   :         : 6A        :                
GND+                         : P2        :        :                   :         : 6A        :                
GND+                         : P3        :        :                   :         : 6A        :                
gpio_reserved[1]             : P4        : output : 3.3-V LVTTL       :         : 6A        : Y              
GND                          : P5        : gnd    :                   :         :           :                
GND                          : P6        : gnd    :                   :         :           :                
GND                          : P7        : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : P8        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : P9        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : P10       :        :                   :         : 6A        :                
VCCPD6A                      : P11       : power  :                   : 3.3V    : 6A        :                
VCC                          : P12       : power  :                   : 0.9V    :           :                
GND                          : P13       : gnd    :                   :         :           :                
VCC                          : P14       : power  :                   : 0.9V    :           :                
GND                          : P15       : gnd    :                   :         :           :                
VCC                          : P16       : power  :                   : 0.9V    :           :                
GND                          : P17       : gnd    :                   :         :           :                
VCC                          : P18       : power  :                   : 0.9V    :           :                
GND                          : P19       : gnd    :                   :         :           :                
VCC                          : P20       : power  :                   : 0.9V    :           :                
GND                          : P21       : gnd    :                   :         :           :                
VCC                          : P22       : power  :                   : 0.9V    :           :                
VCCH_GXB                     : P23       : power  :                   : 1.5V    :           :                
GND                          : P24       : gnd    :                   :         :           :                
VCCL_GXB                     : P25       : power  :                   : 1.1V    :           :                
GND                          : P26       : gnd    :                   :         :           :                
VCCL_GXB                     : P27       : power  :                   : 1.1V    :           :                
GND                          : P28       : gnd    :                   :         :           :                
GXB_NC                       : P29       :        :                   :         : QL1       :                
GXB_NC                       : P30       :        :                   :         : QL1       :                
GND                          : P31       : gnd    :                   :         :           :                
GND                          : P32       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : R1        :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : R2        :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : R3        :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : R4        :        :                   :         : 6A        :                
VCCIO6A                      : R5        : power  :                   : 3.3V    : 6A        :                
GND                          : R6        : gnd    :                   :         :           :                
GND                          : R7        : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : R8        :        :                   :         : 6A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : R9        :        :                   :         : 6A        :                
hsmc_clkin1p                 : R10       : input  : 2.5 V             :         : 5A        : Y              
VREFB6AN0                    : R11       : power  :                   :         : 6A        :                
GND                          : R12       : gnd    :                   :         :           :                
VCC                          : R13       : power  :                   : 0.9V    :           :                
GND                          : R14       : gnd    :                   :         :           :                
VCC                          : R15       : power  :                   : 0.9V    :           :                
GND                          : R16       : gnd    :                   :         :           :                
VCC                          : R17       : power  :                   : 0.9V    :           :                
GND                          : R18       : gnd    :                   :         :           :                
VCC                          : R19       : power  :                   : 0.9V    :           :                
GND                          : R20       : gnd    :                   :         :           :                
VCC                          : R21       : power  :                   : 0.9V    :           :                
GND                          : R22       : gnd    :                   :         :           :                
VCCH_GXB                     : R23       : power  :                   : 1.5V    :           :                
GND                          : R24       : gnd    :                   :         :           :                
GND                          : R25       : gnd    :                   :         :           :                
VCCL_GXB                     : R26       : power  :                   : 1.1V    :           :                
GND                          : R27       : gnd    :                   :         :           :                
GND                          : R28       : gnd    :                   :         :           :                
GND                          : R29       : gnd    :                   :         :           :                
GND                          : R30       : gnd    :                   :         :           :                
GXB_GND*                     : R31       :        :                   :         : QL1       :                
GXB_GND*                     : R32       :        :                   :         : QL1       :                
RESERVED_INPUT_WITH_WEAK_PULLUP : T1        :        :                   :         : 5A        :                
GND                          : T2        : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : T3        :        :                   :         : 5A        :                
hsmc_clkout0                 : T4        : output : 2.5 V             :         : 5A        : Y              
GND                          : T5        : gnd    :                   :         :           :                
GND                          : T6        : gnd    :                   :         :           :                
VCCIO5A                      : T7        : power  :                   : 2.5V    : 5A        :                
GND                          : T8        : gnd    :                   :         :           :                
VCCIO5A                      : T9        : power  :                   : 2.5V    : 5A        :                
hsmc_clkin1n                 : T10       : input  : 2.5 V             :         : 5A        : Y              
GND                          : T11       : gnd    :                   :         :           :                
VCC                          : T12       : power  :                   : 0.9V    :           :                
GND                          : T13       : gnd    :                   :         :           :                
VCC                          : T14       : power  :                   : 0.9V    :           :                
GND                          : T15       : gnd    :                   :         :           :                
VCC                          : T16       : power  :                   : 0.9V    :           :                
GND                          : T17       : gnd    :                   :         :           :                
VCC                          : T18       : power  :                   : 0.9V    :           :                
GND                          : T19       : gnd    :                   :         :           :                
VCC                          : T20       : power  :                   : 0.9V    :           :                
GND                          : T21       : gnd    :                   :         :           :                
VCC                          : T22       : power  :                   : 0.9V    :           :                
GND                          : T23       : gnd    :                   :         :           :                
GND                          : T24       : gnd    :                   :         :           :                
VCCL_GXB                     : T25       : power  :                   : 1.1V    :           :                
GND                          : T26       : gnd    :                   :         :           :                
VCCL_GXB                     : T27       : power  :                   : 1.1V    :           :                
GND                          : T28       : gnd    :                   :         :           :                
GXB_NC                       : T29       :        :                   :         : QL0       :                
GXB_NC                       : T30       :        :                   :         : QL0       :                
GND                          : T31       : gnd    :                   :         :           :                
GND                          : T32       : gnd    :                   :         :           :                
smb_hsmc_dat                 : U1        : bidir  : 2.5 V             :         : 5A        : Y              
smb_hsmc_clk                 : U2        : bidir  : 2.5 V             :         : 5A        : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : U3        :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : U4        :        :                   :         : 5A        :                
GND                          : U5        : gnd    :                   :         :           :                
GND                          : U6        : gnd    :                   :         :           :                
GND                          : U7        : gnd    :                   :         :           :                
VCCIO5A                      : U8        : power  :                   : 2.5V    : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : U9        :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : U10       :        :                   :         : 5A        :                
VCCPD5A                      : U11       : power  :                   : 2.5V    : 5A        :                
GND                          : U12       : gnd    :                   :         :           :                
VCC                          : U13       : power  :                   : 0.9V    :           :                
GND                          : U14       : gnd    :                   :         :           :                
VCC                          : U15       : power  :                   : 0.9V    :           :                
DNU                          : U16       :        :                   :         :           :                
VCC                          : U17       : power  :                   : 0.9V    :           :                
GND                          : U18       : gnd    :                   :         :           :                
VCC                          : U19       : power  :                   : 0.9V    :           :                
GND                          : U20       : gnd    :                   :         :           :                
VCC                          : U21       : power  :                   : 0.9V    :           :                
GND                          : U22       : gnd    :                   :         :           :                
GND                          : U23       : gnd    :                   :         :           :                
GND                          : U24       : gnd    :                   :         :           :                
GND                          : U25       : gnd    :                   :         :           :                
VCCL_GXB                     : U26       : power  :                   : 1.1V    :           :                
GND                          : U27       : gnd    :                   :         :           :                
GND                          : U28       : gnd    :                   :         :           :                
GND                          : U29       : gnd    :                   :         :           :                
GND                          : U30       : gnd    :                   :         :           :                
GXB_GND*                     : U31       :        :                   :         : QL0       :                
GXB_GND*                     : U32       :        :                   :         : QL0       :                
RESERVED_INPUT_WITH_WEAK_PULLUP : V1        :        :                   :         : 5A        :                
GND                          : V2        : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : V3        :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : V4        :        :                   :         : 5A        :                
VCCIO5A                      : V5        : power  :                   : 2.5V    : 5A        :                
GND                          : V6        : gnd    :                   :         :           :                
GND                          : V7        : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : V8        :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : V9        :        :                   :         : 5A        :                
VCCCB                        : V10       : power  :                   : 1.5V    :           :                
VCCPD5A                      : V11       : power  :                   : 2.5V    : 5A        :                
VCC                          : V12       : power  :                   : 0.9V    :           :                
GND                          : V13       : gnd    :                   :         :           :                
VCC                          : V14       : power  :                   : 0.9V    :           :                
GND                          : V15       : gnd    :                   :         :           :                
VCC                          : V16       : power  :                   : 0.9V    :           :                
GND                          : V17       : gnd    :                   :         :           :                
VCC                          : V18       : power  :                   : 0.9V    :           :                
GND                          : V19       : gnd    :                   :         :           :                
VCC                          : V20       : power  :                   : 0.9V    :           :                
GND                          : V21       : gnd    :                   :         :           :                
VCC                          : V22       : power  :                   : 0.9V    :           :                
VCCH_GXB                     : V23       : power  :                   : 1.5V    :           :                
GND                          : V24       : gnd    :                   :         :           :                
VCCL_GXB                     : V25       : power  :                   : 1.1V    :           :                
GND                          : V26       : gnd    :                   :         :           :                
VCCL_GXB                     : V27       : power  :                   : 1.1V    :           :                
GND                          : V28       : gnd    :                   :         :           :                
GXB_NC                       : V29       :        :                   :         : QL0       :                
GXB_NC                       : V30       :        :                   :         : QL0       :                
GND                          : V31       : gnd    :                   :         :           :                
GND                          : V32       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : W1        :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : W2        :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : W3        :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : W4        :        :                   :         : 5A        :                
GND                          : W5        : gnd    :                   :         :           :                
GND                          : W6        : gnd    :                   :         :           :                
VCCIO5A                      : W7        : power  :                   : 2.5V    : 5A        :                
GND                          : W8        : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : W9        :        :                   :         : 5A        :                
VCCIO5A                      : W10       : power  :                   : 2.5V    : 5A        :                
GND                          : W11       : gnd    :                   :         :           :                
GND                          : W12       : gnd    :                   :         :           :                
VCC                          : W13       : power  :                   : 0.9V    :           :                
GND                          : W14       : gnd    :                   :         :           :                
VCC                          : W15       : power  :                   : 0.9V    :           :                
GND                          : W16       : gnd    :                   :         :           :                
VCC                          : W17       : power  :                   : 0.9V    :           :                
GND                          : W18       : gnd    :                   :         :           :                
VCC                          : W19       : power  :                   : 0.9V    :           :                
GND                          : W20       : gnd    :                   :         :           :                
VCC                          : W21       : power  :                   : 0.9V    :           :                
GND                          : W22       : gnd    :                   :         :           :                
VCCH_GXB                     : W23       : power  :                   : 1.5V    :           :                
GND                          : W24       : gnd    :                   :         :           :                
GND                          : W25       : gnd    :                   :         :           :                
VCCL_GXB                     : W26       : power  :                   : 1.1V    :           :                
GND                          : W27       : gnd    :                   :         :           :                
GND                          : W28       : gnd    :                   :         :           :                
GND                          : W29       : gnd    :                   :         :           :                
GND                          : W30       : gnd    :                   :         :           :                
GXB_GND*                     : W31       :        :                   :         : QL0       :                
GXB_GND*                     : W32       :        :                   :         : QL0       :                
RESERVED_INPUT_WITH_WEAK_PULLUP : Y1        :        :                   :         : 5A        :                
GND                          : Y2        : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : Y3        :        :                   :         : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : Y4        :        :                   :         : 5A        :                
GND                          : Y5        : gnd    :                   :         :           :                
GND                          : Y6        : gnd    :                   :         :           :                
GND                          : Y7        : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : Y8        :        :                   :         : 5A        :                
VCCIO5A                      : Y9        : power  :                   : 2.5V    : 5A        :                
RESERVED_INPUT_WITH_WEAK_PULLUP : Y10       :        :                   :         : 5A        :                
GND                          : Y11       : gnd    :                   :         :           :                
GND                          : Y12       : gnd    :                   :         :           :                
GND                          : Y13       : gnd    :                   :         :           :                
VCC                          : Y14       : power  :                   : 0.9V    :           :                
GND                          : Y15       : gnd    :                   :         :           :                
VCC                          : Y16       : power  :                   : 0.9V    :           :                
GND                          : Y17       : gnd    :                   :         :           :                
VCC                          : Y18       : power  :                   : 0.9V    :           :                
GND                          : Y19       : gnd    :                   :         :           :                
VCC                          : Y20       : power  :                   : 0.9V    :           :                
GND                          : Y21       : gnd    :                   :         :           :                
VCC                          : Y22       : power  :                   : 0.9V    :           :                
GND                          : Y23       : gnd    :                   :         :           :                
GND                          : Y24       : gnd    :                   :         :           :                
VCCL_GXB                     : Y25       : power  :                   : 1.1V    :           :                
GND                          : Y26       : gnd    :                   :         :           :                
VCCL_GXB                     : Y27       : power  :                   : 1.1V    :           :                
GND                          : Y28       : gnd    :                   :         :           :                
GXB_GND*                     : Y29       :        :                   :         : QL0       :                
GXB_GND*                     : Y30       :        :                   :         : QL0       :                
GND                          : Y31       : gnd    :                   :         :           :                
GND                          : Y32       : gnd    :                   :         :           :                
