# -------------------------------------------------------------------------- #
#
# Copyright (C) 1991-2011 Altera Corporation
# Your use of Altera Corporation's design tools, logic functions 
# and other software and tools, and its AMPP partner logic 
# functions, and any output files from any of the foregoing 
# (including device programming or simulation files), and any 
# associated documentation or information are expressly subject 
# to the terms and conditions of the Altera Program License 
# Subscription Agreement, Altera MegaCore Function License 
# Agreement, or other applicable license agreement, including, 
# without limitation, that your use is for the sole purpose of 
# programming logic devices manufactured by Altera and sold by 
# Altera or its authorized distributors.  Please refer to the 
# applicable agreement for further details.
#
# -------------------------------------------------------------------------- #
#
# Quartus II 64-Bit
# Version 10.1 Build 197 01/19/2011 Service Pack 1 SJ Full Version
# Date created = 09:47:18  February 25, 2011
#
# -------------------------------------------------------------------------- #
#
# Notes:
#
# 1) The default values for assignments are stored in the file:
#		msmst_test_assignment_defaults.qdf
#    If this file doesn't exist, see file:
#		assignment_defaults.qdf
#
# 2) Altera recommends that you do not modify this file. This
#    file is updated automatically by the Quartus II software
#    and any changes you make may be lost or overwritten.
#
# -------------------------------------------------------------------------- #


set_global_assignment -name FAMILY "Arria II GX"
set_global_assignment -name DEVICE EP2AGXE6XXFPGA
set_global_assignment -name TOP_LEVEL_ENTITY msmst_test_top
set_global_assignment -name ORIGINAL_QUARTUS_VERSION "10.1 SP1"
set_global_assignment -name PROJECT_CREATION_TIME_DATE "09:47:18  FEBRUARY 25, 2011"
set_global_assignment -name LAST_QUARTUS_VERSION "10.1 SP1"
set_global_assignment -name MIN_CORE_JUNCTION_TEMP "-40"
set_global_assignment -name MAX_CORE_JUNCTION_TEMP 100
set_global_assignment -name DEVICE_FILTER_PACKAGE MBGA
set_global_assignment -name ERROR_CHECK_FREQUENCY_DIVISOR 2
set_global_assignment -name PARTITION_NETLIST_TYPE SOURCE -section_id Top
set_global_assignment -name PARTITION_FITTER_PRESERVATION_LEVEL PLACEMENT_AND_ROUTING -section_id Top
set_global_assignment -name PARTITION_COLOR 16764057 -section_id Top
set_global_assignment -name STRATIX_DEVICE_IO_STANDARD "2.5 V"
set_global_assignment -name MISC_FILE "Z:/msmst_test/msmst_test.dpf"
set_global_assignment -name USE_CONFIGURATION_DEVICE OFF
set_global_assignment -name GENERATE_RBF_FILE ON
set_global_assignment -name OUTPUT_IO_TIMING_NEAR_END_VMEAS "HALF VCCIO" -rise
set_global_assignment -name OUTPUT_IO_TIMING_NEAR_END_VMEAS "HALF VCCIO" -fall
set_global_assignment -name OUTPUT_IO_TIMING_FAR_END_VMEAS "HALF SIGNAL SWING" -rise
set_global_assignment -name OUTPUT_IO_TIMING_FAR_END_VMEAS "HALF SIGNAL SWING" -fall
set_global_assignment -name ACTIVE_SERIAL_CLOCK FREQ_40MHZ
set_global_assignment -name TCL_SCRIPT_FILE msmst_pin_constraints.tcl
set_global_assignment -name VHDL_FILE lpc_pod.vhd
set_global_assignment -name VHDL_FILE msmst_test.vhd
set_global_assignment -name VHDL_FILE msmst_test_top.vhd
set_global_assignment -name QIP_FILE msmst_test.qip
set_global_assignment -name SDC_FILE msmst_test.sdc
set_location_assignment PIN_AA31 -to clk_100MHz_pcie5
set_location_assignment PIN_AA32 -to "clk_100MHz_pcie5(n)"
set_location_assignment PIN_AE31 -to rx_in
set_location_assignment PIN_AE32 -to "rx_in(n)"
set_location_assignment PIN_AD29 -to tx_out
set_location_assignment PIN_AD30 -to "tx_out(n)"
set_instance_assignment -name IO_STANDARD "1.5-V PCML" -to rx_in
set_instance_assignment -name IO_STANDARD "1.5-V PCML" -to "rx_in(n)"
set_instance_assignment -name IO_STANDARD "1.5-V PCML" -to tx_out
set_instance_assignment -name IO_STANDARD "1.5-V PCML" -to "tx_out(n)"
set_instance_assignment -name IO_STANDARD HCSL -to clk_100MHz_pcie5
set_instance_assignment -name IO_STANDARD HCSL -to "clk_100MHz_pcie5(n)"
set_location_assignment PIN_F4 -to arria_rst_n
set_location_assignment PIN_D20 -to lpc_ad[0]
set_location_assignment PIN_C20 -to lpc_ad[1]
set_location_assignment PIN_B21 -to lpc_ad[2]
set_location_assignment PIN_A21 -to lpc_ad[3]
set_location_assignment PIN_D21 -to lpc_frame_n
set_location_assignment PIN_D17 -to lpc_clk
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to arria_rst_n
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to lpc_ad
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to lpc_frame_n
set_instance_assignment -name IO_STANDARD "3.3-V LVCMOS" -to lpc_clk
set_location_assignment PIN_K24 -to gpio_rxp[1]
set_location_assignment PIN_C27 -to gpio_rxp[2]
set_location_assignment PIN_A26 -to gpio_rxp[3]
set_location_assignment PIN_A28 -to gpio_rxp[4]
set_location_assignment PIN_C25 -to gpio_rxp[5]
set_location_assignment PIN_D25 -to gpio_rxp[6]
set_location_assignment PIN_C24 -to gpio_rxp[7]
set_location_assignment PIN_A24 -to gpio_rxp[8]
set_location_assignment PIN_K23 -to gpio_clkoutp
set_location_assignment PIN_D26 -to gpio_txp[1]
set_location_assignment PIN_J18 -to gpio_txp[2]
set_location_assignment PIN_K18 -to gpio_txp[3]
set_location_assignment PIN_J17 -to gpio_txp[4]
set_location_assignment PIN_K16 -to gpio_txp[5]
set_location_assignment PIN_D23 -to gpio_txp[6]
set_location_assignment PIN_D22 -to gpio_txp[7]
set_location_assignment PIN_D19 -to gpio_txp[8]
set_location_assignment PIN_K25 -to gpio_rxn[1]
set_location_assignment PIN_B27 -to gpio_rxn[2]
set_location_assignment PIN_A25 -to gpio_rxn[3]
set_location_assignment PIN_A27 -to gpio_rxn[4]
set_location_assignment PIN_B25 -to gpio_rxn[5]
set_location_assignment PIN_D24 -to gpio_rxn[6]
set_location_assignment PIN_B24 -to gpio_rxn[7]
set_location_assignment PIN_A23 -to gpio_rxn[8]
set_location_assignment PIN_C26 -to gpio_txn[1]
set_location_assignment PIN_H18 -to gpio_txn[2]
set_location_assignment PIN_K17 -to gpio_txn[3]
set_location_assignment PIN_H16 -to gpio_txn[4]
set_location_assignment PIN_J16 -to gpio_txn[5]
set_location_assignment PIN_C23 -to gpio_txn[6]
set_location_assignment PIN_C22 -to gpio_txn[7]
set_location_assignment PIN_D18 -to gpio_txn[8]
set_location_assignment PIN_K22 -to gpio_clkoutn
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to gpio_txp
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to gpio_txn
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to gpio_rxp
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to gpio_rxn
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to gpio_clkoutp
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to gpio_clkoutn
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to gpio_txp
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to gpio_txn
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to gpio_rxp
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to gpio_rxn
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to gpio_clkoutp
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to gpio_clkoutn
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to gpio_txp
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to gpio_txn
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to gpio_rxp
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to gpio_rxn
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to gpio_clkoutp
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to gpio_clkoutn
set_location_assignment PIN_T4 -to hsmc_clkout0
set_location_assignment PIN_AJ18 -to hsmc_clkin0
set_location_assignment PIN_U1 -to smb_hsmc_dat
set_location_assignment PIN_U2 -to smb_hsmc_clk
set_instance_assignment -name IO_STANDARD "2.5 V" -to hsmc_clkout0
set_instance_assignment -name IO_STANDARD "2.5 V" -to hsmc_clkin0
set_instance_assignment -name IO_STANDARD "2.5 V" -to smb_hsmc_dat
set_instance_assignment -name IO_STANDARD "2.5 V" -to smb_hsmc_clk
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to smb_hsmc_dat
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to smb_hsmc_clk
set_location_assignment PIN_A16 -to hsmc_d0_2p
set_location_assignment PIN_A15 -to hsmc_d0_2n
set_location_assignment PIN_C18 -to hsmc_d1_3p
set_location_assignment PIN_B18 -to hsmc_d1_3n
set_location_assignment PIN_J11 -to hsmc_txp[0]
set_location_assignment PIN_H12 -to hsmc_txn[0]
set_location_assignment PIN_C9 -to hsmc_txp[1]
set_location_assignment PIN_B9 -to hsmc_txn[1]
set_location_assignment PIN_D6 -to hsmc_txp[2]
set_location_assignment PIN_C6 -to hsmc_txn[2]
set_location_assignment PIN_C8 -to hsmc_txp[3]
set_location_assignment PIN_B8 -to hsmc_txn[3]
set_location_assignment PIN_D8 -to hsmc_txp[4]
set_location_assignment PIN_D7 -to hsmc_txn[4]
set_location_assignment PIN_K11 -to hsmc_txp[5]
set_location_assignment PIN_K10 -to hsmc_txn[5]
set_location_assignment PIN_D10 -to hsmc_txp[6]
set_location_assignment PIN_D9 -to hsmc_txn[6]
set_location_assignment PIN_C13 -to hsmc_txp[7]
set_location_assignment PIN_B14 -to hsmc_txn[7]
set_location_assignment PIN_A20 -to hsmc_clkout1p
set_location_assignment PIN_A19 -to hsmc_clkout1n
set_location_assignment PIN_C15 -to hsmc_rxp[0]
set_location_assignment PIN_D15 -to hsmc_rxn[0]
set_location_assignment PIN_D11 -to hsmc_rxp[1]
set_location_assignment PIN_C11 -to hsmc_rxn[1]
set_location_assignment PIN_D5 -to hsmc_rxp[2]
set_location_assignment PIN_C5 -to hsmc_rxn[2]
set_location_assignment PIN_B5 -to hsmc_rxp[3]
set_location_assignment PIN_B4 -to hsmc_rxn[3]
set_location_assignment PIN_A6 -to hsmc_rxp[4]
set_location_assignment PIN_A5 -to hsmc_rxn[4]
set_location_assignment PIN_A8 -to hsmc_rxp[5]
set_location_assignment PIN_A7 -to hsmc_rxn[5]
set_location_assignment PIN_A12 -to hsmc_rxp[6]
set_location_assignment PIN_A11 -to hsmc_rxn[6]
set_location_assignment PIN_C14 -to hsmc_rxp[7]
set_location_assignment PIN_D14 -to hsmc_rxn[7]
set_location_assignment PIN_R10 -to hsmc_clkin1p
set_location_assignment PIN_T10 -to hsmc_clkin1n
set_instance_assignment -name IO_STANDARD "2.5 V" -to hsmc_d0_2p
set_instance_assignment -name IO_STANDARD "2.5 V" -to hsmc_d0_2n
set_instance_assignment -name IO_STANDARD "2.5 V" -to hsmc_d1_3p
set_instance_assignment -name IO_STANDARD "2.5 V" -to hsmc_d1_3n
set_instance_assignment -name IO_STANDARD "2.5 V" -to hsmc_txp
set_instance_assignment -name IO_STANDARD "2.5 V" -to hsmc_txn
set_instance_assignment -name IO_STANDARD "2.5 V" -to hsmc_rxp
set_instance_assignment -name IO_STANDARD "2.5 V" -to hsmc_rxn
set_instance_assignment -name IO_STANDARD "2.5 V" -to hsmc_clkout1p
set_instance_assignment -name IO_STANDARD "2.5 V" -to hsmc_clkout1n
set_instance_assignment -name IO_STANDARD "2.5 V" -to hsmc_clkin1p
set_instance_assignment -name IO_STANDARD "2.5 V" -to hsmc_clkin1n
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to hsmc_d0_2p
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to hsmc_d0_2n
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to hsmc_d1_3p
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to hsmc_d1_3n
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to hsmc_txp
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to hsmc_txn
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to hsmc_rxp
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to hsmc_rxn
set_location_assignment PIN_AE12 -to hsmc_txp[8]
set_location_assignment PIN_AE13 -to hsmc_txn[8]
set_location_assignment PIN_AC13 -to hsmc_txp[9]
set_location_assignment PIN_AD13 -to hsmc_txn[9]
set_location_assignment PIN_AL8 -to hsmc_txp[10]
set_location_assignment PIN_AM8 -to hsmc_txn[10]
set_location_assignment PIN_AL7 -to hsmc_txp[11]
set_location_assignment PIN_AM7 -to hsmc_txn[11]
set_location_assignment PIN_AL10 -to hsmc_txp[12]
set_location_assignment PIN_AL11 -to hsmc_txn[12]
set_location_assignment PIN_AC11 -to hsmc_txp[13]
set_location_assignment PIN_AD11 -to hsmc_txn[13]
set_location_assignment PIN_AM11 -to hsmc_txp[14]
set_location_assignment PIN_AM12 -to hsmc_txn[14]
set_location_assignment PIN_AC12 -to hsmc_txp[15]
set_location_assignment PIN_AD12 -to hsmc_txn[15]
set_location_assignment PIN_AJ14 -to hsmc_txp[16]
set_location_assignment PIN_AK14 -to hsmc_txn[16]
set_location_assignment PIN_AC15 -to hsmc_clkout2p
set_location_assignment PIN_AC16 -to hsmc_clkout2n
set_location_assignment PIN_AM15 -to hsmc_rxp[8]
set_location_assignment PIN_AM16 -to hsmc_rxn[8]
set_location_assignment PIN_AM9 -to hsmc_rxp[9]
set_location_assignment PIN_AM10 -to hsmc_rxn[9]
set_location_assignment PIN_AJ9 -to hsmc_rxp[10]
set_location_assignment PIN_AK9 -to hsmc_rxn[10]
set_location_assignment PIN_AJ5 -to hsmc_rxp[11]
set_location_assignment PIN_AK5 -to hsmc_rxn[11]
set_location_assignment PIN_AJ8 -to hsmc_rxp[12]
set_location_assignment PIN_AK8 -to hsmc_rxn[12]
set_location_assignment PIN_AJ10 -to hsmc_rxp[13]
set_location_assignment PIN_AK10 -to hsmc_rxn[13]
set_location_assignment PIN_AJ12 -to hsmc_rxp[14]
set_location_assignment PIN_AK12 -to hsmc_rxn[14]
set_location_assignment PIN_AJ11 -to hsmc_rxp[15]
set_location_assignment PIN_AK11 -to hsmc_rxn[15]
set_location_assignment PIN_AJ13 -to hsmc_rxp[16]
set_location_assignment PIN_AK13 -to hsmc_rxn[16]
set_location_assignment PIN_AD16 -to hsmc_clkin2p
set_location_assignment PIN_AE16 -to hsmc_clkin2n
set_instance_assignment -name IO_STANDARD "2.5 V" -to hsmc_clkout2p
set_instance_assignment -name IO_STANDARD "2.5 V" -to hsmc_clkout2n
set_instance_assignment -name IO_STANDARD "2.5 V" -to hsmc_clkin2p
set_instance_assignment -name IO_STANDARD "2.5 V" -to hsmc_clkin2n
set_location_assignment PIN_P4 -to gpio_reserved[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to gpio_reserved
set_global_assignment -name MISC_FILE "D:/MSMST_iotest/fpga/msmst_test.dpf"
set_global_assignment -name IOBANK_VCCIO 2.5V -section_id 4A
set_global_assignment -name IOBANK_VCCIO 2.5V -section_id 7A
set_instance_assignment -name PARTITION_HIERARCHY root_partition -to | -section_id Top