This release note and the software that accompanies it are copyright (c) 2010, Intel Corporation or its suppliers, and may only be installed and used in accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not be construed as a commitment by Intel Corporation or its suppliers to market, license, sell or support any product or technology. Unless otherwise provided for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means without the express written consent of Intel Corporation.

==========================
Supported RAID Controllers
==========================
This download supports Intel(R) RAID controllers using SAS software stack (SRCSAS18E, SRCSAS144E, SRCSASPH16I and SROMBSAS18E), please verify that this utility has been tested with the RAID card you have chosen to use by checking the drivers web page for your controller at http://support.intel.com.

===================
Package Information
===================
Flash package = 7.0.1-0075
Firmware Version = 1.12.280-0826

==========
Attention!
==========
Intel recommends to loading Factory Default setting after the firmware upgrade which will not affect data on any existing array. To do so:
1. Reboot the system and login to the RAID BIOS Console. 
2. Select the controller and select 'Adapter Properties'->'Next'
3. Set the 'Set Factory Defaults' setting to 'Yes' and submit the change.
4. Reboot the system (the default settings are applied).
5. Re-configure to the desired settings in RAID Web Console2.

=======================
Contents on the package
=======================
The following files are included in this zip:

Name:								Description:
IR3_1068SASHWR_FW-v1.12.280-0826_readme.txt	This file
68_fw826.rom						Firmware binary
68_fw826_4MB.rom						4MB Firmware binary
update.bat							DOS firmware update batch file
update.nsh							UEFI shell firmware update script file
License_v2.pdf						License Agreement
CmdTool2\DOS\*						DOS update utility and support files
CmdTool2\UEFI\*						UEFI update utility and support files
CmdTool2\Linux\*						Linux update utility and support files
CmdTool2\Windows\*					Windows update utility and support files
CmdTool2\Solaris\*					Solaris update utility and support files


==========================
Installation instructions:
==========================
DOS instructions for updating RAID Firmware:
-----------------
   1. Download and extract all files to a local drive.
   2. Ensure RAID DIMM (for SRCSAS18E or SROMBSAS18E) is installed. 
   3. Boot the target system to DOS. 
   4. Change directory to the local drive and directory containing the flash update files and the firmware image file.
   5. Type "update.bat" or "cmdtool2 -adpfwflash -f 68_fw826.rom -aall"
   6. Wait for the flash to complete. Do NOT reboot the system during the update.

Note: The DOS4GW.EXE file may not work on machines that do not support legacy port 60/64 keyboard calls.  If you have problems, please try the UEFI version of CmdTool2.

UEFI (EFI 2.0) instructions for updating RAID Firmware:
-----------------
   1. Download and extract all files to a local drive.
   2. Ensure RAID DIMM (for SRCSAS18E) is installed. 
   3. Boot the target system to EFI shell. 
   4. Change directory to the local drive and directory containing the flash update files and the firmware image file.
   5. Type "update.nsh" or "efi\cmdtool2 -adpfwflash -f 68_fw826.rom -aall"
   6. Wait for the flash to complete. Do NOT reboot the system during the update.

Windows and Linux instructions for updating RAID Firmware:
-----------------
The firmware update may be run from Within Windows or Linux using the appropriate versions of CmdTool2.
  In Windows, unzip the utility into the same directory as the rom file by typing 
      "cmdtool2 -adpfwflash -f 68_fw826.rom -aall". 
  The Linux CmdTool2 by running the rpm and then calling the utility from /opt/MegaRAID/CmdTool2 as 
      "./CmdTool2 -AdpFwFlash -f 68_fw826.rom -aall"


=============
Fixes/Updates 
=============
v1.12.280-0826
1) Fixed Firmware should not set the WCE bit in the saved page of the disk.
2) Fixed BBU1 is missing intermittently or permanently at boot.
3) Fixed RWC2 Failed to show all drives
4) Fixed HWR FW marks drive dead after receiving Sense 0x03,11,00 (ECC Error) for recovery write (SCSI CDB 0x2E) using SATA HDD.

v1.12.270-0718
1) Fixed SMART error still reported in 24 hours, even after replacing with good disk.
2) Fixed SAS Topology Error.
3) Added set self affiliation SATA link reset bit.
4) Fixed predictive failures reported for removed drives.

v1.12.260-0687
1) Added Check Additional length in mode sense command   
2) Disallow creation of GHS with smaller size PD   
3) Fixed null pointer access with in a print statement   
4) Fixed Selection of any PD fails if GHS is created out of smaller PD.   
5) Modify to support 1068 controller reset for IOP hangs with Prefetch abort exception   
6) Restrict number of medium errors per message   
7) Changes to support FW flushing disk cache during Hibernation or when no file system is present.   
8) Fixed Continuous Media Error (CME) causing driver to dump 84016   
9) Added Prefetch work-around   
10) Fixed CC does not work properly after correcting medium   
11) Fixed hangs when it found a single inconsistency on RAID 5.

v1.12.230-0598
1) Fixed FW not getting event logs with wrapped events   
2) Fixed data integrity issue with multi row write on media error block   
3) Fixed commands lost issue during Heavy I/O   
4) Fixed FW incorrectly sets battery status as missing   
5) Fixed pull single drive causes all drives on quad to fail issue   
6) Fixed check consistency doesn't regenerate parity with double media errors   
7) Fixed¡°OS not found¡± issue when media error occurred on the DDF anchor of OS drive.   
8) Fixed NVRAM checksum error which could induce the next scheduled BBU auto relearn started immediately   
9) Updated the Gas Gauge temperature offset to 0.7 for all Li-ION batteries   
10) Fixed BGI and MDC not working issue   
11) Fixed inconsistency error during CC after bad block recovery where the data and P parity are bad on R6   

v1.12.220-0560
1) Fixed system delays detecting drives on internal Enclosure   
2) Fixed existing VD gets initialized while creating new VD   
3) Fixed auto re-learn does not start issue   
4) Fixed LION battery max error =25% after relearn   
5) Fixed Data Integrity issue when do the AC power-off after the data(file) write during the rebuild with BBU installed.   
6) Fixed Data Integrity issue when reconstruction found uncorrectable media error.   
7) Fixed Data Integrity issue with medium errors on R5 while rebuilding   
8) Updated BBU's factory setting   

v1.12.200-0527
1) Fix potential data loss RAID 6 double media Error issue
2) Fixed data miscompare issue while running IO on double media error RAID 6 array

v1.12.190-0507
1) Fixed Patrol Read cannot run in the certain condition
2) Fixed Battery removed event when battery is still connected
3) Fixed FW never sets the next schedule of Patrol Read.
4) Adding debug code and pre-fetch workaround 
5) Fixed Configuration not found when cold boot. 
6) Fixed LEDs (I2C) do not work issue 
7) Fixed SATA drives are not getting punctured correctly during a rebuild 
8) Fixed F/W crash in Group SGL parse. 
9) Fixed GLOBAL SAS ACTIVITY LED
10) Fixed NMI occurs while running Diskspd on Windows XP 
11) Fixed Suddenly Write Cache policy becomes into Write Through from Write Back. 
12) Fixed Firmware hang when PR doing media recovery 
13) Fixed Firmware hangs on extended reboot test 
14) Fixed Firmware detects illegal request against CDB 0x15 and 0x1A in SATA environment. 
15) Fixed Firmware hangs with Fatal Firmware Error when it detect sense 0x03,0C,03 after medium error recovery on Patrol Read. 
16) Firxed Firmware hangs with Fatal Firmware Error when it detect sense 0x0B after medium error recovery on Patrol Read. 

v1.12.170-0471
1) Fixed Firmware hang issue when Patrol Read doing media recovery
2) Fixed the activity LED malfunction issue under Windows and Linux
3) Fixed suddenly Write Cache policy becomes into Write Through from Write Back issue
4) Fixed The I2C LED support does not work issue
5) Fixed SATA drives are not getting punctured correctly during a rebuild
6) Fixed the Firmware hang issue under heavy stress test

v1.12.160-0462
1) Fixed configuration not found issue when cold boot
2) Fixed out-of-band SES2 enclosure management support issue
3) Updated bootblock to support LiON Battery backup unit

V1.12.150-0438
1) Added support for LiON Battery Backup Unit
2) Added programmable delay feature during boot up
3) Fixed Hard disk activity LED always on issue
4) Forced SATA drives speed to 1.5Gb for specified config
5) Suspend BBU discharging if temperature goes up more

V1.12.130-0418
1) Fixed FW breoken issue during RAID level migration if media error detected
2) Fixed controller hang issue under outstanding I/O

V1.12.120-0394
1) Enabled offline HDD FW flash.
2) Fixed HWR FW violates the DDR2 spec during the initialization sequence in 1078 ROMB environment.
3) Fixed 1078 FW cannot mark a drive dead after the Sense response 0x03-0C-03 for Write command.
4) Fixed Offline HDD/ESM microcode update feature broken
5) Fixed SATA Drives dropping for Internal ports of SRCSASJV
6) Fixed Partial VD is deleted automatically which is created during rebuild
7) Fixed Rebuilding source SATA HDD becomes failed, when some of ECC errors detected on source drive during rebuild
8) Fixed Data miscompare occurred on a SAS "Degraded" RAID6 VD while running iomonkey
9) Fixed Grammatical Errors and Improper Line Breaks in ECC error messaging
10) Fixed jump to Megamon during Error Injection (PFA)06/5D/00 FAILURE PREDICTION THRESHOLD EXCEEDED
11) Fixed after Drive migration size varies in the target server
12) Fixed PL reset reported during booting sequence into RHEL 5 64bit OS
13) Fixed sequential write performance for recent sql overlapped issue
14) Fixed "F/W Flushing Cache" message is not displayed at POST when flushing data on an array that is Partially Degraded or Degraded
15) Fixed Fixed SQLIO Stress tool returned failure
16) Fixed FT32 halts with RAID Memory Error doing reboots
17) Fixed Large Number of Drives and TPC-C
18) Fixed Rebuilding source SATA HDD becomes failed, when some of ECC errors detected on source drive during rebuild
19) Fixed 1078 errata w/ 32G DMA memory range
20) Fixed AUTO Port configuration not working on Casseipeia with External connectors
21) Fixed SES w/ Riggins not working on 1078 cards
22) Fixed Grammatical Errors and Improper Line Breaks in ECC error messaging
23) Fixed Partial VD is deleted automatically which is created during rebuild.
24) Fixed Deleting the partial VD during rebuild leads to Configuration loss
25) Fixed Partial VD able to be created during a rebuild
26) Fixed Rebuild on RAID 6 Physical disks toggles percentage completion.
27) Fixed Orphaned drive in RAID6 reports incorrect size after re-insertion.
28) Fixed OS crashed after S3 resume and restart manually
29) Fixed Data integrality issue occurred during enclosure power cycle test.
30) Fixed Firmware crashed during boot with bad SAS cable between two enclosures.
31) Fixed Data integrality issue with media errors with IOS and rebuild going on in parallel
32) Fixed VD created on the Physical disks that were part of RLM, goes in offline state
33) Fixed Controller enters megamon when a rebuilding span is removed.
34) Fixed System Halted, will not enter BIOS
35) Fixed Global HDD summary LED (GPIO Pin 11 on 1078) not working
36) Fixed Unable to import foreign configuration
37) Fixed Cassiopeia controller does not work with 6m cable with OEM enclosure attached to external connector
38) Fixed CTRL-Y pre-OS command line utility memory allocation issue
39) Fixed data integrity issue during stress with R50 in degraded mode
40) Fixed data integrity issue when all medium errors were punctured
41) Fixed S3 mode BSOD issue
42) Fixed data inconsistency issue which occurs running I/O and performing capacity expansion.

v1.12.00-0310
1) Fixed Wrong event generated for VD creation(OS: W2K3 32bit:2.0.0.32)
2) Fixed After rebooting the system, the old configuration is disappear
3) Fixed Backplanes are not visible by FW
4) Fixed FW hit megamon with hotplug
5) Fixed configuration created on foreign drives
6) Fixed Open_Flag in DDF anchor header is set to 0x00 instead of 0xFF
7) Fixed Offline FW Download doesn't work in 1078 codebase
8) Fixed DDF structrure storage consumes too much DRAM
9) Fixed For Foreign configuration, FW didn't fill up correct info for enclosure ID and PD slots
10) Fixed Oconee 2 firmware is not working
11) Fixed DDF_populateBvdList, Ran out of Memory Space; FW went to debugger
12) Fixed SAS_CIM_Linux:PDEnclosureDeviceID of an NonEnclPD is misleading
13) Fixed Amber LED not functional while rebuilding pd
14) Fixed NEC Stinger backplane is not assigned enclosure ID
15) Fixed SAS-OCONEE2-FW:Alarm sound behaves incorrectly
16) Fixed FW break during boot
17) Fixed SAS-OCONEE-FW:Unexpected AEN of PD State Change if remove a pd when initialization is going on
18) Fixed ROMB solution does not recognize internal backplanes
19) Fixed Alarm not functioning properly after reconsturction completes
20) Fixed Enable/Disable NCQ on SATA drives attached to Occone-2 via ENV variable.
21) Fixed Scheduled Consistency Check does not start
22) Fixed RBC display Wrong SAS Controller's name
23) Fixed NiMH and the lithium Ion bbu on both ports 0 and 2 need to be seen by FW
24) Fixed Pdclear starts automatically on an initializing VD when another VD with BGI running is deleted
25) Fixed DIsable Adding Reset Q Rdm print
26) Fixed Driver detected possible FW hang, halting FW
27) Fixed Take too long for Hibernation command to Hibernate
28) Fixed Reconstruction Rate feature
29) Fixed Exceed the max media error entries in sBBM table
30) Fixed LD goes offline after several reboots
31) Fixed FW_OCONEE2_SYSTEM: Coerced Size of PDs increase after importing foreign config
32) Fixed FW_OCONEE2_SYSTEM:PD is becoming "Not Importable" for "All Config" in WebBios
33) Fixed EVT#13099-06/05/07 18:54:58: 34=Not enough controller memory
34) Fixed iBBU boot message on POSW shows twice
35) Fixed SAS-OCONEE2:"Bad block table on PD is full" event comes if SAS pd is having more than 254 media errors
36) Fixed Returns SMART warning though SMART is disabled
37) Fixed Caph is unable to detect foreign config from SWR Clark
38) Fixed Imported R6 with CC running does not restart any CC activity
39) Fixed FW Device Module does not handle 02/04/11
40) Fixed Rebuild failed on PD 07(e0x00/s8) due to target drive error
41) Fixed Redesign delaying of driver load as per fix for DF#68156.
42) Fixed Ensure TM process queue task is only created when needed
43) Fixed Multi dead
44) Fixed XOR/Memory test on Hydra controller do not complete.
45) Fixed BBU MFG SEAL Failed
46) Fixed DDR2: Regras value should be minimum of 31 or above
47) Fixed jump to Megamon during Error Injection (PFA)06/5D/00 FAILURE PREDICTION THRESHOLD EXCEEDED
48) Fixed LDBBM table is not cleared during Fast and Full Init.
49) Fixed RBC does not change the controller mux setting to auto.
50) Fixed Link Status Change Event missing
51) Fixed MsgRelease: Msg is not in use
52) Fixed With PDFailed History enabled, a pulled and reinserted drive starts rebuilding automatically
53) Fixed WHQL DTM Driver Reliability Job ID 1177 Disable Enable with IO test fails
54) Fixed DTm test Common Scenario stress fails with stop 109 error on ws2003 x64 on embedded 1078
55) Fixed Estimated time left indicator shows wrong value
56) Fixed Incorrect non-ECC message being posted
57) Fixed An IR config that is migrated to a RAID controller only imports one drive from each array
58) Fixed An offline IR R0 config can successfully be imported on RAID
59) Fixed Data Miscompare Found
60) Fixed Cache flushing not working with specific OEM selected
61) Fixed Problem with 1078 on Systems with More than 32 GB of Memory
62) Fixed BBU ON causes hangs/scrolling in CTRL _R on SAS 2.1 fw
63) Fixed An IR R0 imported to MR is shown as half the original size
64) Fixed FW goes to megamon
65) Fixed Assertion failure during RLM from R5 to R6 with uncorrectable medium errors
66) Fixed LDBBM Data Abort on Raid 6 during Rebuild with I/O in the background
67) Fixed Missing merge SAS 1.03 to Oconee 2 for Intermittent link failure causes HDD marked dead
68) Fixed Missing merge from SAS 1.03 to Oconee 2 for skipping temp differencial of 5 degree for one OEM
69) Fixed VD created on the Physical disks that were part of RLM, goes in offline state
70) Fixed Grammatical Errors and Improper Line Breaks in ECC error messaging
71) Fixed OS crashed after S3 resume and restart manually
72) Fixed Unable to import foreign configuration
73) Fixed PL reset reported during booting sequence into RHEL 5 64bit OS
74) Fixed Controller enters megamon when a rebuilding span is removed.
75) Fixed Data miscompare occurred on a SAS "Degraded" RAID6 VD while running iomonkey
76) Fixed Data miscompare occurred on a SAS "Degraded" RAID6 VD while running iomonkey
77) Fixed Imported degraded array does not result in automatic rebuild
78) Fixed Using storelibtest, the sequence event 0 and 1 are returning same event info
79) Fixed OCONEE2_PreRegression: MSM-2.25 does not start the fast/slow initialization at the time of making LD
80) Fixed ZCR - Foreign Import causing FW break
81) Fixed Lost Configuration after cold boot and config comes back after warm boot
82) Fixed Oconee 2 FW code does not pass function test
83) Fixed Reduce number of pdCODs to save DRAM
84) Fixed RMU shows Hot Spare drives with a ¡°¡±
85) Fixed Purge unused DDF data structure
86) Fixed SAS-SNMP:Intermittent prob: Storelibtest is displaying an unexpected value for BBU Charger Status
87) Fixed VD deletion stops rebuild operation on another VD that shares the member PDs.
88) Fixed Every LD creation causes cache init
89) Fixed "Memory/Battery problems were detected, ...cache data was lost" msg when setting BBUON
90) Fixed Migrating TBBU discards dirty cache
91) Fixed Migrating TBBU discards dirty cache
92) Fixed i2cSetMux: ERROR 0x2 setting I2C Mux
93) Fixed During heavy I/O and rebuild, the system hits MegaMon & reboot by itselft.
94) Fixed Controller experienced driver-induced dead adapter condition during I/O stress.
95) Fixed RAID init hangs during boot after driver-induced FW break.
96) Fixed RAID fw auto-imports a foreign config at boot when a native config is present.
97) Fixed FW break while running I/O overnight
98) Fixed Auto Rebuilds fail to start @ first then FW break after a minute later
99) Fixed 7% drop in Seqential Writes Peformance on R6 on I/O size 4K, 8K and 16K from FW 227 to FW 234
100) Fixed FW hangs when running R6 rebuild on each different PD vendor
101) Fixed Performance drop with WB enabled for certian Strip sizes.
102) Fixed Controller loses communication with enclosure after SEP reboot command is issued.
103) Fixed Firmware does not correctly handle internal backplane/encl fw upgrade.
104) Fixed Quick PD removal/insertion can cause incorrect drive write cache setting
105) Fixed MSM window freezes on attempting to open Group Initialization screen after creation of 64 VDs.
106) Fixed Firmware reports incorrect enclosure position number
107) Fixed Global hsp become offline when creating after ld degrared while FGI is running
108) Fixed Global hotspare goes offline during FGI on RAID5
109) Fixed Target Resets fails ( IOCStatus = 0x4a) after 3 retry
110) Fixed Hitachi SATA drives did not function properly during I/O
111) Fixed FW break after removing drives from arrays
112) Fixed FW break while running HS rebuilds loop
113) Fixed FW crashed after pulling the second drive from each R6
114) Fixed Reset Chip 0: CurQdepth reset for Ld[0] to LD[100] FW went to debugger
115) Fixed Target Resets fails ( IOCStatus = 0x4a) after 3 retry
116) Fixed Hitachi SATA drives did not function properly during I/O
117) Fixed FW break after removing drives from arrays
118) Fixed FW break while running HS rebuilds loop
119) Fixed FW crashed after pulling the second drive from each R6
120) Fixed Reset Chip 0: CurQdepth reset for Ld[0] to LD[100] FW went to debugger
121) Fixed IR Raid 0 imported to MegaRaid BAIL_OUT cmdStat=3
122) Fixed Firmware reports incorrect controller connector number in enclosure AENs.
123) Fixed Some backplane SEP returns the complete page even if only 4 bytes are requested.
124) Fixed FW hang while running error injection script under I/O
125) Fixed FW crashed while running error injection script under I/O
126) Fixed Deleting a degraded 8 partition (32) Disk RAID6 breaks into megamon from CTRL-R
127) Fixed x32 HDD RAID6 w/ 8 equal 1.2TB VD's causes driver disconnect
128) Fixed RAID firmware reports that no free messages are available; causes I/O pauses.
129) Fixed Can not import configuration from SWR to HWR. If the config contains SATA drives.
130) Fixed x32 HDD RAID6 w/ 16 LDs using different stripe sizes causes driver disconnect
131) Fixed SBBM table is not imported while importing foreign config from SWR to HWR raid.
132) Fixed VD offlined due to puncture table full is lost after server reboot
133) Fixed fw break During rebuild and BGI and heavy IO
134) Fixed Filling the ECC error count causes repeatedly generates AEN's
135) Fixed No post message when discarding dirty cache when VDs are missing
136) Fixed LDs drop offline while running I/O across max R5s
137) Fixed System experiences BSOD during enclosure power cycle test.
138) Fixed PDs dropped offline while running rebuild script
139) Fixed RAID firmware reports event with sense data of zero
140) Fixed When PD caches disabled causing PDs drop offline
141) Fixed Continuous SEP reset from enclosure debugger causes PL fw to stop communicating
142) Fixed System experiences BSOD during enclosure power cycle test.
143) Fixed System experiences BSOD during enclosure power cycle test.
144) Fixed Invalid SAS topology w/ 2 enclosures
145) Fixed Rebuilding does not start on Raid 60
146) Fixed FW breaks when running I/O on 45x R1s
147) Fixed FW hang when running I/O on 45x R1s
148) Fixed FW breaks when have a bad drive
149) Fixed Data integrality issue during Heavy IO (10 x 3PD x R5 rebuilding across 3 encl. Stripe 64k-1mb)
150) Fixed Data integrality issue During Heavy IO 
151) Fixed 1078 Errata 16 not implemented
152) Fixed FW break when running error injection script along with rebuilding drive.
153) Fixed 1078 controller to SEP I2C connection not functioning properly
154) Fixed FW break running muliple stripe R6 from a single disk group of 30 PDs
155) Fixed FW break when running multiple pulls & force offline R1s + R6s with GHS using multiple stripe sizes
156) Fixed FW goes to Megamon during heavy IO, Rebuild and Recon
157) Fixed Fw Hits MegaMon during heavy I/O over the weekend
158) Fixed RAID 0 WB performance w/ 1078 lower than obersved w/ 1068
159) Fixed Firmware failed online drives when a separate enclosure was powered off.
160) Fixed FW breaks into megamon when timeout fw used to timeout send diagnostic cmds
161) Fixed Firmware crashed during boot with bad SAS cable between two enclosures.
162) Fixed incorrect connector string for enclosure events
163) Fixed Potential data integrality issue during WB IOs with media errors on degraded/partially degraded LD
164) Fixed Data integrality issue when running error injection script along with I/O in partially degraded mode
165) Fixed Verify Cache Flushing on Raid after pulling power cable
166) Fixed Verify Cache Flushing on Raid after pulling power cable
167) Fixed FW breaks while running rebuilds across 32 drive with mixing different stripe sizes per array
168) Fixed FW breaks During heavy IO, rebuild and BGI
169) Fixed FW breaks R6 in degaded mode during heavy IO
170) Fixed FW breaks with I/O over multiple LDs
171) Fixed FW breaks during Heavy IO and Reconstruction using Multiple stripe sizes
172) Fixed FW breaks when disconnecting cable during rebuild
173) Fixed Complete delivery of Xyratex fix to Integration stream.
174) Fixed FW went to debugger
175) Fixed FW breaks when running multiple R5s pulls/reinsertions
176) Fixed FW hang when disconnecting cable during rebuild
177) Fixed Data integrality issue occurred during enclosure power cycle test.
178) Fixed Multiple R1s pulls/insertions caused LDs dropping offline
179) Fixed Data integrality issue when running error injection script along with rebuilding drive
180) Fixed OEM ROMB not working with 667MHz memory
181) Fixed Blue screen when delete VD after finish rebuild
182) Fixed creating an unrecoverable medium error causes the drive to be taken offline
183) Fixed Driver Disconnect due to a FW hang w/ 32HDD/BGI/Multi-Strip and FW 6.0.1-0058
184) Fixed BST R6 Rebuild Data integrality issue
185) Fixed Rebuild on RAID 6 Physical disks toggles percentage completion.
186) Fixed Controller enters megamon when a rebuilding span is removed.
187) Fixed OEM system cause memory SPD not to be read correctly
188) Fixed Incorrect non-ECC message being posted
189) Fixed POST halts indefinately when invalid SAS address is found
190) Fixed "Unstable Enclousure" message seen in Windows
191) Fixed SAS ZCR BBU never charges after reconditioning cycle until after a reboot.
192) Fixed SAS ZCR relearn should hold off until fast charge is complete
193) Fixed The 1068 is asserting INTA/ and ALT_INTA/ together when he is in ZCR mode
194) Fixed 6850 BMC holds ROMB VOLT ERR state after I learn cycle
195) Fixed Data abort
196) Fixed DTM Sleep Stress Failure on SRCSAS144E FW0211 Driver 2.8 and 2.11
197) Fixed Hang when the Windows drive initializes the ZCR during OS boot
198) Fixed I/O fail issue with JBOD
199) Fixed Auto learn mode does not work properly
200) Fixed GHS without affinity take place first then GHS with affinity.

v1.03.60-0255
1) Fixed Temp diff message 
2) Fixed Intermittent link failure causes HDD marked dead 
3) Fixed "Unstable Enclousure" message seen in Windows 
4) Fixed BMC holds ROMB VOLT ERR state after controller learn cycle 
5) Fixed Data abort 
6) Fixed No post message when discarding dirty cache when VDs are missing 
7) Fixed Hang when the Windows drive initializes the controller during OS boot 
8) Fixed I/O fail issue with JBOD 
9) Fixed Auto learn mode does not work properly 
10) Fixed GHS without affinity take place first then GHS with affinity. 
11) Fixed DTM Sleep Stress Failure issue 
12) Fixed Fix debug code and serial dumping
13) Fixed Read from ENV STAMP to enable/disable NCQ 
14) Fixed IO errors and aborted journal running stress 
15) Fixed Foreign View page displays incorrect RAID level and size for a foreignVD 
16) Fixed FW writes MFI command status followed by the extended status 
17) Fixed Migrating TBBU discards dirty cache when VDs are not available 
18) Fixed WCE bit reversed issue. 
19) Fixed Verify command does not always detect Media error 
20) Fixed FW hault when bad block management tables reaches 202 in DDF table 
21) Fixed Config lost after rebooting 
22) Fixed HDD Spin-up setting values are not possible. 
23) Fixed Stop error after HotRebuild 

*Third-party trademarks are the property of their respective owners.


