For installing RAID, use USB Port 2 on the 886LCD-M/Flex for external USB floppy 
connection during the required driver installation.

Install the "Intel Matrix Storage Console" in windows, this will monitor the RAID
and can also repair the Raid.