PICA-PRIVATE-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Counter32, Gauge32, Counter64,
    Integer32, TimeTicks, mib-2, snmpModules,IpAddress,
    NOTIFICATION-TYPE                        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, DisplayString,
    PhysAddress, TruthValue, RowStatus,
    TimeStamp, AutonomousType, TestAndIncr   FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP,
    NOTIFICATION-GROUP                       FROM SNMPv2-CONF
    snmpTraps                                FROM SNMPv2-MIB
    IANAifType                               FROM IANAifType-MIB
    enterprises				     			 FROM RFC1155-SMI;
              
    picaPrivateMib MODULE-IDENTITY
        LAST-UPDATED "201104280000Z"
        ORGANIZATION "Pica8 Inc."
        CONTACT-INFO
            "                      Customer Support
            E-Mail:                support@pica8.com
            WWW:                   http://www.pica8.com"
        DESCRIPTION
            "The MIB module to manage Pica8's Pronto product."
        REVISION
            "201104280000Z"
        DESCRIPTION
            "The Pica8 Private MIB, Initial Version.
             Author: Robin Wan."

        ::= { enterprises 35098 }           
   	
   	hostStatusGroup OBJECT IDENTIFIER ::= { picaPrivateMib 1 }

    cpuUsage OBJECT-TYPE
        SYNTAX		INTEGER(0..100)
        MAX-ACCESS	read-only
        STATUS		current
        DESCRIPTION
                "The usage of CPU, the output format is integer."
        ::= { hostStatusGroup 1 }  
        
    totalPhyMemory OBJECT-TYPE
        SYNTAX		DisplayString
        MAX-ACCESS	read-only
        STATUS		current
        DESCRIPTION
                "The total physical memory size, the output format is string."
        ::= { hostStatusGroup 2 }   
            
    usedPhyMemory OBJECT-TYPE
        SYNTAX		DisplayString
        MAX-ACCESS	read-only
        STATUS		current
        DESCRIPTION
                "The used physical memory size, the output format is string."
        ::= { hostStatusGroup 3 }

    freePhyMemory OBJECT-TYPE
        SYNTAX		DisplayString
        MAX-ACCESS	read-only
        STATUS		current
        DESCRIPTION
                "The free physical memory size, the output format is string."
        ::= { hostStatusGroup 4 }
                
    switchTemperature OBJECT-TYPE
        SYNTAX		DisplayString
        MAX-ACCESS	read-only
        STATUS		current
        DESCRIPTION
                "The temperature of switch, the output format is integer."
        ::= { hostStatusGroup 5 }
    
    cpuTemperature OBJECT-TYPE
        SYNTAX		DisplayString
        MAX-ACCESS  read-only
        STATUS		current
        DESCRIPTION
                 "The teperature of CPU, the output format is integer."
        ::= { hostStatusGroup 6 }

    switchChipTemperature OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                 "The teperature of switch chip."
        ::= { hostStatusGroup 7 }
    
    switchFanSpeed OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                 "The fan speed of switch chip."
        ::= { hostStatusGroup 8 }

    switchPWM OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                 "Pulse Width Modulation(PWM) of switch chip."
        ::= { hostStatusGroup 9 }     

    sfpstatusTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF SfpstatusEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "A list of sfp moudule status entries."
        ::= { hostStatusGroup 10 }

    sfpstatusEntry OBJECT-TYPE
        SYNTAX      SfpstatusEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry containing all sfp module stauts"
        INDEX   { sfpIndex }
        ::= { sfpstatusTable 1 }
    
    SfpstatusEntry ::=
    SEQUENCE {
        sfpIndex                INTEGER,
        sfpVendorName           DisplayString,
        sfpSerialNumber         DisplayString,
        sfpTemp                 DisplayString,
        sfpVoltage              DisplayString,
        sfpBias                 DisplayString,
        sfpTxPower              DisplayString,
        sfpRxPower              DisplayString,
        sfpType                 DisplayString
    }

    sfpIndex OBJECT-TYPE
    SYNTAX      INTEGER (1..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The port number of interface."
    ::= { sfpstatusEntry 1 }

    sfpVendorName OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The vendor name of sfp ransceiver transfer."
    ::= { sfpstatusEntry 2 }

    sfpSerialNumber  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The serial number of sfp ransceiver transfer."
    ::= { sfpstatusEntry 3 }
    
    sfpTemp   OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The temperature of sfp ransceiver transfer."
    ::= { sfpstatusEntry 4 }
    
    sfpVoltage   OBJECT-TYPE
    SYNTAX        DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The voltage of sfp ransceiver transfer."
    ::= { sfpstatusEntry 5 }

    sfpBias     OBJECT-TYPE
    SYNTAX         DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The bias current of sfp ransceiver transfer."
    ::= { sfpstatusEntry 6 }
    
    sfpTxPower  OBJECT-TYPE
    SYNTAX         DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The Tx power of sfp ransceiver transfer(dBm)."
    ::= { sfpstatusEntry 7 }    

    sfpRxPower   OBJECT-TYPE
    SYNTAX           DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The Rx power of sfp ransceiver transfer(dBm)."
    ::= { sfpstatusEntry 8 }

    sfpType    OBJECT-TYPE
    SYNTAX          DisplayString    
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The type of sfp ransceiver transfer(dBm)."
    ::= { sfpstatusEntry 9 }    

      
    rpsustatusTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF RpsustatusEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "A list of Redundancy power supply unit(RPSU) status entries."
        ::= { hostStatusGroup 11 }
    rpsustatusEntry OBJECT-TYPE
        SYNTAX      RpsustatusEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
            "An entry containing all Redundancy power supply unit(RPSU) stauts."
        INDEX   { rpsuIndex }
        ::= { rpsustatusTable 1 }

    RpsustatusEntry ::=
     SEQUENCE {
        rpsuIndex                INTEGER,
        serialNumber             DisplayString,
        rpsuStatus               INTEGER,
        rpsuTemprature           DisplayString,
        rpsuFanSpeed             INTEGER,
        rpsuPWM                  DisplayString
    }
    rpsuIndex OBJECT-TYPE
    SYNTAX      INTEGER(0..10)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The slot number Redundancy power supply unit(RPSU)."
    ::= { rpsustatusEntry 1 }

    serialNumber OBJECT-TYPE
    SYNTAX       DisplayString
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The serial number Redundancy power supply unit(RPSU)."
    ::= { rpsustatusEntry 2 }

    rpsuStatus OBJECT-TYPE
    SYNTAX      INTEGER (0..1)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The status of Redundancy power supply unit(RPSU).
             1: The Redundancy power supply unit(RPSU) power on.
             0: The Redundancy power supply unit(RPSU) power off."
    ::= { rpsustatusEntry 3 }

    rpsuTemprature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Temprature of the Redundancy power supply unit(RPSU)."
    ::= { rpsustatusEntry 4 }
    
    rpsuFanSpeed OBJECT-TYPE
    SYNTAX      INTEGER(1..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Fan speed of the Redundancy power supply unit(RPSU)."
    ::= { rpsustatusEntry 5 }
    
    rpsuPWM OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Pulse Width Modulation(PWM) of the Redundancy power supply unit(RPSU)."
    ::= { rpsustatusEntry 6 }

   switchConfigGroup OBJECT IDENTIFIER ::= { picaPrivateMib 2 }
   
   tftpConfigFilePath OBJECT-TYPE
            SYNTAX     OCTET STRING (SIZE (2..255))
            MAX-ACCESS read-write
            STATUS     current
            DESCRIPTION
                    "If the tftp path of defined config file is set, the configurations
                    included in the config file are also applied meanwhile. "
            ::= { switchConfigGroup 0 }

   tftpBatchFilePath OBJECT-TYPE
            SYNTAX     OCTET STRING (SIZE (2..255))
            MAX-ACCESS read-write
            STATUS     current
            DESCRIPTION
                    "If the tftp path of a command batch file is set, the present configurations
                    will changed depending on the execution of the command in the batch file."
            ::= { switchConfigGroup 1 }
   
picaConformance OBJECT IDENTIFIER ::= { picaPrivateMib  20}
picaGroups      OBJECT IDENTIFIER ::= { picaConformance 1 }
picaCompliances OBJECT IDENTIFIER ::= { picaConformance 2 }

picaBasicGroup    OBJECT-GROUP
    OBJECTS {
        cpuUsage,
        totalPhyMemory,
        usedPhyMemory,
        freePhyMemory,
        switchTemperature,
        cpuTemperature,
        switchChipTemperature,
        switchFanSpeed,
        switchPWM
        
    }
    STATUS  current
    DESCRIPTION
       "These objects are required for pica private mib."
   ::= { picaGroups 1 }
picasfpGroup  OBJECT-GROUP
OBJECTS {
        sfpIndex,
        sfpVendorName,
        sfpSerialNumber,
        sfpTemp,
        sfpVoltage,
        sfpBias,
        sfpTxPower,
        sfpRxPower,
        sfpType
    }  
   STATUS  current
    DESCRIPTION
       "These objects are required for pica private mib."
   ::= { picaGroups 2 }

picarpsuGroup OBJECT-GROUP
OBJECTS {
        rpsuIndex,
        serialNumber,
        rpsuStatus,
        rpsuTemprature,
        rpsuFanSpeed,
        rpsuPWM
    }
   STATUS  current
    DESCRIPTION
       " These objects are required for pica private mib."
    ::= { picaGroups 3 }
 
 picaConfigGroup OBJECT-GROUP
 OBJECTS {
        tftpConfigFilePath,
        tftpBatchFilePath
     }
     STATUS current
     DESCRIPTION
        " These objects are required for pica private mib."
     ::= {picaGroups 4 }
 
   picaCompliance MODULE-COMPLIANCE
        STATUS  current
        DESCRIPTION
           "The compliance statement "
       MODULE  -- this module
       MANDATORY-GROUPS {
        picaBasicGroup,
        picasfpGroup,
        picarpsuGroup,
        picaConfigGroup
        }
       ::= { picaCompliances 1 }


END
