LLDP-EXT-MED-MIB DEFINITIONS ::= BEGIN
IMPORTS
MODULE-IDENTITY, OBJECT-TYPE, Integer32, Gauge32, Unsigned32,
NOTIFICATION-TYPE
FROM SNMPv2-SMI
TEXTUAL-CONVENTION, TruthValue
FROM SNMPv2-TC
MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
FROM SNMPv2-CONF
lldpExtensions, lldpLocPortNum,
lldpRemTimeMark, lldpRemLocalPortNum, lldpRemIndex,
lldpPortConfigEntry, lldpRemChassisIdSubtype, lldpRemChassisId
FROM LLDP-MIB
Dscp
FROM DIFFSERV-DSCP-TC
SnmpAdminString
FROM SNMP-FRAMEWORK-MIB;
lldpXMedMIB MODULE-IDENTITY
LAST-UPDATED "200507280000Z" -- July 28th, 2005
ORGANIZATION "TIA TR41.4 Working Group"
CONTACT-INFO
" WG-URL: http://www.tiaonline.org/standards/sfg/scope.cfm#TR-41.4
WG-EMail: tr41@tiacomm.org
Contact: Chair, TIA TR-41
Postal: Telecommunications Industry Association
2500 Wilson Blvd., Suite 300
Arlington, VA 22201 USA
Tel: (703) 907-7700
E-mail: tr41@tiacomm.org"
DESCRIPTION
"The LLDP Management Information Base extension module for
TIA-TR41.4 Media Endpoint Discovery information.
In order to assure the uniqueness of the LLDP-MIB,
lldpXMedMIB is branched from lldpExtensions using the TIA OUI
value as the node. An OUI/'company_id' is a 24 bit globally
unique assigned number referenced by various standards.
Copyright (C) TIA (2005). This version of this MIB module
is published as Section 13.3 of ANSI/TIA-1057.
See the standard itself for full legal notices."
REVISION "200507280000Z" -- July 28th, 2005
DESCRIPTION
"Published as part of ANSI/TIA-1057."
-- OUI for TIA TR-41 is 4795 (00-12-BB)
::= { lldpExtensions 4795 }
lldpXMedNotifications OBJECT IDENTIFIER ::= { lldpXMedMIB 0 }
lldpXMedObjects OBJECT IDENTIFIER ::= { lldpXMedMIB 1 }
-- LLDP MED Extension Notifications
-- Transmission of LLDP MED Extension Notification is controlled by the
-- lldpNotificationInterval object in the LLDP MIB defined in
-- IEEE 802.1AB-2005
lldpXMedTopologyChangeDetected NOTIFICATION-TYPE
OBJECTS { lldpRemChassisIdSubtype,
lldpRemChassisId,
lldpXMedRemDeviceClass
}
STATUS current
DESCRIPTION
"A notification generated by the local device sensing
a change in the topology that indicates that a new remote
device attached to a local port, or a remote device disconnected
or moved from one port to another."
::= { lldpXMedNotifications 1 }
-- LLDP MED extension MIB groups
lldpXMedConfig OBJECT IDENTIFIER ::= { lldpXMedObjects 1 }
lldpXMedLocalData OBJECT IDENTIFIER ::= { lldpXMedObjects 2 }
lldpXMedRemoteData OBJECT IDENTIFIER ::= { lldpXMedObjects 3 }
-- textual conventions
LldpXMedDeviceClass ::= TEXTUAL-CONVENTION
STATUS current
DESCRIPTION
"Device Class to which the device is a member.
A value of notDefined(0) indicates that the device
has capabilities not covered by any of the LLDP-MED classes.
A value of endpointClass1(1) indicates that the device
has endpoint class 1 capabilities.
A value of endpointClass2(2) indicates that the device
has endpoint class 2 capabilities.
A value of endpointClass3(3) indicates that the device
has endpoint class 3 capabilities.
A value of networkConnectivity(4) indicates that the device
has network connectivity device capabilities.
"
SYNTAX INTEGER {
notDefined(0),
endpointClass1(1),
endpointClass2(2),
endpointClass3(3),
networkConnectivity(4)
}
-- LLDP-MED Capabilities TC
LldpXMedCapabilities ::= TEXTUAL-CONVENTION
STATUS current
DESCRIPTION
"Bitmap that includes the MED organizationally defined set of LLDP
TLVs the device is capable of and whose transmission is allowed on
the local LLDP agent by network management.
Each bit in the bitmap corresponds to an LLDP-MED subtype associated
with a specific TIA TR41.4 MED TLV.
Having the bit 'capabilities(0)' set indicates that the LLDP
agent refers to the Capabilities TLVs.
Having the bit 'networkPolicy(1)' set indicates that the LLDP
agent refers to the Network Policy TLVs.
Having the bit 'location(2)' set indicates that
the LLDP agent refers to the Emergency Communications
System Location TLVs.
Having the bit 'extendedPSE(3)' set indicates that
the LLDP agent refers to the Extended PoE TLVs with PSE
capabilities.
Having the bit 'extendedPD(4)' set indicates that
the LLDP agent refers to the Extended PoE TLVs with PD
capabilities.
Having the bit 'inventory(5)' set indicates that
the LLDP agent refers to the Hardware Revision, Firmware
Revision, Software Revision, Serial Number, Manufacturer Name,
Model Name, and Asset ID TLVs."
SYNTAX BITS {
capabilities(0),
networkPolicy(1),
location(2),
extendedPSE(3),
extendedPD(4),
inventory(5)
}
-- Location Subtype Textual Convention
LocationSubtype ::= TEXTUAL-CONVENTION
STATUS current
DESCRIPTION
"The location subtype advertised by the remote endpoint.
A value coordinateBased(2) indicates that the location subtype
advertised by the endpoint is defined to use the relevant subfields
of the DHCP option for Coordinate LCI as specified in
ANSI/TIA-1057, Section 10.2.4.3.1.
A value civicAddress(3) indicates that the location subtype
advertised by the endpoint is defined to use the relevant subfields
of the DHCP option for Civic Address as specified in
ANSI/TIA-1057, Section 10.2.4.3.2.
A value elin(4) indicates that the location subtype
advertised by the endpoint is defined to use the Emergency
Location Information Number (ELIN) as specified in
ANSI/TIA-1057, Section 10.2.4.3.3."
SYNTAX INTEGER {
unknown(1),
coordinateBased(2),
civicAddress(3),
elin(4)
}
-- Policy Application Type Textual Convention
PolicyAppType ::= TEXTUAL-CONVENTION
STATUS current
DESCRIPTION
"The media type that defines the primary function of the
application for the policy advertised by an endpoint.
Having the bit voice(1) set indicates that the media type defining
a primary function of the application for the policy advertised on
the local port is voice.
Having the bit voiceSignaling(3) set indicates that the media type
defining a primary function of the application for the policy
advertised on the local port is voice signaling.
Having the bit guestVoice(4) set indicates that the media type
Defining a primary function of the application for the policy
advertised on the local port is guest voice.
Having the bit guestVoiceSignaling(5) set indicates that the media
type defining a primary function of the application for the policy
advertised on the local port is guest voice signaling.
Having the bit softPhoneVoice(6) set indicates that the media type
Defining a primary function of the application for the policy
advertised on the local port is softphone voice.
Having the bit videoConferencing(7) set indicates that the media
type defining a primary function of the application for the policy
advertised on the local port is voice.
Having the bit streamingVideo(8) set indicates that the media type
defining a primary function of the application for the policy
advertised on the local port is streaming video.
Having the bit videoSignaling(2) set indicates that the media type
defining a primary function of the application for the policy
advertised on the local port is video signaling."
SYNTAX BITS {
unknown(0),
voice(1),
voiceSignaling(2),
guestVoice(3),
guestVoiceSignaling(4),
softPhoneVoice(5),
videoconferencing(6),
streamingVideo(7),
videoSignaling(8)
}
lldpXMedLocDeviceClass OBJECT-TYPE
SYNTAX LldpXMedDeviceClass
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Local Device Class."
REFERENCE
" ANSI/TIA-1057, Section 10.2.2.2"
::= { lldpXMedConfig 1 }
lldpXMedPortConfigTable OBJECT-TYPE
SYNTAX SEQUENCE OF LldpXMedPortConfigEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"A table that controls selection of LLDP TLVs to be transmitted
on individual ports."
::= { lldpXMedConfig 2 }
lldpXMedPortConfigEntry OBJECT-TYPE
SYNTAX LldpXMedPortConfigEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"LLDP configuration information that controls the
transmission of the MED organizationally defined TLVs on
LLDP transmission capable ports.
This configuration object augments the lldpPortConfigEntry of
the LLDP-MIB, therefore it is only present along with the port
configuration defined by the associated lldpPortConfigEntry
entry.
Each active lldpXMedPortConfigEntry must be stored and
retrieved from non-volatile storage (along with the
corresponding lldpPortConfigEntry) after a re-initialization
of the management system."
AUGMENTS { lldpPortConfigEntry }
::= { lldpXMedPortConfigTable 1 }
LldpXMedPortConfigEntry ::= SEQUENCE {
lldpXMedPortCapSupported LldpXMedCapabilities,
lldpXMedPortConfigTLVsTxEnable LldpXMedCapabilities,
lldpXMedPortConfigNotifEnable TruthValue
}
lldpXMedPortCapSupported OBJECT-TYPE
SYNTAX LldpXMedCapabilities
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The bitmap includes the MED organizationally defined set of LLDP
TLVs whose transmission is possible for the respective port
on the LLDP agent of the device. Each bit in the bitmap corresponds
to an LLDP-MED subtype associated with a specific TIA TR41.4 MED
optional TLV. If the bit is set, the agent supports the
corresponding TLV."
REFERENCE
"ANSI/TIA-1057, Section 10.2.2.3"
::= { lldpXMedPortConfigEntry 1 }
lldpXMedPortConfigTLVsTxEnable OBJECT-TYPE
SYNTAX LldpXMedCapabilities
MAX-ACCESS read-write
STATUS current
DESCRIPTION
"The lldpXMedPortConfigTLVsTxEnable, defined as a bitmap,
includes the MED organizationally defined set of LLDP
TLVs whose transmission is allowed on the local LLDP agent by
the network management. Each bit in the bitmap corresponds
to an LLDP-MED subtype associated with a specific TIA TR41.4 MED
optional TLV. If the bit is set, the agent will send the
corresponding TLV if the respective capability is supported per
port.
Setting a bit with in this object for a non-supported capability
shall have no functional effect and will result in an inconsistent
value error returned to the management application.
There are other rules and restrictions that prevent arbitrary
combinations of TLVs to be enabled on LLDP-MED devices according to
the device classes. These rules are defined in Section 10.2.1,
Tables 5 - 9 of ANSI/TIA-1057. In case a management application
attempts to set this object to a value that does not follow the rules,
the set operation shall have and will result in an inconsistent
value error returned to the management application.
Setting this object to an empty set is valid and effectively
disables LLDP-MED on a per-port basis by disabling transmission of
all MED organizational TLVs. In this case the remote tables objects
in the LLDP-MED MIB corresponding to the respective port will not
be populated.
The default value for lldpXMedPortConfigTLVsTxEnable object
is an empty set, which means no enumerated values are set.
The value of this object must be restored from non-volatile
storage after a re-initialization of the management system."
REFERENCE
"ANSI/TIA-1057, Section 10.2.2.3"
DEFVAL { { } }
::= { lldpXMedPortConfigEntry 2 }
lldpXMedPortConfigNotifEnable OBJECT-TYPE
SYNTAX TruthValue
MAX-ACCESS read-write
STATUS current
DESCRIPTION
"A value of 'true(1)' enables sending the topology change
traps on this port.
A value of 'false(2)' disables sending the topology change
traps on this port."
REFERENCE
" ANSI/TIA-1057, Section 12.3"
DEFVAL { false }
::= { lldpXMedPortConfigEntry 3 }
lldpXMedFastStartRepeatCount OBJECT-TYPE
SYNTAX Unsigned32 (1..10)
MAX-ACCESS read-write
STATUS current
DESCRIPTION
"The number of times the fast start LLDPDU are being sent during the
activation of the fast start mechanism defined by LLDP-MED."
REFERENCE
" ANSI/TIA-1057, Section 11.2.1"
DEFVAL { 3 }
::= { lldpXMedConfig 3 }
---
--- lldpXMedLocMediaPolicyTable: Local Media Policy
--- Information Table
---
---
lldpXMedLocMediaPolicyTable OBJECT-TYPE
SYNTAX SEQUENCE OF LldpXMedLocMediaPolicyEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"This table contains one row per policy type per port
of media policy information (as a part of the MED
organizational extension) on the local system known
to this agent."
::= { lldpXMedLocalData 1 }
lldpXMedLocMediaPolicyEntry OBJECT-TYPE
SYNTAX LldpXMedLocMediaPolicyEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"Information about a particular policy on a specific
port component."
INDEX { lldpLocPortNum, lldpXMedLocMediaPolicyAppType }
::= { lldpXMedLocMediaPolicyTable 1 }
LldpXMedLocMediaPolicyEntry ::= SEQUENCE {
lldpXMedLocMediaPolicyAppType PolicyAppType,
lldpXMedLocMediaPolicyVlanID Integer32,
lldpXMedLocMediaPolicyPriority Integer32,
lldpXMedLocMediaPolicyDscp Dscp,
lldpXMedLocMediaPolicyUnknown TruthValue,
lldpXMedLocMediaPolicyTagged TruthValue
}
lldpXMedLocMediaPolicyAppType OBJECT-TYPE
SYNTAX PolicyAppType
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"The media type that defines the primary function of the
application for the policy advertised by an endpoint."
REFERENCE
"ANSI/TIA-1057, Section 10.2.3.1"
::= { lldpXMedLocMediaPolicyEntry 1 }
lldpXMedLocMediaPolicyVlanID OBJECT-TYPE
SYNTAX Integer32 (0|1..4094|4095)
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"An extension of the VLAN Identifier for the port,
as defined in IEEE 802.1P-1998.
A value of 1 through 4094 is used to define a valid PVID.
A value of 0 shall be used if the device is using priority tagged
frames, meaning that only the 802.1p priority level is significant
and the default VID of the ingress port is being used instead.
A value of 4095 is reserved for implementation use."
REFERENCE
" ANSI/TIA-1057, Section 10.2.3.5"
::= { lldpXMedLocMediaPolicyEntry 2 }
lldpXMedLocMediaPolicyPriority OBJECT-TYPE
SYNTAX Integer32 (0..7)
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"This object contains the value of the 802.1p priority
which is associated with the given port on the
local system."
REFERENCE
" ANSI/TIA-1057, Section 10.2.3.6 "
::= { lldpXMedLocMediaPolicyEntry 3 }
lldpXMedLocMediaPolicyDscp OBJECT-TYPE
SYNTAX Dscp
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"This object contains the value of the Differentiated Service
Code Point (DSCP) as defined in IETF RFC 2474 and RFC 2475
which is associated with the given port on the local system."
REFERENCE
" ANSI/TIA-1057, Section 10.2.3.7"
::= { lldpXMedLocMediaPolicyEntry 4 }
lldpXMedLocMediaPolicyUnknown OBJECT-TYPE
SYNTAX TruthValue
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"A value of 'true' indicates that the
network policy for the specified application type is
currently unknown. In this case, the VLAN ID, the
layer 2 priority and the DSCP value fields are ignored.
A value of 'false' indicates that this network policy
is defined "
REFERENCE
" ANSI/TIA-1057, Section 10.2.3.2"
::= { lldpXMedLocMediaPolicyEntry 5 }
lldpXMedLocMediaPolicyTagged OBJECT-TYPE
SYNTAX TruthValue
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"A value of 'true' indicates that the application is using a
tagged VLAN.
A value of 'false' indicates that for the specific application
the device either is using an untagged VLAN or does not
support port based VLAN operation. In this case, both the
VLAN ID and the Layer 2 priority fields are ignored and
only the DSCP value has relevance "
REFERENCE
" ANSI/TIA-1057, Section 10.2.3.3"
::= { lldpXMedLocMediaPolicyEntry 6 }
--- Inventory Information
--- Local Inventory Information transmitted by an endpoint
lldpXMedLocHardwareRev OBJECT-TYPE
SYNTAX SnmpAdminString (SIZE (0..32))
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The vendor-specific hardware revision string
as advertised by the endpoint."
REFERENCE
" ANSI/TIA-1057, Section 10.2.6.1"
::= { lldpXMedLocalData 2 }
lldpXMedLocFirmwareRev OBJECT-TYPE
SYNTAX SnmpAdminString (SIZE (0..32))
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The vendor-specific firmware revision string
as advertised by the endpoint."
REFERENCE
" ANSI/TIA-1057, Section 10.2.6.2"
::= { lldpXMedLocalData 3 }
lldpXMedLocSoftwareRev OBJECT-TYPE
SYNTAX SnmpAdminString (SIZE (0..32))
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The vendor-specific software revision string
as advertised by the endpoint."
REFERENCE
" ANSI/TIA-1057, Section 10.2.6.3"
::= { lldpXMedLocalData 4 }
lldpXMedLocSerialNum OBJECT-TYPE
SYNTAX SnmpAdminString (SIZE (0..32))
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The vendor-specific serial number
as advertised by the endpoint."
REFERENCE
" ANSI/TIA-1057, Section 10.2.6.4"
::= { lldpXMedLocalData 5 }
lldpXMedLocMfgName OBJECT-TYPE
SYNTAX SnmpAdminString (SIZE (0..32))
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The vendor-specific manufacturer name
as advertised by the endpoint."
REFERENCE
" ANSI/TIA-1057, Section 10.2.6.5"
::= { lldpXMedLocalData 6 }
lldpXMedLocModelName OBJECT-TYPE
SYNTAX SnmpAdminString (SIZE (0..32))
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The vendor-specific model name
as advertised by the endpoint."
REFERENCE
" ANSI/TIA-1057, Section 10.2.6.6"
::= { lldpXMedLocalData 7 }
lldpXMedLocAssetID OBJECT-TYPE
SYNTAX SnmpAdminString (SIZE (0..32))
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The vendor-specific asset tracking identifier
as advertised by the endpoint."
REFERENCE
" ANSI/TIA-1057, Section 10.2.6.7"
::= { lldpXMedLocalData 8 }
--- Location Information
--- Local Location Information transmitted by an endpoint
--- lldpXMedLocLocationTable - Location Information
---
lldpXMedLocLocationTable OBJECT-TYPE
SYNTAX SEQUENCE OF LldpXMedLocLocationEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"This table contains Location information as advertised
by the local system.
The information may be configured per port by a Location
Information Server (LIS) or other management application.
Multiple Location TLVs of different subtypes may be transmitted
in the same PDU.
The information in this table MUST be stored in non-volatile-memory
and persist over restart/reboot sequences."
::= { lldpXMedLocalData 9 }
lldpXMedLocLocationEntry OBJECT-TYPE
SYNTAX LldpXMedLocLocationEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"Information about Location information for the local device."
INDEX { lldpLocPortNum, lldpXMedLocLocationSubtype}
::= { lldpXMedLocLocationTable 1 }
LldpXMedLocLocationEntry ::= SEQUENCE {
lldpXMedLocLocationSubtype LocationSubtype,
lldpXMedLocLocationInfo OCTET STRING
}
lldpXMedLocLocationSubtype OBJECT-TYPE
SYNTAX LocationSubtype
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"The location subtype advertised by the local device."
REFERENCE
"ANSI/TIA-1057, Section 10.2.4.2"
::= { lldpXMedLocLocationEntry 1 }
lldpXMedLocLocationInfo OBJECT-TYPE
SYNTAX OCTET STRING (SIZE (0..256))
MAX-ACCESS read-write
STATUS current
DESCRIPTION
"The location information. Parsing of this information is
dependent upon the location subtype, as defined by the value of the
lldpXMedLocLocationSubtype object. "
REFERENCE
"ANSI/TIA-1057, Section 10.2.4.3"
DEFVAL { "" }
::= { lldpXMedLocLocationEntry 2 }
--- Extended Power over Ethernet objects
---
lldpXMedLocXPoEDeviceType OBJECT-TYPE
SYNTAX INTEGER {
unknown(1),
pseDevice(2),
pdDevice(3),
none(4)
}
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Defines the type of Power-via-MDI (Power over Ethernet) advertised
by the local device.
A value pseDevice(2) indicates that the device is advertised as a
Power Sourcing Entity (PSE).
A value pdDevice(3) indicates that the device is advertised as a
Powered Device (PD).
A value of none(4) indicates that the device does not support PoE."
REFERENCE
"ANSI/TIA-1057, Section 10.2.5.1"
::= { lldpXMedLocalData 10 }
--- Extended PoE - PSE objects
--- PSE Port Table
lldpXMedLocXPoEPSEPortTable OBJECT-TYPE
SYNTAX SEQUENCE OF LldpXMedLocXPoEPSEPortEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"This table contains one row per port of PSE PoE
information on the local system known to this agent."
::= { lldpXMedLocalData 11 }
lldpXMedLocXPoEPSEPortEntry OBJECT-TYPE
SYNTAX LldpXMedLocXPoEPSEPortEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"Information about a particular port PoE information."
INDEX { lldpLocPortNum }
::= { lldpXMedLocXPoEPSEPortTable 1 }
LldpXMedLocXPoEPSEPortEntry ::= SEQUENCE {
lldpXMedLocXPoEPSEPortPowerAv Gauge32,
lldpXMedLocXPoEPSEPortPDPriority INTEGER
}
lldpXMedLocXPoEPSEPortPowerAv OBJECT-TYPE
SYNTAX Gauge32 (0..1023)
UNITS "tenth of watt"
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"This object contains the value of the power available from the
PSE via this port expressed in units of 0.1 watts."
REFERENCE
" ANSI/TIA-1057, Section 10.2.5.4 "
::= { lldpXMedLocXPoEPSEPortEntry 1 }
lldpXMedLocXPoEPSEPortPDPriority OBJECT-TYPE
SYNTAX INTEGER {
unknown(1),
critical(2),
high(3),
low(4)
}
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Reflects the PD power priority that is being advertised on this
PSE port.
If both locally configure priority and
ldpXMedRemXPoEPDPowerPriority are available on this port, it is
a matter of local policy which one takes precedence. This object
reflects the active value on this port.
If the priority is not configured or known by the PD, the value
unknown(1) will be returned.
A value critical(2) indicates that the device advertises its power
Priority as critical, as per RFC 3621.
A value high(3) indicates that the device advertises its power
Priority as high, as per RFC 3621.
A value low(4) indicates that the device advertises its power
Priority as low, as per RFC 3621."
REFERENCE
"ANSI/TIA-1057, Section 10.2.5.3"
::= { lldpXMedLocXPoEPSEPortEntry 2 }
lldpXMedLocXPoEPSEPowerSource OBJECT-TYPE
SYNTAX INTEGER {
unknown(1),
primary(2),
backup(3)
}
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Defines the type of PSE Power Source advertised
by the local device.
A value primary(2) indicates that the device advertises its power
source as primary.
A value backup(3) indicates that the device advertises its power
Source as backup."
REFERENCE
"ANSI/TIA-1057, Section 10.2.5.2"
::= { lldpXMedLocalData 12 }
--- Extended PoE - PD objects
lldpXMedLocXPoEPDPowerReq OBJECT-TYPE
SYNTAX Gauge32 (0..1023)
UNITS "tenth of watt"
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"This object contains the value of the power required by a
PD expressed in units of 0.1 watts."
REFERENCE
" ANSI/TIA-1057, Section 10.2.4.3 "
::= { lldpXMedLocalData 13 }
lldpXMedLocXPoEPDPowerSource OBJECT-TYPE
SYNTAX INTEGER {
unknown(1),
fromPSE(2),
local(3),
localAndPSE(4)
}
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Defines the type of Power Source advertised as being used
by the local device.
A value fromPSE(2) indicates that the device advertises its power
source as received from a PSE.
A value local(3) indicates that the device advertises its power
source as local.
A value localAndPSE(4) indicates that the device advertises its
power source as using both local and PSE power."
REFERENCE
"ANSI/TIA-1057, Section 10.2.5.2"
::= { lldpXMedLocalData 14 }
lldpXMedLocXPoEPDPowerPriority OBJECT-TYPE
SYNTAX INTEGER {
unknown(1),
critical(2),
high(3),
low(4)
}
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Defines the priority advertised as being required by this PD.
A value critical(2) indicates that the device advertises its power
Priority as critical, as per RFC 3621.
A value high(3) indicates that the device advertises its power
Priority as high, as per RFC 3621.
A value low(4) indicates that the device advertises its power
Priority as low, as per RFC 3621."
REFERENCE
"ANSI/TIA-1057, Section 10.2.5.3"
::= { lldpXMedLocalData 15 }
-- LLdpXMedRemCapabilitiesTable
-- this table is read by a manager to determine what capabilities
-- exists and are enabled on the remote system connected to the port
-- The information in this table is based upon the information advertised
-- by the remote device and received on each port in the capabilities TLV
lldpXMedRemCapabilitiesTable OBJECT-TYPE
SYNTAX SEQUENCE OF LldpXMedRemCapabilitiesEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"A table that displays LLDP-MED capabilities of remote devices
connected to individual ports."
::= { lldpXMedRemoteData 1 }
lldpXMedRemCapabilitiesEntry OBJECT-TYPE
SYNTAX LldpXMedRemCapabilitiesEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"LLDP-MED capabilities of remote devices connected to the device
ports and communicating via LLDP-MED.
The remote tables in the LLDP-MED MIB excepting this table may be
sparsely populate. An entry in one of these table is meaningful
and shall be populated by the agent only if the corresponding bits
for the respective function are set in the objects in this table. "
INDEX { lldpRemTimeMark,
lldpRemLocalPortNum,
lldpRemIndex }
::= { lldpXMedRemCapabilitiesTable 1 }
LldpXMedRemCapabilitiesEntry ::= SEQUENCE {
lldpXMedRemCapSupported LldpXMedCapabilities,
lldpXMedRemCapCurrent LldpXMedCapabilities,
lldpXMedRemDeviceClass LldpXMedDeviceClass
}
lldpXMedRemCapSupported OBJECT-TYPE
SYNTAX LldpXMedCapabilities
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The bitmap includes the MED organizationally defined set of LLDP
TLVs whose transmission is possible on the LLDP agent of the remote
device connected to this port. Each bit in the bitmap corresponds
to an LLDP-MED subtype associated with a specific TIA TR41.4 MED
optional TLV. If the bit is set, the agent has the capability
to support the corresponding TLV."
REFERENCE
"ANSI/TIA-1057, Sections 10.2.2.1"
::= { lldpXMedRemCapabilitiesEntry 1 }
lldpXMedRemCapCurrent OBJECT-TYPE
SYNTAX LldpXMedCapabilities
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The bitmap includes the MED organizationally defined set of LLDP
TLVs whose transmission is possible on the LLDP agent of the remote
device connected to this port. Each bit in the bitmap corresponds
to an LLDP-MED subtype associated with a specific TIA TR41.4 MED
optional TLV. If the bit is set, the agent currently supports the
corresponding TLV."
REFERENCE
"ANSI/TIA-1057, Sections 10.2.2.1"
::= { lldpXMedRemCapabilitiesEntry 2 }
lldpXMedRemDeviceClass OBJECT-TYPE
SYNTAX LldpXMedDeviceClass
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Device Class as advertised by the device remotely connected to the
port."
REFERENCE
" ANSI/TIA-1057, Section 10.2.2.2"
::= { lldpXMedRemCapabilitiesEntry 3 }
---
---
--- lldpXMedRemMediaPolicyTable: Media Policy Table
---
---
lldpXMedRemMediaPolicyTable OBJECT-TYPE
SYNTAX SEQUENCE OF LldpXMedRemMediaPolicyEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"This table contains media policy information as advertised
by the remote system.
This table may be sparsely populated. Entries in this table are
relevant only if the networkPolicy(0) bits in the
lldpXMedRemCapSupported and lldpXMedRemCapCurrent objects of the
corresponding ports are set."
::= { lldpXMedRemoteData 2 }
lldpXMedRemMediaPolicyEntry OBJECT-TYPE
SYNTAX LldpXMedRemMediaPolicyEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"Information about the per port per policy type policy
information for a particular physical network connection."
INDEX { lldpRemTimeMark,
lldpRemLocalPortNum,
lldpRemIndex,
lldpXMedRemMediaPolicyAppType }
::= { lldpXMedRemMediaPolicyTable 1 }
LldpXMedRemMediaPolicyEntry ::= SEQUENCE {
lldpXMedRemMediaPolicyAppType PolicyAppType,
lldpXMedRemMediaPolicyVlanID Integer32,
lldpXMedRemMediaPolicyPriority Integer32,
lldpXMedRemMediaPolicyDscp Dscp,
lldpXMedRemMediaPolicyUnknown TruthValue,
lldpXMedRemMediaPolicyTagged TruthValue
}
lldpXMedRemMediaPolicyAppType OBJECT-TYPE
SYNTAX PolicyAppType
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"The media type that defines the primary function of the
application for the policy advertised by the endpoint connected
remotely to this port."
REFERENCE
"ANSI/TIA-1057, Section 10.2.3.1"
::= { lldpXMedRemMediaPolicyEntry 1 }
lldpXMedRemMediaPolicyVlanID OBJECT-TYPE
SYNTAX Integer32 (0|1..4094|4095)
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"An extension of the VLAN Identifier for the remote system
connected to this port, as defined in IEEE 802.1P-1998.
A value of 1 through 4094 is used to define a valid PVID.
A value of 0 shall be used if the device is using priority tagged
frames, meaning that only the 802.1p priority level is significant
and the default VID of the ingress port is being used instead.
A value of 4095 is reserved for implementation use."
REFERENCE
" ANSI/TIA-1057, Section 10.2.3.5"
::= { lldpXMedRemMediaPolicyEntry 2 }
lldpXMedRemMediaPolicyPriority OBJECT-TYPE
SYNTAX Integer32 (0..7)
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"This object contains the value of the 802.1p priority
which is associated with the remote system connected at
given port."
REFERENCE
" ANSI/TIA-1057, Section 10.2.3.6"
::= { lldpXMedRemMediaPolicyEntry 3 }
lldpXMedRemMediaPolicyDscp OBJECT-TYPE
SYNTAX Dscp
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"This object contains the value of the Differentiated Service
Code Point (DSCP) as defined in IETF RFC 2474 and RFC 2475
which is associated with remote system connected at the port."
REFERENCE
" ANSI/TIA-1057, Section 10.2.3.7"
::= { lldpXMedRemMediaPolicyEntry 4 }
lldpXMedRemMediaPolicyUnknown OBJECT-TYPE
SYNTAX TruthValue
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"A value of 'true' indicates that the
network policy for the specified application type is
currently unknown. In this case, the VLAN ID, the
layer 2 priority and the DSCP value fields are ignored.
A value of 'false' indicates that this network policy
is defined."
REFERENCE
" ANSI/TIA-1057, Section 10.2.3.2"
::= { lldpXMedRemMediaPolicyEntry 5 }
lldpXMedRemMediaPolicyTagged OBJECT-TYPE
SYNTAX TruthValue
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"A value of 'true' indicates that the application is using a
tagged VLAN.
A value of 'false' indicates that for the specific application
the device either is using an untagged VLAN or does not
support port based VLAN operation. In this case, both the
VLAN ID and the Layer 2 priority fields are ignored and
only the DSCP value has relevance "
REFERENCE
" ANSI/TIA-1057, Section 10.2.3.3"
::= { lldpXMedRemMediaPolicyEntry 6 }
--- lldpXMedRemInventoryTable - Remote Inventory Information
---
lldpXMedRemInventoryTable OBJECT-TYPE
SYNTAX SEQUENCE OF LldpXMedRemInventoryEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"This table contains inventory information as advertised
by the remote system.
This table may be sparsely populated. Entries in this table are
relevant only if the inventory(2) bits in the
lldpXMedRemCapSupported and lldpXMedRemCapCurrent objects of the
corresponding ports are set "
::= { lldpXMedRemoteData 3 }
lldpXMedRemInventoryEntry OBJECT-TYPE
SYNTAX LldpXMedRemInventoryEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"Information about inventory information for the remote devices
connected to the ports."
INDEX { lldpRemTimeMark,
lldpRemLocalPortNum,
lldpRemIndex }
::= { lldpXMedRemInventoryTable 1 }
LldpXMedRemInventoryEntry ::= SEQUENCE {
lldpXMedRemHardwareRev SnmpAdminString,
lldpXMedRemFirmwareRev SnmpAdminString,
lldpXMedRemSoftwareRev SnmpAdminString,
lldpXMedRemSerialNum SnmpAdminString,
lldpXMedRemMfgName SnmpAdminString,
lldpXMedRemModelName SnmpAdminString,
lldpXMedRemAssetID SnmpAdminString
}
lldpXMedRemHardwareRev OBJECT-TYPE
SYNTAX SnmpAdminString (SIZE (0..32))
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The vendor-specific hardware revision string
as advertised by the remote endpoint."
REFERENCE
" ANSI/TIA-1057, Section 10.2.6.1"
::= { lldpXMedRemInventoryEntry 1 }
lldpXMedRemFirmwareRev OBJECT-TYPE
SYNTAX SnmpAdminString (SIZE (0..32))
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The vendor-specific firmware revision string
as advertised by the remote endpoint."
REFERENCE
" ANSI/TIA-1057, Section 10.2.6.2"
::= { lldpXMedRemInventoryEntry 2 }
lldpXMedRemSoftwareRev OBJECT-TYPE
SYNTAX SnmpAdminString (SIZE (0..32))
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The vendor-specific software revision string
as advertised by the remote endpoint."
REFERENCE
" ANSI/TIA-1057, Section 10.2.6.3"
::= { lldpXMedRemInventoryEntry 3 }
lldpXMedRemSerialNum OBJECT-TYPE
SYNTAX SnmpAdminString (SIZE (0..32))
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The vendor-specific serial number
as advertised by the remote endpoint."
REFERENCE
" ANSI/TIA-1057, Section 10.2.6.4"
::= { lldpXMedRemInventoryEntry 4 }
lldpXMedRemMfgName OBJECT-TYPE
SYNTAX SnmpAdminString (SIZE (0..32))
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The vendor-specific manufacturer name
as advertised by the remote endpoint."
REFERENCE
" ANSI/TIA-1057, Section 10.2.6.5"
::= { lldpXMedRemInventoryEntry 5 }
lldpXMedRemModelName OBJECT-TYPE
SYNTAX SnmpAdminString (SIZE (0..32))
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The vendor-specific model name
as advertised by the remote endpoint."
REFERENCE
" ANSI/TIA-1057, Section 10.2.6.6"
::= { lldpXMedRemInventoryEntry 6 }
lldpXMedRemAssetID OBJECT-TYPE
SYNTAX SnmpAdminString (SIZE (0..32))
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The vendor-specific asset tracking identifier
as advertised by the remote endpoint."
REFERENCE
" ANSI/TIA-1057, Section 10.2.6.7"
::= { lldpXMedRemInventoryEntry 7 }
--- lldpXMedRemLocationTable - Remote Location Information
---
lldpXMedRemLocationTable OBJECT-TYPE
SYNTAX SEQUENCE OF LldpXMedRemLocationEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"This table contains Location information as advertised
by the remote system.
This table may be sparsely populated. Entries in this table are
relevant only if the Location(3) bits in the
lldpXMedRemCapSupported and lldpXMedRemCapCurrent objects of the
corresponding ports are set "
::= { lldpXMedRemoteData 4 }
lldpXMedRemLocationEntry OBJECT-TYPE
SYNTAX LldpXMedRemLocationEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"Information about Location information for the remote devices
connected to the ports."
INDEX { lldpRemTimeMark,
lldpRemLocalPortNum,
lldpRemIndex,
lldpXMedRemLocationSubtype}
::= { lldpXMedRemLocationTable 1 }
LldpXMedRemLocationEntry ::= SEQUENCE {
lldpXMedRemLocationSubtype LocationSubtype,
lldpXMedRemLocationInfo OCTET STRING
}
lldpXMedRemLocationSubtype OBJECT-TYPE
SYNTAX LocationSubtype
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"The location subtype advertised by the remote endpoint."
REFERENCE
"ANSI/TIA-1057, Section 10.2.4.2 "
::= { lldpXMedRemLocationEntry 1 }
lldpXMedRemLocationInfo OBJECT-TYPE
SYNTAX OCTET STRING (SIZE (0..256))
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"The location information advertised by the remote endpoint.
Parsing of this information is dependent upon the location
subtype, as defined by the value of the corresponding
lldpXMedRemLocationSubType object. "
REFERENCE
"ANSI/TIA-1057, Section 10.2.4.3 "
::= { lldpXMedRemLocationEntry 2 }
--- lldpXMedRemXPoETable - Information about Remote PoE Device Type
---
lldpXMedRemXPoETable OBJECT-TYPE
SYNTAX SEQUENCE OF LldpXMedRemXPoEEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"This table contains information about the PoE device type
as advertised by the remote system.
This table is densely populated."
::= { lldpXMedRemoteData 5 }
lldpXMedRemXPoEEntry OBJECT-TYPE
SYNTAX LldpXMedRemXPoEEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"Information about PoE type of the remote devices
connected to the ports."
INDEX { lldpRemTimeMark,
lldpRemLocalPortNum,
lldpRemIndex }
::= { lldpXMedRemXPoETable 1 }
LldpXMedRemXPoEEntry ::= SEQUENCE {
lldpXMedRemXPoEDeviceType INTEGER
}
lldpXMedRemXPoEDeviceType OBJECT-TYPE
SYNTAX INTEGER {
unknown(1),
pseDevice(2),
pdDevice(3),
none(4)
}
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Defines the type of Power-via-MDI (Power over Ethernet) advertised
by the remote device.
A value pseDevice(2) indicates that the device is advertised as a
Power Sourcing Entity (PSE).
A value pdDevice(3) indicates that the device is advertised as a
Powered Device (PD).
A value none(4) indicates that the device does not support PoE."
REFERENCE
"ANSI/TIA-1057, Section 10.2.5.1"
::= { lldpXMedRemXPoEEntry 1 }
--- lldpXMedRemXPoEPDTable - Extended PoE PSE Information from the remote device
---
lldpXMedRemXPoEPSETable OBJECT-TYPE
SYNTAX SEQUENCE OF LldpXMedRemXPoEPSEEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"This table contains extended PoE information as advertised
by the remote devices of PSE type.
This table may be sparsely populated. Entries in this table are
relevant only if the extendedPSE(4) bits in the
lldpXMedRemCapSupported and lldpXMedRemCapCurrent objects of the
corresponding ports are set "
::= { lldpXMedRemoteData 6 }
lldpXMedRemXPoEPSEEntry OBJECT-TYPE
SYNTAX LldpXMedRemXPoEPSEEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"Information about Extended PoE PSE information for
the remote devices connected to the ports."
INDEX { lldpRemTimeMark,
lldpRemLocalPortNum,
lldpRemIndex }
::= { lldpXMedRemXPoEPSETable 1 }
LldpXMedRemXPoEPSEEntry ::= SEQUENCE {
lldpXMedRemXPoEPSEPowerAv Gauge32,
lldpXMedRemXPoEPSEPowerSource INTEGER,
lldpXMedRemXPoEPSEPowerPriority INTEGER
}
lldpXMedRemXPoEPSEPowerAv OBJECT-TYPE
SYNTAX Gauge32 (0..1023)
UNITS "tenth of watt"
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"This object contains the value of the power available from the
PSE via this port expressed in units of 0.1 watts on the remote
device."
REFERENCE
" ANSI/TIA-1057, Section 10.2.5.4"
::= { lldpXMedRemXPoEPSEEntry 1 }
lldpXMedRemXPoEPSEPowerSource OBJECT-TYPE
SYNTAX INTEGER {
unknown(1),
primary(2),
backup(3)
}
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Defines the type of PSE Power Source advertised
by the remote device.
A value primary(2) indicates that the device advertises its power
source as primary.
A value backup(3) indicates that the device advertises its power
Source as backup."
REFERENCE
"ANSI/TIA-1057, Section 10.2.5.2"
::= { lldpXMedRemXPoEPSEEntry 2 }
lldpXMedRemXPoEPSEPowerPriority OBJECT-TYPE
SYNTAX INTEGER {
unknown(1),
critical(2),
high(3),
low(4)
}
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"This object contains the value of the PSE power priority
advertised by the remote device.
A value critical(2) indicates that the device advertises its power
priority as critical, as per RFC 3621.
A value high(3) indicates that the device advertises its power
priority as high, as per RFC 3621.
A value low(4) indicates that the device advertises its power
priority as low, as per RFC 3621."
REFERENCE
"ANSI/TIA-1057, Section 10.2.5.3"
::= { lldpXMedRemXPoEPSEEntry 3 }
--- lldpXMedRemXPoEPDTable - Extended PoE PD Information from the remote device
---
lldpXMedRemXPoEPDTable OBJECT-TYPE
SYNTAX SEQUENCE OF LldpXMedRemXPoEPDEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"This table contains extended PoE information as advertised
by the remote devices of PD type.
This table may be sparsely populated. Entries in this table are
relevant only if the extendedPD(5) bits in the
lldpXMedRemCapSupported and lldpXMedRemCapCurrent objects of the
corresponding ports are set "
::= { lldpXMedRemoteData 7 }
lldpXMedRemXPoEPDEntry OBJECT-TYPE
SYNTAX LldpXMedRemXPoEPDEntry
MAX-ACCESS not-accessible
STATUS current
DESCRIPTION
"Information about XPoEPD information for the remote devices
connected to the ports."
INDEX { lldpRemTimeMark,
lldpRemLocalPortNum,
lldpRemIndex }
::= { lldpXMedRemXPoEPDTable 1 }
LldpXMedRemXPoEPDEntry ::= SEQUENCE {
lldpXMedRemXPoEPDPowerReq Gauge32,
lldpXMedRemXPoEPDPowerSource INTEGER,
lldpXMedRemXPoEPDPowerPriority INTEGER
}
lldpXMedRemXPoEPDPowerReq OBJECT-TYPE
SYNTAX Gauge32 (0..1023)
UNITS "tenth of watt"
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"This object contains the value of the power required by a
PD connected remotely to the port
expressed in units of 0.1 watts."
REFERENCE
" ANSI/TIA-1057, Section 10.2.5.4 "
::= { lldpXMedRemXPoEPDEntry 1 }
lldpXMedRemXPoEPDPowerSource OBJECT-TYPE
SYNTAX INTEGER {
unknown(1),
fromPSE(2),
local(3),
localAndPSE(4)
}
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Defines the type of Power Source advertised as being used
by the device connected remotely to the port.
A value fromPSE(2) indicates that the device advertises its power
source as received from a PSE.
A value local(3) indicates that the device advertises its power
source as local.
A value localAndPSE(4) indicates that the device advertises its
power source as using both local and PSE power."
REFERENCE
"ANSI/TIA-1057, Section 10.2.5.2"
::= { lldpXMedRemXPoEPDEntry 2 }
lldpXMedRemXPoEPDPowerPriority OBJECT-TYPE
SYNTAX INTEGER {
unknown(1),
critical(2),
high(3),
low(4)
}
MAX-ACCESS read-only
STATUS current
DESCRIPTION
"Defines the priority advertised as being required by the PD
connected remotely to the port.
A value critical(2) indicates that the device advertises its power
Priority as critical, as per RFC 3621.
A value high(3) indicates that the device advertises its power
Priority as high, as per RFC 3621.
A value low(4) indicates that the device advertises its power
Priority as low, as per RFC 3621."
REFERENCE
"ANSI/TIA-1057, Section 10.2.5.3"
::= { lldpXMedRemXPoEPDEntry 3 }
---
-- conformance information
lldpXMedConformance OBJECT IDENTIFIER ::= { lldpXMedMIB 2 }
lldpXMedCompliances OBJECT IDENTIFIER ::= { lldpXMedConformance 1 }
lldpXMedGroups OBJECT IDENTIFIER ::= { lldpXMedConformance 2 }
-- compliance statements
lldpXMedCompliance MODULE-COMPLIANCE
STATUS current
DESCRIPTION
"The compliance statement for SNMP entities which implement
the LLDP MED extension MIB."
MODULE -- this module
MANDATORY-GROUPS { lldpXMedConfigGroup,
lldpXMedRemSysGroup,
lldpXMedNotificationsGroup
}
GROUP lldpXMedOptMediaPolicyGroup
DESCRIPTION
"This group represents the information associated with
the LLDP-MED optional Media Policy TLVs,
therefore the agent may not implement them."
GROUP lldpXMedOptInventoryGroup
DESCRIPTION
"This group represents the information associated with
the LLDP-MED optional inventory TLVs,
therefore the agent may not implement them."
GROUP lldpXMedOptLocationGroup
DESCRIPTION
"This group represents the information associated with
the LLDP-MED optional Location TLVs,
therefore the agent may not implement them."
GROUP lldpXMedOptPoEPSEGroup
DESCRIPTION
"This group represents the information associated with
the LLDP-MED optional extended PoE PolicyTLVs, carrying
PSE information, therefore the agent may
not implement them."
GROUP lldpXMedOptPoEPDGroup
DESCRIPTION
" This group represents the information associated with
the LLDP-MED optional extended PoE Policy TLVs, carrying
PD information, therefore the agent may
not implement them."
::= { lldpXMedCompliances 1 }
-- MIB groupings
lldpXMedConfigGroup OBJECT-GROUP
OBJECTS {
lldpXMedPortCapSupported,
lldpXMedPortConfigTLVsTxEnable,
lldpXMedPortConfigNotifEnable,
lldpXMedFastStartRepeatCount,
lldpXMedLocXPoEDeviceType,
lldpXMedLocDeviceClass
}
STATUS current
DESCRIPTION
"The collection of objects which are used to configure or
describe the configuration or behavior of the LLDP-MED
organizational extension implementation."
::= { lldpXMedGroups 1 }
lldpXMedOptMediaPolicyGroup OBJECT-GROUP
OBJECTS {
lldpXMedLocMediaPolicyVlanID,
lldpXMedLocMediaPolicyPriority,
lldpXMedLocMediaPolicyDscp,
lldpXMedLocMediaPolicyUnknown,
lldpXMedLocMediaPolicyTagged
}
STATUS current
DESCRIPTION
"The collection of objects which are used to represent LLDP
MED organizational extensions for Media Policy Information."
::= { lldpXMedGroups 2 }
lldpXMedOptInventoryGroup OBJECT-GROUP
OBJECTS {
lldpXMedLocHardwareRev,
lldpXMedLocFirmwareRev,
lldpXMedLocSoftwareRev,
lldpXMedLocSerialNum,
lldpXMedLocMfgName,
lldpXMedLocModelName,
lldpXMedLocAssetID
}
STATUS current
DESCRIPTION
"The collection of objects which are used to represent LLDP
MED organizational extension for inventory Information."
::= { lldpXMedGroups 3 }
lldpXMedOptLocationGroup OBJECT-GROUP
OBJECTS {
lldpXMedLocLocationInfo
}
STATUS current
DESCRIPTION
"The collection of objects which are used to represent LLDP
MED organizational extension for Location Information."
::= { lldpXMedGroups 4 }
lldpXMedOptPoEPSEGroup OBJECT-GROUP
OBJECTS {
lldpXMedLocXPoEPSEPortPowerAv,
lldpXMedLocXPoEPSEPortPDPriority,
lldpXMedLocXPoEPSEPowerSource
}
STATUS current
DESCRIPTION
"The collection of objects which are used to represent LLDP
MED organizational extensions for PoE PSE Information."
::= { lldpXMedGroups 5 }
lldpXMedOptPoEPDGroup OBJECT-GROUP
OBJECTS {
lldpXMedLocXPoEPDPowerReq,
lldpXMedLocXPoEPDPowerSource,
lldpXMedLocXPoEPDPowerPriority
}
STATUS current
DESCRIPTION
"The collection of objects which are used to represent LLDP
MED organizational extensions for PoE PD Information."
::= { lldpXMedGroups 6 }
lldpXMedRemSysGroup OBJECT-GROUP
OBJECTS {
lldpXMedRemCapSupported,
lldpXMedRemCapCurrent,
lldpXMedRemDeviceClass,
lldpXMedRemMediaPolicyVlanID,
lldpXMedRemMediaPolicyPriority,
lldpXMedRemMediaPolicyDscp,
lldpXMedRemMediaPolicyUnknown,
lldpXMedRemMediaPolicyTagged,
lldpXMedRemHardwareRev,
lldpXMedRemFirmwareRev,
lldpXMedRemSoftwareRev,
lldpXMedRemSerialNum,
lldpXMedRemMfgName,
lldpXMedRemModelName,
lldpXMedRemAssetID,
lldpXMedRemLocationInfo,
lldpXMedRemXPoEDeviceType,
lldpXMedRemXPoEPSEPowerAv,
lldpXMedRemXPoEPSEPowerSource,
lldpXMedRemXPoEPSEPowerPriority,
lldpXMedRemXPoEPDPowerReq,
lldpXMedRemXPoEPDPowerSource,
lldpXMedRemXPoEPDPowerPriority
}
STATUS current
DESCRIPTION
"The collection of objects which are used to represent LLDPMED
organizational extension Remote Device Information."
::= { lldpXMedGroups 7 }
lldpXMedNotificationsGroup NOTIFICATION-GROUP
NOTIFICATIONS { lldpXMedTopologyChangeDetected }
STATUS current
DESCRIPTION
"Notifications sent by an LLDP-MED agent."
::= { lldpXMedGroups 8 }
END