KT-VPT KT965 v1005 (Kontron Technology Video Port Trap Driver package version 1.0.0.5 for KT965 family)

Ref. 2008-07-02/MLA.

Used to fix the onboard CRT, ADD2-CRT and ADD2-DVI so that displays always turns on if selected in Graphic Driver.

Installation procedure:

Install graphic driver "6.14.10.4957"
reboot
add "startdrv.reg" regerstry
copy vpt.sys to c:\windows\system32\drivers\
reboot

