#########################################################################	
#									#
#   KOMMisc Readme file						#
#									#
#   Edition 5.0								#
#   2010-09-17								#
#									#
#   (c) by KONTRON MODULAR COMPUTERS 2010				#
#									#
#########################################################################

 
Operating systems:

   Windows 7 (32bit)
   Windows XP
   

################ Installation notes #####################################

Windows XP:
  run the KommiscInstaller.msi 
Windows 7: 
  run setup.exe with administrator rights.

################ BSP contents ###########################################

File name          Version number  Description
-------------------------------------------------------------------------
KOMMiscInstaller.msi
setup.exe
			
################ Documentation files in BSP package #####################

Readme_WIN_MISCxxx.txt        This file (xxx = number in file name)

################ Files installed by KOMMiscInstaller.msi ################

		
			
   
   KOMMisc.sys			1.3.0.0
   KomLED.dll			1.5.0.0  
   KomSys.dll			1.4.0.0
   KomWdg.dll			1.4.0.0
   komdio.dll			1.2.0.0
   Uninstmsg.txt			
   WdfCoInstaller01007.dll	1.7.6001.18000

   KontronMSILogo.JPG			

   KomLEDDemo.exe		1.3.0.0
   KomLedApi.chm			
   KomLED.h			
   KomLED.exp			
   KomLED.lib			
   KomLEDDemo.cpp			

   KomSysDemo.exe		1.2.0.0
   KomSysApi.chm			
   KomSys.h			
   KomSys.exp			
   KomSys.lib			
   KomSysDemo.cpp			

   KomWdgDemo.exe		1.2.0.0
   KomWdgApi.chm			
   KomWdg.h			
   KomWdg.exp			
   KomWdg.lib			
   KomWdgDemo.cpp			

   KomdioDemo.exe		1.0.0.1
   KomdioApi.chm			
   Komdio_api.h			
   Komdio.exp			
   Komdio.lib			
   KomdioDemo.cpp			

   BoardSettings.chm			
   BoardSettings.exe		1.3.0.0


################ Restrictions ###########################################
 - Watchdog
   The watchdog timer settings 512 - 4096 sec are not available on all boards.
   For available watchdog timersettings refer to the hardware manual of
   the board in use.
   The BoardSettings.exe will allow selection of the timer settings mentioned
   above even if they are not available for the board in use.

 - Rear I/O
   On some boards the second Ethernet port is fixed to Front I/O. 
   In this case only the first Ethernet port can be switched to rear I/O.
   Refer to the hardware manual of the board in use.
   
################ Notes ##################################################

- This installation description is based on a clean installation of one
  of the following Microsoft operating systems:
  Windows 7 (32bit)
  Windows XP (32bit)

- On some boards the availability of the watchdog modes "Interrupt" and 
  "Cascaded" depend on BIOS settings. Refer to the BIOS manual of the board
  in use.

- The demo applications and source codes are general examples for programmers only! 
  They do not necessarily represent the actual features of the board in use.Therefore, 
  depending on the board in use, not every demo application and not every setting in 
  a demo application is functional. 
  For available board features refer to the hardware manual.



################ Version history ########################################

Revision 10:
- initial version 

