Update Instruction for Phoenix Bios:

For manual update of the Bios only two files out of this archive are needed.

Phlash16.exe the update utility and BIOS.WPH the binary image of the Bios.

Phlash16.exe needs to be executed under MS-Dos. Please ensure that no memory
managers like emm386 ... are loaded.

PHLASH16 will return an error message in such cases.

The most convenient way to update is booting the board from an MS-Dos boot disk.
Copy both files to a second diskette.

Insert second diskette and run phlash16. Phlash16.exe will search for image file
and run update procedure without any further input.
File name of image must be Bios.wph.

After successful update reboot the board and enter bios setup.
It is strongly recommended to load Bios defaults as first step.

By this CMOS setup data and security copy of setup data inside EEPROM
are in sync.

A more detailed description of Bios update and Crisis Bios recovery can
be found inside the board manual.
