Intel(R) Server Board T5520UR 
System Software Update Instructions for EFI environment

Important NOTES: 

It is highly recommended that you read the Release Notes for the software updates provided to
understand what the known issues are, what issues were addressed from previous updates, and 
what new features (if any) were added.  Release notes for each update are combined into the 
file "release.txt" in the directory where zip was extracted. 


*******************************************************

*********  Standard EFI Update Procedure **************

*******************************************************

The updates must be loaded as specified below. 


- Extract directory structure from Update Package .zip file to a USB Disk-on-key device

System Update script for BIOS/BMC/FRUSDR/ME
   1.  Boot the system to EFI Shell
   2.  Copy all files from SUP zip archive to a HD or USB Flash Drive
   3.  Map the respective storage device in system with the command
	      Shell> map -r
   4.  Change the Shell to mapped device file system
	   Example: Shell> fs0: (or fs1:)
   5.  Run the EFIUP.NSH script at the EFI prompt
	   fs0:\> efiup.nsh
   6.  Reboot system after the update is completed.
