;*******************************************************************************
;*                                                                            **
;*                     I N T E L   P R O P R I E T A R Y                      **
;*                                                                            **
;*   COPYRIGHT (c) 1999-2005 BY INTEL CORPORATION. ALL RIGHTS RESERVED.  NO   **
;*   PART  OF  THIS  PROGRAM OR PUBLICATION MAY BE REPRODUCED, TRANSMITTED,   **
;*   TRANSCRIBED, STORED IN A RETRIEVAL  SYSTEM,  OR  TRANSLATED  INTO  ANY   **
;*   LANGUAGE OR COMPUTER LANGUAGE IN ANY FORM OR BY ANY MEANS, ELECTRONIC,   **
;*   MECHANICAL, MAGNETIC, OPTICAL, CHEMICAL, MANUAL, OR OTHERWISE, WITHOUT   **
;*   THE PRIOR WRITTEN PERMISSION OF :                                        **
;*                                                                            **
;*                             INTEL CORPORATION                              **
;*                                                                            **
;*                          2200 MISSION COLLEGE BLVD                         **
;*                                                                            **
;*                     SANTA CLARA, CALIFORNIA 95052-8119                     **
;*                                                                            **
;*******************************************************************************
;* iresole.INF                                                                 **
;*                                                                            **
;*   Based on: MSPORTS.INF                                                    **
;*             Copyright (c) 1994-1998 Microsoft Corporation                  **
;*                                                                            **
;******************************************************************************* 

[version]
signature="$Windows NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%Intel%
CatalogFile = iresole.cat
DriverVer=10/08/2008,5.1.2600.2181

[DestinationDirs]
DefaultDestDir  = 11        ;LDID_SYS


; Drivers
;----------------------------------------------------------
[Manufacturer]
%Intel%=Intel, NTamd64.5.2, NTamd64.6.0.1, NTamd64.6.0

[Intel.NTamd64.6.0]
; Windows 2008 and above not supported by this INF
%E1085_serial.DeviceDesc% =  NO_DRV,  "PCI\VEN_8086&DEV_1085&CC_0700"
%E108f_serial.DeviceDesc% =  NO_DRV,  "PCI\VEN_8086&DEV_108f&CC_0700"

[Intel.NTamd64.6.0.1]
%E1085_serial.DeviceDesc% =  ComPort,  "PCI\VEN_8086&DEV_1085&CC_0700"
%E108f_serial.DeviceDesc% =  ComPort,  "PCI\VEN_8086&DEV_108f&CC_0700"

[Intel.NTamd64.5.2]
%E1085_serial.DeviceDesc% =  ComPort,  "PCI\VEN_8086&DEV_1085&CC_0700"
%E108f_serial.DeviceDesc% =  ComPort,  "PCI\VEN_8086&DEV_108f&CC_0700"

[Intel]
; Empty section, so this INF does not support Windows 2000 and Win9x.

;--------- SourceDiskNames and SourceDiskFiles Section -----------------------
; These sections identify source disks and files for installation.
[SourceDisksFiles]
prounstl.exe = 1

; NO_DRV installation
;---------------------------------------------------------------;
[NO_DRV]
AddReg=NoDrv.reg
Include=machine.inf
Needs=NO_DRV

[NO_DRV.Services]
Include=machine.inf
Needs=NO_DRV.Services

[NoDrv.reg]
HKR,,Version,,"%DriverVer%"

; COM sections
;----------------------------------------------------------
[ComPort.AddReg]
HKR,,PortSubClass,1,01

[ComPort.NT]
AddReg=ComPort.AddReg, ComPort.NT.AddReg, IRESOL.Uninstall.AddReg
LogConfig=c14,c1a,c23,c2a,c34,c3a,c43,c4a,caa
SyssetupPnPFlags = 1

[ComPort.NT.HW]
AddReg=ComPort.NT.HW.AddReg

[ComPort.NT.AddReg]
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"
; Uncomment the following line if you want to override the advanced dialog for
; your device.  See msports.h for protoype of OverrideAdvancedFunction
; HKR,,EnumAdvancedDialog,,"yourdll.dll,OverrideAdvancedFunction"

[ComPort.NT.HW.AddReg]
HKR,,"UpperFilters",0x00010000,"serenum"

[IRESOL.Uninstall.AddReg]
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1085, 0, "ESB2 SOL"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 108F, 0, "82573E SOL"

;-------------- Service installation
; Port Driver (function driver for this device)
[ComPort.NT.Services]
AddService = Serial, 0x00000002, Serial_Service_Inst, Serial_EventLog_Inst
AddService = Serenum,,Serenum_Service_Inst

; -------------- Serial Port Driver install sections
[Serial_Service_Inst]
DisplayName    = %Serial.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 1               ; SERVICE_SYSTEM_START (this driver may do detection)
ErrorControl   = 0               ; SERVICE_ERROR_IGNORE
ServiceBinary  = %12%\serial.sys
LoadOrderGroup = Extended base

; -------------- Serenum Driver install section
[Serenum_Service_Inst]
DisplayName    = %Serenum.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\serenum.sys
LoadOrderGroup = PNP Filter

[Serial_EventLog_Inst]
AddReg = Serial_EventLog_AddReg

[Serial_EventLog_AddReg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\serial.sys"
HKR,,TypesSupported,0x00010001,7

; The following sections are COM port resource configs.
; Section name format means:
; Char 1 = c (COM port)
; Char 2 = I/O config: 1 (3f8), 2 (2f8), 3 (3e8), 4 (2e8), a (any)
; Char 3 = IRQ config: #, a (any)

[c14]                   ; COM1,IRQ4
ConfigPriority=HARDRECONFIG
IOConfig=3f8-3ff(3ff::)
IRQConfig=LS:4

[c1a]                   ; COM1, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=3f8-3ff(3ff::)
IRQConfig=LS:3,4,5,7,9,10,11,12,14,15

[c23]                   ; COM2, IRQ3
ConfigPriority=HARDRECONFIG
IOConfig=2f8-2ff(3ff::)
IRQConfig=LS:3

[c2a]                   ; COM2, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=2f8-2ff(3ff::)
IRQConfig=LS:3,4,5,7,9,10,11,12,14,15

[c34]                   ; COM3, IRQ4
ConfigPriority=HARDRECONFIG
IOConfig=3e8-3ef(3ff::)
IRQConfig=LS:4

[c3a]                   ; COM3, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=3e8-3ef(3ff::)
IRQConfig=LS:3,4,5,7,9,10,11,12,14,15

[c43]                   ; COM4, IRQ3
ConfigPriority=HARDRECONFIG
IOConfig=2e8-2ef(3ff::)
IRQConfig=LS:3,5

[c4a]                   ; COM4, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=2e8-2ef(3ff::)
IRQConfig=LS:3,4,5,7,9,10,11,12,14,15

[caa]                   ; Any base, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=8@100-ffff%fff8(3ff::)
IRQConfig=LS:3,4,5,7,9,10,11,12,14,15

; End COM port LogConfig sections


[ComPort.NT.PosDup]
*PNP0500,*PNP0501,*PNP0502,*PNP0510,*PNP0511,*SMCF010,*NSC6001

; User readable strings
;----------------------------------------------------------
[Strings]

Intel="Intel"

Serial.SVCDESC  = "Serial port driver"
Serenum.SVCDESC = "Serenum Filter Driver"

E1085_serial.DeviceDesc = "Intel(R) PRO/1000 Serial over LAN"
E108f_serial.DeviceDesc = "Intel(R) Active Management Technology - SOL"
; User readable strings
;----------------------------------------------------------
[Strings.0804] ; Chinese (Simplified)

Intel="Intel"

Serial.SVCDESC  ="串行端口驱动程序"
Serenum.SVCDESC ="Serenum 过滤器驱动程序"

E1085_serial.DeviceDesc ="Intel(R) PRO/1000 Serial over LAN"
E108f_serial.DeviceDesc ="Intel(R) Active Management Technology - SOL"
; User readable strings
;----------------------------------------------------------
[Strings.0404] ; Chinese (Traditional)

Intel="Intel"

Serial.SVCDESC  ="硈钡梆臱笆祘Α"
Serenum.SVCDESC ="Serenum 縵匡竟臱笆祘Α"

E1085_serial.DeviceDesc ="Intel(R) PRO/1000 Serial over LAN"
E108f_serial.DeviceDesc ="Intel(R) Active Management Technology - SOL"
; User readable strings
;----------------------------------------------------------
[Strings.0406] ; Danish (Denmark)

Intel="Intel"

Serial.SVCDESC  ="Seriel portdriver"
Serenum.SVCDESC ="Serenum filterdriver"

E1085_serial.DeviceDesc ="Intel(R) PRO/1000 Serial over LAN"
E108f_serial.DeviceDesc ="Intel(R) Active Management Technology - SOL"
; User readable strings
;----------------------------------------------------------
[Strings.0407] ; German (Germany)

Intel="Intel"

Serial.SVCDESC  ="Serieller Anschlusstreiber"
Serenum.SVCDESC ="Serenum-Filtertreiber"

E1085_serial.DeviceDesc ="Intel(R) PRO/1000 Serial over LAN"
E108f_serial.DeviceDesc ="Intel(R) Active Management Technology - SOL"
; User readable strings
;----------------------------------------------------------
[Strings.0C0A] ; Spanish (Spain)

Intel="Intel"

Serial.SVCDESC  ="Controlador de puerto serie"
Serenum.SVCDESC ="Controlador de filtro Serenum"

E1085_serial.DeviceDesc ="Intel(R) PRO/1000 Serial over LAN"
E108f_serial.DeviceDesc ="Intel(R) Active Management Technology - SOL"
; User readable strings
;----------------------------------------------------------
[Strings.040B] ; Finnish (Finland)

Intel="Intel"

Serial.SVCDESC  ="Sarjaporttiohjain"
Serenum.SVCDESC ="Serenum-suodatinohjain"

E1085_serial.DeviceDesc ="Intel(R) PRO/1000 Serial over LAN"
E108f_serial.DeviceDesc ="Intel(R) Active Management Technology - SOL"
; User readable strings
;----------------------------------------------------------
[Strings.040C] ; French (France)

Intel="Intel"

Serial.SVCDESC  ="Pilote de port s閞ie"
Serenum.SVCDESC ="Pilote de filtre Serenum"

E1085_serial.DeviceDesc ="Intel(R) PRO/1000 Serial over LAN"
E108f_serial.DeviceDesc ="Intel(R) Active Management Technology - SOL"
; User readable strings
;----------------------------------------------------------
[Strings.0410] ; Italian (Italy)

Intel="Intel"

Serial.SVCDESC  ="Driver della porta seriale"
Serenum.SVCDESC ="Driver filtro Serenum"

E1085_serial.DeviceDesc ="Intel(R) PRO/1000 Serial over LAN"
E108f_serial.DeviceDesc ="Intel(R) Active Management Technology - SOL"
; User readable strings
;----------------------------------------------------------
[Strings.0411] ; Japanese (Japan)

Intel="Intel"

Serial.SVCDESC  ="僔儕傾儖 僋儔僗 僪儔僀僶"
Serenum.SVCDESC ="Serenum 僼傿儖僞 僪儔僀僶"

E1085_serial.DeviceDesc ="Intel(R) PRO/1000 Serial over LAN"
E108f_serial.DeviceDesc ="Intel(R) Active Management Technology - SOL"
; User readable strings
;----------------------------------------------------------
[Strings.0412] ; Korean (Korea)

Intel="Intel"

Serial.SVCDESC  ="流纺 器飘 靛扼捞滚"
Serenum.SVCDESC ="Serenum 鞘磐 靛扼捞滚"

E1085_serial.DeviceDesc ="Intel(R) PRO/1000 Serial over LAN"
E108f_serial.DeviceDesc ="Intel(R) Active Management Technology - SOL"
; User readable strings
;----------------------------------------------------------
[Strings.0413] ; Dutch (Netherlands)

Intel="Intel"

Serial.SVCDESC  ="Stuurprogramma voor seri雔e poort"
Serenum.SVCDESC ="Serenum Filter-stuurprogramma"

E1085_serial.DeviceDesc ="Intel(R) PRO/1000 Serial over LAN"
E108f_serial.DeviceDesc ="Intel(R) Active Management Technology - SOL"
; User readable strings
;----------------------------------------------------------
[Strings.0414] ; Norwegian (Bokm錶) (Norway)

Intel="Intel"

Serial.SVCDESC  ="Seriellportdriver"
Serenum.SVCDESC ="Sereneumfilterdriver"

E1085_serial.DeviceDesc ="Intel(R) PRO/1000 Serial over LAN"
E108f_serial.DeviceDesc ="Intel(R) Active Management Technology - SOL"
; User readable strings
;----------------------------------------------------------
[Strings.0416] ; Portuguese (Brazil)

Intel="Intel"

Serial.SVCDESC  ="Driver de porta serial"
Serenum.SVCDESC ="Driver de filtro Serenum"

E1085_serial.DeviceDesc ="Intel(R) PRO/1000 Serial over LAN"
E108f_serial.DeviceDesc ="Intel(R) Active Management Technology - SOL"
; User readable strings
;----------------------------------------------------------
[Strings.041D] ; Swedish (Sweden)

Intel="Intel"

Serial.SVCDESC  ="Drivrutin f鰎 seriell port"
Serenum.SVCDESC ="Drivrutin f鰎 Serenum-filter"

E1085_serial.DeviceDesc ="Intel(R) PRO/1000 Serial over LAN"
E108f_serial.DeviceDesc ="Intel(R) Active Management Technology - SOL"
