# Supported Intel® 10GbE Server Adapters

This driver and software are designed to operate with the following Intel® 10GbE Server Adapters:

Product Name | Board ID #† | Controller
--- | --- | ---
Intel® 82598EB 10 Gigabit BX Network Connection | n/a | 82598EB
Intel® 82598EB 10 Gigabit KX4 Network Connection | n/a | 82598EB
Intel® 10 Gigabit AF DA Dual Port Server Adapter | E37002-xxx | 82598EB
Intel® 10 Gigabit SR Dual Port Express Module | n/a | 82598EB
Intel® 10 Gigabit AT Server Adapter | D79893-xxx | 82598EB
Intel® 10 Gigabit CX4 Dual Port Server Adapter | E25335-xxx | 82598EB
Intel® 10 Gigabit XF SR Server Adapter | E16791-xxx | 82598EB
Intel® 10 Gigabit XF SR Dual Port Server Adapter | E15728-xxx | 82598EB
Intel® 10 Gigabit XF LR Server Adapter | D95857-xxx | 82598EB
Intel® 82598EB 10 Gigabit AT CX4 Network Connection | n/a | 82598EB
Intel® 82598EB 10 Gigabit AF Dual Port Network Connection | n/a | 82598EB
Intel® 82598EB 10GbE AF Network Connection | n/a | 82598EB
Intel® PRO/10GbE CX4 Server Adapter | D18727-xxx | 82597EX
Intel® PRO/10GbE LR Server Adapter | C72665-xxx C54891-xxx | 82597EX
Intel® PRO/10GbE SR Server Adapter | C72663-xxx C54889-xxx | 82597EX

†Board ID # = A 6-digit code with a 3-digit extension; printed on barcode sticker on the front of the card.

See the Adapter & Driver ID Guide: http://support.intel.com/support/go/network/adapter/home.htm

### Compatibility Notes

The following devices are not supported by Microsoft* Windows Vista*

- Intel® 10 Gigabit AT Server Adapter
- Intel® PRO/10GbE CX4 Server Adapter
- Intel® PRO/10GbE LR Server Adapter
- Intel® PRO/10GbE SR Server Adapter

The following devices are not supported by Microsoft Windows Server* 2008

- Intel® PRO/10GbE LR Server Adapter

Some Intel® 10 Gigabit Network Adapters and Connections support SFP+ pluggable optical modules.

- Intel® Network Adapters that support removable optical modules only support their original module type (i.e., the Intel® 10 Gigabit SR Dual Port Express Module only supports SR optical modules). If you plug in a different type of module, the driver will not load.
- Hot Swapping/hot plugging optical modules is not supported.
- Only single speed, 10 gigabit modules are supported.
- LAN on Motherboard (LOMs) may support DA, SR, or LR modules. Please see your system documentation for details.

`Last modified on 12/18/08 4:32p Revision 19`