
;
; Memory configuration for GD82559ER adapter.  These memory parameters must
; be included in the master CONFIG.BIB (or one of the other .BIB source
; files) in the WinCE image.
;


MEMORY

; Reserve storage for GD82559ER shared packet buffers.  Note that in the
; default image configuration, this range is already reserved for
; "debug Ethernet packet buffers".
   EPKTBUF  801DC000  00020000  RESERVED

