#########################################################################	
#									#
#   Readme_CP605_WXP.txt file						#
#									#
#   Edition 1.2								#
#   2006-04-27								#
#									#
#   c) by KONTRON MODULAR COMPUTERS 2006				#
#									#
#########################################################################


################ Installation notes #####################################

For proper use of this product you should install following drivers
in your Windows XP system in order as follows:

I845VGA: graphics driver.
To install the driver run the installer application in driver folder.

I825XX: network interface driver.
To install the driver run "autorun.exe"application in driver folder.

INFINST: Intel Chipset Software Installation Utility
To install the utility, run "setup.exe" file in INFINST folder.
WARNING: The setup utility may fail to run from removable devices
  (USB drives). In this case copy the INFINST package to hard
  drive or run it from the network.
WARNING: Long paths may cause the INFINST installer to fail. In
  that case, try to keep installation path as short as possible.

KOMMISC: KOM System functions driver
To install the driver:
- If you have Service Pack 2 installed in the system:
  - Find "High precision event timer" in Device Manager window
  - In Properties window of the device choose "Update Driver"
  - Select "Install from a list or specific location..." and click Next
  - Select "Don't search, I will choose the driver to install" and click
    Next
  - Click "Have disk..." button
  - Navigate to KOMMISC folder
- If you have not installed Service Pack 2:
  - Find "Other system device" in device manager window
  - In Properties window for the device choose "Update driver"
  - Select "Install from a list or specific location..." and click Next
  - De-select "Search removable media...", and select "Include this
    location in the search" options,
  - Click Browse button and locate the KOMMISC driver folder
- Proceed with KOMMISC installation

I82801Smb: SM-Bus driver
To install the driver follow the instructions from "Release.txt" file
in I82801Smb folder

LM81: Hardware monitor library
To install the library run "install.bat" file in LM81\INSTALL folder

MAX1617: Hardware monitor library
To install the library run "install.bat" file in MAX1617\INSTALL folder

HWMON: Hardware Monitor application
The application can be found in HWMON folder. It is required to
install I82801Smb, LM81 and MAX1617 components for HWMON to work properly.


################ BSP contents ###########################################

File name          Version number  Description
-------------------------------------------------------------------------
### I845VGA driver package: product version 6.14.10.4342 ###
ialmnt5.sys        6.14.10.4342
hccutils.dll       3.0.0.4342
hkcmd.exe          3.0.0.4342
ialmcoin_v4342.dll  1.00.1000.1
ialmdd5.dll        6.14.10.4342
ialmdev5.dll       6.14.10.4342
ialmdnt5.dll       6.14.10.4342
ialmgdev.dll       6.14.10.4342
ialmgicd.dll       6.14.10.4342
ialmrem.dll        6.14.10.4342
ialmrnt5.dll       6.14.10.4342
igfxcfg.exe        3.0.0.4342
igfxcpl.cpl        3.0.0.4342
igfxdev.dll        3.0.0.4342
igfxdgps.dll       3.0.0.4342
igfxdiag.exe       3.0.0.4342
igfxdo.dll         3.0.0.4342
igfxeud.dll        3.0.0.4342
igfxexps.dll       3.0.0.4342
igfxhk.dll         3.0.0.4342
igfxpph.dll        3.0.0.4342
igfxrara.lrc       3.0.0.4342
igfxrarb.lrc       3.0.0.4342
igfxrchs.lrc       3.0.0.4342
igfxrcht.lrc       3.0.0.4342
igfxrcsy.lrc       3.0.0.4342
igfxrdan.lrc       3.0.0.4342
igfxrdeu.lrc       3.0.0.4342
igfxrell.lrc       3.0.0.4342
igfxreng.lrc       3.0.0.4342
igfxrenu.lrc       3.0.0.4342
igfxresp.lrc       3.0.0.4342
igfxress.dll       3.0.0.4342
igfxrfin.lrc       3.0.0.4342
igfxrfra.lrc       3.0.0.4342
igfxrfrc.lrc       3.0.0.4342
igfxrheb.lrc       3.0.0.4342
igfxrhun.lrc       3.0.0.4342
igfxrita.lrc       3.0.0.4342
igfxrjpn.lrc       3.0.0.4342
igfxrkor.lrc       3.0.0.4342
igfxrnld.lrc       3.0.0.4342
igfxrnor.lrc       3.0.0.4342
igfxrplk.lrc       3.0.0.4342
igfxrptb.lrc       3.0.0.4342
igfxrptg.lrc       3.0.0.4342
igfxrrus.lrc       3.0.0.4342
igfxrsve.lrc       3.0.0.4342
igfxrtha.lrc       3.0.0.4342
igfxrtrk.lrc       3.0.0.4342
igfxsrvc.dll       3.0.0.4342
igfxtray.exe       3.0.0.4342
igfxzoom.exe       3.0.0.4342

### I825XX: network interface driver ###
e100b325.sys       8.0.19.0        I825XX driver file
e100bmsg.dll       8.0.18.0        I825XX driver file
IntelNic.dll       8.2.9.0         I825XX driver file
e1000325.sys       8.5.14.0        I825XX driver file
e1000msg.dll       8.5.12.0        I825XX driver file
EtCoInst.dll       2.2.1.0         I825XX driver file
Prounstl.exe       8.0.7.0         I825XX driver file

### INFINST package: product version 6.3.0.1007 ###
Setup.exe          6.22.100.1441   Installer application

### KOMMISC: KOM System functions driver ###
Kommisc.inf        ---             KOMMISC driver installation file
Kommisc.sys        1.0.1.0         KOMMISC driver
MiscPropPage.dll   1.0.0.8         KOMMISC property page

### I82801Smb: SM-Bus driver ###
I82801Smb.inf      ---             I82801Smb driver installation file
I82801Smb.sys      1.0.0.5         I82801Smb driver

### LM81: Hardware monitor library ###
LM81.dll           1.3.0.0         LM81 hardware monitor library

###MAX1617: Hardware monitor library ###
MAX1617.dll        1.4.0.0         MAX1617 hardware monitor library

### HWMON: Hardware Monitor application ###
HWMON.exe          1.4.0.1         Hardware Monitor application


################ Documentation ##########################################

Readme_CP605_IXxxxx_WXP.txt        This file

INFINST\Readme.txt                 INFINST Intel release notes

KOMMISC\HLPKOMmisc.chm             KOMMISC driver help file

I82801Smb\Release.txt              I82801Smb driver release notes

LM81\SDK\LM81.chm                  LM81 help file

MAX1617\SDK\MAX1617.chm            MAX1617 help file

HWMON\HWMon.chm                    HWMON application help


################ Restrictions ###########################################

- The INFINST installation may fail to run from removable devices
  (USB drives). In this case copy the INFINST package to hard
  drive or run it from the network.
- Long paths may cause the INFINST installer to fail. In
  that case, try to keep installation path as short as possible.
- To be able to use USB 2.0 make sure Windows Service Pack 1 (or later)
  is installed.

################ Notes ##################################################

- This release is based on CP605 with BIOS version IX0110
- This installation description is based on a clean installation of
  Microsoft Windows XP with service pack 2
- Installing devices in different order may result in different ways of
  installation

################ Version history ########################################

Version 0100:
- Initial version.

Version 0200:
- Updated I825XX (ethernet) driver.

Version 0201:
- Updated I845VGA driver,
- Updated INFINST package,
- Updated I825XX driver,
- Updated KOMMISC driver,
- Updated HWMON application,
- Removed USB2.0 component,
- Initial version of all-in-one BSP.

