- ##### IPMI002_R10
  WXPE BSP

- Introduction
- Installation
- Notes
- Restrictions
- Version history
- BSP contents
- List of documentation files

kontron readme

# IPMI002_R10 WXPE BSP

       Readme_WXPE_IPMI002_R10.htm file

       Edition 2
       2012-09-28
       ©by KONTRON MODULAR COMPUTERS 2012

## Introduction

      Note: using this BSP requires a solid knowledge about Windows XP embedded and
      the Windows XP Embedded Design Suite!

      This Board Support Package (BSP) installs a NUll-Driver for the
      IPMI device under Windows XP embedded.
      (see List of supported Kontron Boards and supported devices)

      The BSP contains files which will be imported into the WXPE Database repository.
      (see BSP contents)

       Windows XP does not support IPMI. The only purpose of this component is
       to suppress the display of an unkwnon device in the device manager.
       It is not required for any other function of the target machine.

## Contents of this readme file:

      Installation
    	Notes
    	Restrictions
    	Version history
    	BSP contents
    	List of documentation files

## Installation

       System Requirements:
       Windows XP Embedded Design Suite

       Import sld file
       - Create an empty directory folder and unpack the WXPE_IPMI002_R10.zip file in this directory.
       - Open the WXPe Database Manager.
       - Import the IPMI002_R10.sld file into the Windows XP Embedded Database (for
         detailed instructions please refer to SLDUserGuide.chm file).

            back to contents list

## Notes

    This  BSP is released for:

     Kontron BoardBIOS Version
    CP6003, CP6003RA/RCB3C01 13.0
    CP6004B3D01 10.0

    BSP created with:Database update state:
     Windows XP embedded SP3 with Feature Pack 2007April 2012

             This SLD file does installs a Null driver only! It's only
    purpose is to suppress the display of an unknown device in the
    device manager.

    back to contents list

## Restrictions

                    none

    back to contents list

## Version history

            R10:  initial release

    back to contents list

## BSP contents

    Supported DevicesSupport based on:
    IPMI	Null driver for IPMI device

    IPMI002_R10.sld
    Files ----
       null.inf

    back to contents list

## List of documentation files

            The BSP contains the following documentation files:

            none

    back to contents list