- ##### STORE001_R11
  WXPE BSP

- Introduction
- Installation
- Notes
- Restrictions
- Version history
- BSP contents
- List of documentation files

kontron readme

# STORE001_R11 WXPE BSP

       Readme_WXPE_STORE001_R11.htm file

       Edition 1
       2012-06-15
       ©by KONTRON MODULAR COMPUTERS 2012

## Introduction

      Note: using this BSP requires a solid knowledge about Windows XP embedded and
      the Windows XP Embedded Design Suite!

      This Board Support Package (BSP) supports the
      Intel(R) Rapid Storage Technology Driver for Windows XP embedded.
      (see List of supported Kontron Boards and supported devices)

      The BSP contains files which will be imported into the WXPE Database repository.
      (see BSP contents)

      This SLD file is required if the target machines SataMode is set to "ahci" or "raid"!

## Contents of this readme file:

      Installation
    	Notes
    	Restrictions
    	Version history
    	BSP contents
    	List of documentation files

## Installation

       System Requirements:
       Windows XP Embedded Design Suite

       Import sld file
       - Create an empty directory folder and unpack the WXPE_STORE001_R11.zip file in this directory.
       - Open the WXPe Database Manager.
       - Import the STORE001_R11.sld file into the Windows XP Embedded Database (for
         detailed instructions please refer to SLDUserGuide.chm file).

            back to contents list

## Notes

    This  BSP is released for:

     Kontron BoardBIOS Version
    CP6004B3D01 10.0

    BSP created with:Database update state:
     Windows XP embedded SP3 with Feature Pack 2007August 2012

             Before running the FBA on the target machine,  check the
             SataMode configuration via "kboardconfig" uEFI shell command
             set to [ahci] or [raid].

    back to contents list

## Restrictions

                    The application STOR_Win7_XP_11.2.0.1006.exe contained in this package
                    needs the .NET Framework 3.0 in order to install the
                    the Raid/AHCI user interface.

    back to contents list

## Version history

            R11:  update to driver version 11.2.0.1006
            R10:  initial release

    back to contents list

## BSP contents

    Supported DevicesSupport based on:
    Intel(R) Rapid Storage Technology Driver Intel(R) 7 Series Chipset Family SATA AHCI Controller

    Intel(R) Mobile Express Chipset SATA RAID Controller

    STORE001_R11.sld
    Files ----Version
       F6Readme.txt
       iaahci.cat
       iaAHCI.inf
       iastor.cat
       iaStor.inf
       iaStor.sys11.2.0.1006
       STOR_Win7_XP_11.2.0.1006.exe12.0.0.49974
       license.txt
       TXTSETUP.OEM

    back to contents list

## List of documentation files

            The BSP contains the following documentation files:

             F6Readme.txt
             license.txt

    back to contents list